Table D STD |  0 | 14
# Standard WMO BUFR Table D, Master Table 0, Version 14
# Last updated: October 6, 2009
# Meaning of Descriptor CODes:
#
#====================================================================================================
# F-XX-YYY | MNEMONIC   ;DCOD ; NAME           <-- sequence definition
#          | F-XX-YYY > | NAME                 <-- element definition (first thru next-to-last)
#          | F-XX-YYY   | NAME                 <-- element definition (last)
#====================================================================================================

  3-00-002 | TABLACAT   ;     ; Table A category definition 
           | 0-00-002 > | Table A category, line 1
           | 0-00-003   | Table A category, line 2

  3-00-003 | FXYDESCR   ;     ; FXY descriptor
           | 0-00-010 > | F, part descriptor
           | 0-00-011 > | X, part descriptor
           | 0-00-012   | Y, part descriptor

  3-00-004 | ELUNSCRW   ;     ; Table B element definition 
           | 3-00-003 > | Table B descriptor to be defined
           | 0-00-013 > | Element name, line 1
           | 0-00-014 > | Element name, line 2
           | 0-00-015 > | Units name
           | 0-00-016 > | Units scale sign
           | 0-00-017 > | Units scale
           | 0-00-018 > | Units reference sign
           | 0-00-019 > | Units reference value
           | 0-00-020   | Element data width

  3-00-010 | DELAYREP   ;     ; Table D sequence definition 
           | 3-00-003 > | Table D descriptor to be defined
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 0-00-030   | Descriptor defining sequence

  3-01-001 | WMOBLKST   ;     ;  
           | 0-01-001 > | WMO block number
           | 0-01-002   | WMO station number

  3-01-002 | WMORGPLT   ;     ;  
           | 0-01-003 > | WMO Region number
           | 0-01-004 > | WMO Region sub-area
           | 0-01-005   | Buoy/platform identifier

  3-01-003 | SHIPCSDS   ;     ;  
           | 0-01-011 > | Ship's call sign
           | 0-01-012 > | Direction of motion of moving observing platform
           | 0-01-013   | Speed of motion of moving observing platform

  3-01-004 | SFCSTNID   ;     ; Surface station identification
           | 0-01-001 > | WMO block number
           | 0-01-002 > | WMO station number
           | 0-01-015 > | Station or site name
           | 0-02-001   | Type of station

  3-01-005 | STNIDTIM   ;     ; Origin and identification sequence
           | 0-01-035 > | Originating centre
           | 0-01-034   | Identification of originating/generating sub-centre

  3-01-011 | YYMMDD     ;     ;  
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003   | Day

  3-01-012 | HHMM       ;     ;  
           | 0-04-004 > | Hour
           | 0-04-005   | Minute

  3-01-013 | HHMMSS     ;     ;  
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-04-006   | Second

  3-01-014 | TIMEPERD   ;     ; Time period
           | 1-02-002 > | Replication of 2 descriptors 2 times
           | 3-01-011 > | Year, Month, Day
           | 3-01-012   | Hour, Minute

  3-01-021 | LTLONH     ;     ;  
           | 0-05-001 > | Latitude
           | 0-06-001   | Longitude

  3-01-022 | LTLONHHT   ;     ;  
           | 0-05-001 > | Latitude (high accuracy)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-07-001   | Height of station

  3-01-023 | LTLONC     ;     ;  
           | 0-05-002 > | Latitude (coarse accuracy)
           | 0-06-002   | Longitude (coarse accuracy)

  3-01-024 | LALOLV     ;     ;  
           | 0-05-002 > | Latitude (coarse accuracy)
           | 0-06-002 > | Longitude (coarse accuracy)
           | 0-07-001   | Height of station

  3-01-025 | LTLONCDT   ;     ;  
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-04-003 > | Day
           | 3-01-012   | Time

  3-01-026 | LTLONHTP   ;     ;  
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-04-003 > | Start of time period in days
           | 0-04-003 > | End of time period in days
           | 0-04-004 > | Start of time period in hours
           | 0-04-004 > | End of time period in hours
           | 0-04-005 > | Start of time period in minutes
           | 0-04-005   | End of time period in minutes

  3-01-027 | DESCFEAT   ;     ; Description of a feature in 3-D or 2-D
           | 0-08-007 > | Dimensional significance, 0=Point, 1=Line, 2=Area, 3=Volume
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-01-028 > | Description of horizontal section
           | 0-08-007   | Dimensional significance, Missing=Cancel

  3-01-028 | FEATPOLY   ;     ; Horizontal section of a feature described as a polygon, circle, line or point
           | 0-08-040 > | Flight level significance
           | 0-33-042 > | Type of limit represented by following (flight level) value
           | 0-07-010 > | Flight level
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended replication factor
           | 3-01-023 > | Location
           | 0-19-007 > | Radius of feature
           | 0-08-040   | Flight level significance, Missing=Cancel

  3-01-031 | IDTIMLOH   ;     ;  
           | 3-01-001 > | WMO block and station number
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-022   | Latitude and longitude (high accuracy), height of station

  3-01-032 | IDTIMLOC   ;     ;  
           | 3-01-001 > | WMO block and station number
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-024   | Latitude and longitude (coarse accuracy), height of station

  3-01-033 | BUOYPLTH   ;     ; Buoy/platform - fixed
           | 0-01-005 > | Buoy/platform identifier
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021   | Latitude and longitude (high accuracy)

  3-01-034 | BUOYPLTC   ;     ; Buoy/platform - fixed
           | 0-01-005 > | Buoy/platform identifier
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023   | Latitude and longitude (coarse accuracy)

  3-01-035 | BUOYPLTM   ;     ; Buoy/platform - moving
           | 0-01-005 > | Buoy/platform identifier
           | 0-01-012 > | Direction of motion of moving observing platform
           | 0-01-013 > | Speed of motion of moving observing platform
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023   | Latitude and longitude (coarse accuracy)

  3-01-036 | SHIPSEQ1   ;     ; Ship
           | 3-01-003 > | Ship's call sign and motion
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023   | Latitude and longitude (coarse accuracy)

  3-01-037 | LDSTNVSH   ;     ; Land station for vertical soundings
           | 3-01-001 > | WMO block and station number
           | 0-02-011 > | Radiosonde type
           | 0-02-012 > | Radiosonde computational method
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-022   | Latitude and longitude (high accuracy), height of station

  3-01-038 | LDSTNVSC   ;     ; Land station for vertical soundings
           | 3-01-001 > | WMO block and station number
           | 0-02-011 > | Radiosonde type
           | 0-02-012 > | Radiosonde computational method
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-024   | Latitude and longitude (coarse accuracy), height of station

  3-01-039 | SHIPVSND   ;     ; Ship for vertical soundings
           | 3-01-003 > | Ship's call sign and motion
           | 0-02-011 > | Radiosonde type
           | 0-02-012 > | Radiosonde computational method
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023   | Latitude and longitude (coarse accuracy)

  3-01-040 | SHIPCALL   ;     ;  
           | 3-01-003 > | Ship's call sign and motion
           | 0-02-011 > | Radiosonde type
           | 0-02-012 > | Radiosonde computational method
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-024   | Latitude and longitude (coarse accuracy), height of station

  3-01-041 | SAIDTIME   ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-02-021 > | Satellite instrument data used in processing
           | 0-02-022 > | Satellite data processing technique used
           | 3-01-011 > | Date
           | 3-01-012   | Time

  3-01-042 | SAIDLALO   ;     ;  
           | 3-01-041 > | Satellite identifier, data used, and data processing technique; date/time
           | 3-01-021   | Latitude, longitude

  3-01-043 | SAIDCMCM   ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-02-023 > | Cloud motion computational method
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021   | Latitude, longitude

  3-01-044 | SAIDIMHU   ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-02-024 > | Integrated mean humidity computational method
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021   | Latitude, longitude

  3-01-045 | SATLOVEL   ;     ; Satellite location and velocity
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Time (hour, minute)
           | 2-01-138 > | Change width to 16 bits
           | 2-02-131 > | Change scale to 3
           | 0-04-006 > | Second
           | 2-01-000 > | Change width back to Table B
           | 2-02-000 > | Change scale back to Table B
           | 3-04-030 > | Location relative to the Earth's centre
           | 3-04-031   | Velocity relative to the Earth's centre

  3-01-046 | SAIDDMOP   ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-01-012 > | Direction of motion of moving observing platform
           | 0-02-048 > | Satellite sensor indicator
           | 0-21-119 > | Wind scatterometer geophysical model function
           | 0-25-060 > | Software identification
           | 2-02-124 > | Change scale
           | 0-02-026 > | Cross-track resolution
           | 0-02-027 > | Along-tract resolution
           | 2-02-000 > | Change scale back to Table B
           | 0-05-040   | Orbit number

  3-01-047 | ERSPRODH   ;     ; ERS product header
           | 0-01-007 > | Satellite identifier
           | 0-25-060 > | Software identification
           | 0-01-033 > | Originating/generating centre
           | 0-01-034 > | Originating/generating sub-centre
           | 0-01-012 > | Direction of motion of moving observation platform
           | 3-01-045 > | Satellite location and velocity
           | 0-02-021 > | Satellite instrument data used in processing
           | 3-01-011 > | Date (year, month, day)
           | 3-01-012 > | Time (hour, minute)
           | 2-01-138 > | Change bit width to 16 bits
           | 2-02-131 > | Change scale to 3
           | 0-04-006 > | Second
           | 2-01-000 > | Change width back to Table B
           | 2-02-000 > | Change scale back to Table B
           | 3-01-023   | Location (latitude, longitude)

  3-01-048 | RADARPRM   ;     ; Radar parameters
           | 0-02-104 > | Antenna polarization
           | 0-02-121 > | Mean frequency
           | 0-02-113 > | Number of azimuth looks
           | 0-02-026 > | Cross-track resolution
           | 0-02-027 > | Along-track resolution
           | 0-02-111 > | Radar incidence angle
           | 0-02-140 > | Satellite radar beam azimuth angle
           | 2-02-127 > | Change scale to -1
           | 0-01-013 > | Radar platform velocity
           | 2-02-000 > | Change scale to Table B
           | 2-02-126 > | Change scale to -2
           | 0-07-001 > | Radar platform altitude
           | 2-02-000 > | Change scale to Table B
           | 0-25-010 > | Clutter treatment
           | 0-21-064   | Clutter noise estimate

  3-01-049 | RADARBMD   ;     ; Radar beam data
           | 0-02-111 > | Radar incidence angle
           | 0-02-112 > | Radar look angle
           | 0-21-062 > | Backscatter
           | 0-21-063 > | Radiometric resolution (Noise value)
           | 0-21-065   | Missing packet counter

  3-01-051 | ACFTSEQN   ;     ;  
           | 0-01-006 > | Aircraft flight number
           | 0-02-061 > | Navigational system
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021 > | Latitude, longitude
           | 0-08-004   | Phase of aircraft flight

  3-01-055 | BUOYSEQN   ;     ;  
           | 0-01-005 > | Buoy/platform identifier
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-01-012 > | Direction of motion of moving observing platform
           | 0-01-014   | Platform drift speed (high precision)

  3-01-062 | RADARLOC   ;     ; Radar locations
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-01-001   | WMO block and station number

  3-01-065 | ACARID     ;     ; ACARS identification
           | 0-01-006 > | Aircraft flight number
           | 0-01-008 > | Aircraft registration number
           | 0-02-001 > | Type of station
           | 0-02-002 > | Type of instrumentation for wind measurement
           | 0-02-005 > | Precision of temperature observation
           | 0-02-062 > | Type of aircraft data relay system
           | 0-02-070 > | Original specification of latitude/longitude
           | 0-02-065   | ACARS ground receiving station

  3-01-066 | ACARLO     ;     ; ACARS location
           | 3-01-011 > | Year, month, day
           | 3-01-013 > | Hour, minute, second
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-07-004 > | Pressure
           | 0-02-064 > | Aircraft roll angle quality
           | 0-08-004   | Phase of aircraft flight

  3-01-071 | SIDGRSEQ   ;     ; Satellite identifier/Generating resolution
           | 0-01-007 > | Satellite identifier
           | 0-01-031 > | Generating centre
           | 0-02-020 > | Satellite classification
           | 0-02-028 > | Segment size at nadir in X direction
           | 0-02-029   | Segment size at nadir in Y direction

  3-01-072 | SIDENSEQ   ;     ; Satellite identification
           | 3-01-071 > | Satellite identification, Generation resolution
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021   | Latitude, longitude

  3-01-090 | SFIDTIME   ;     ; Surface station identification; time, horizontal and vertical co-ordinates
           | 3-01-004 > | Surface station identification
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Hour, minute
           | 3-01-021 > | Latitude, longitude (high accuracy)
           | 0-07-030 > | Height of station ground above mean sea level
           | 0-07-031   | Height of barometer above mean sea level

  3-01-091 | SFCSTNIN   ;     ; Surface station instrumentation
           | 0-02-180 > | Main present weather detecting system
           | 0-02-181 > | Supplementary present weather sensor
           | 0-02-182 > | Visibility measurement system
           | 0-02-183 > | Cloud detection system
           | 0-02-184 > | Type of lightning detection sensor
           | 0-02-179 > | Type of sky condition algorithm
           | 0-02-186 > | Capability to detect precipitation phenomena
           | 0-02-187 > | Capability to detect other weather phenomena
           | 0-02-188 > | Capability to detect obscuration
           | 0-02-189   | Capability to discriminate lightning strikes

  3-01-092 | MOBIDENT   ;     ; Mobile surface station identification, date/time, horizontal and vertical coordinates
           | 0-01-011 > | Mobile land station identifier
           | 0-01-003 > | WMO Region number
           | 0-02-001 > | Type of station
           | 3-01-011 > | Year, Month, Day
           | 3-01-012 > | Hour, Minute
           | 3-01-021 > | Latitude (high accuracy), Longitude (high accuracy)
           | 0-07-030 > | Height of station ground above mean sea level
           | 0-07-031 > | Height of barometer above mean sea level
           | 0-33-024   | Station elevation quality mark

  3-01-093 | SHPIDENT   ;     ; Ship identification, movement, date/time, horizontal and vertical coordinates
           | 3-01-036 > | Ship identification
           | 0-07-030 > | Height of station platform above mean sea level
           | 0-07-031   | Height of barometer above mean sea level

  3-01-110 | IDLSIWDM   ;     ; Identification of launch site and instrumentation for wind measurements
           | 3-01-001 > | WMO block number, WMO station number
           | 0-01-011 > | Ship or mobile land station identifier
           | 0-02-011 > | Radiosonde type
           | 0-02-014 > | Tracking technique/status of system used
           | 0-02-003   | Type of measuring equipment used

  3-01-111 | IDLSIPTM   ;     ;  Identification of launch site and instrumentation for P, T, U and wind measurements
           | 3-01-001 > | WMO block number, WMO station number
           | 0-01-011 > | Ship or mobile land station identifier
           | 0-02-011 > | Radiosonde type
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-02-014 > | Tracking technique/status of system used
           | 0-02-003   | Type of measuring equipment used

  3-01-112 | IDLPIDRP   ;     ; Identification of launch point and instrumentation of dropsonde
           | 0-01-006 > | Aircraft identifier
           | 0-02-011 > | Radiosonde type
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-02-014 > | Tracking technique/status of system used
           | 0-02-003   | Type of measuring equipment used

  3-01-113 | DATETMLN   ;     ; Date/time of launch
           | 0-08-021 > | Time significance ( = 18 (launch time))
           | 3-01-011 > | Year, month, day of launch
           | 3-01-013   | Hour, minute, second of launch

  3-01-114 | HAVCOLS    ;     ; Horizontal and vertical coordinates of launch site
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-07-030 > | Height of station ground above mean sea level
           | 0-07-031 > | Height of barometer above mean sea level
           | 0-07-007 > | Height of release of sonde above mean sea level
           | 0-33-024   | Station elevation quality mark (for mobile stations)

  3-01-120 | RAOBHLIN   ;     ; Radiosonde abbreviated header and launch information
           | 3-01-001 > | WMO block and station number
           | 0-01-094 > | WBAN number
           | 0-02-011 > | Radiosonde type
           | 3-01-121   | Radiosonde launch point location

  3-01-121 | RAOBLPTL   ;     ; Radiosonde launch point location
           | 0-08-041 > | Data significance (3 = "balloon launch point")
           | 3-01-122 > | Date/time (to hundredths of second)
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-07-031 > | Height of barometer above MSL
           | 0-07-007   | Height (of radiosonde release above MSL)

  3-01-122 | DATETIME   ;     ; Date/time to hundredths of second
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 2-01-135 > | Change data width
           | 2-02-130 > | Change scale
           | 0-04-006 > | Second
           | 2-02-000 > | Cancel change scale
           | 2-01-000   | Cancel change data width

  3-01-123 | RAOBHEAD   ;     ; Radiosonde full header information
           | 1-02-002 > | Replicate 2 descriptors 2 times
           | 0-08-041 > | Data significance (0 = "parent site", 1 = "observation site")
           | 0-01-062 > | Short ICAO location identifier
           | 3-01-001 > | WMO block and station number
           | 0-01-094 > | WBAN number
           | 0-02-011 > | Radiosonde type
           | 0-01-018 > | Short station or site name
           | 0-01-095 > | Observer identification
           | 0-25-061 > | Software identification
           | 0-25-068 > | Number of archive recomputes
           | 0-01-082 > | Radiosonde ascension number
           | 0-01-083 > | Radiosonde release number
           | 0-01-081 > | Radiosonde serial number
           | 0-02-067 > | Radiosonde operating frequency
           | 0-02-066 > | Radiosonde ground receiving system
           | 0-02-014 > | Tracking technique/status of system used
           | 0-25-067 > | Release point pressure correction
           | 0-25-065 > | Orientation correction (azimuth)
           | 0-25-066 > | Orientation correction (elevation)
           | 0-02-095 > | Type of pressure sensor
           | 0-02-096 > | Type of temperature sensor
           | 0-02-097 > | Type of humidity sensor
           | 0-02-016 > | Radiosonde configuration
           | 0-02-083 > | Type of balloon shelter
           | 0-02-080 > | Balloon manufacturer
           | 0-02-081 > | Type of balloon
           | 0-01-093 > | Balloon lot number
           | 0-02-084 > | Type of gas used in balloon
           | 0-02-085 > | Amount of gas used in balloon
           | 0-02-086 > | Balloon flight train length
           | 0-02-082 > | Weight of balloon
           | 0-08-041 > | Data significance (2 = "balloon manufacture date")
           | 3-01-011   | Date

  3-01-125 | ASCATHDR   ;     ; ASCAT header information
           | 0-01-033 > | Identification of originating/generating centre
           | 0-01-034 > | Identification of originating/generating sub-centre
           | 0-25-060 > | Software identification
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instruments
           | 0-01-012   | Direction of motion of moving observing platform

  3-02-001 | PRESSQ03   ;     ;  
           | 0-10-004 > | Pressure (at station level)
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-10-061 > | 3-hour pressure change
           | 0-10-063   | Characteristic of pressure tendency

  3-02-002 | HIALTST1   ;     ; High altitude station
           | 0-10-004 > | Pressure (at station level)
           | 0-07-004 > | Pressure level
           | 0-10-003 > | Geopotential of pressure level
           | 0-10-061 > | 3-hour pressure change
           | 0-10-063   | Characteristic of pressure tendency

  3-02-003 | WTDRHVWX   ;     ;
           | 0-11-011 > | Wind direction (10 m)
           | 0-11-012 > | Wind speed (10 m)
           | 0-12-004 > | Temperature (2 m)
           | 0-12-006 > | Dew point (2 m)
           | 0-13-003 > | Relative humidity
           | 0-20-001 > | Horizontal visibility
           | 0-20-003 > | Present weather
           | 0-20-004 > | Past weather (1)
           | 0-20-005   | Past weather (2)

  3-02-004 | GENCLOUD   ;     ; General cloud information
           | 0-20-010 > | Cloud cover (total in %)
           | 0-08-002 > | Vertical significance
           | 0-20-011 > | Cloud amount
           | 0-20-013 > | Height of base of cloud
           | 0-20-012 > | Cloud type
           | 0-20-012 > | Cloud type
           | 0-20-012   | Cloud type

  3-02-005 | CLOUDSQ1   ;     ;  
           | 0-08-002 > | Vertical significance
           | 0-20-011 > | Cloud amount
           | 0-20-012 > | Cloud type
           | 0-20-013   | Height of base of cloud

  3-02-006 | PRESSQ24   ;     ;  
           | 0-10-004 > | Pressure (at station level)
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-10-062 > | 24-hour pressure change
           | 0-10-063   | Characteristic of pressure tendency

  3-02-011 | LOALTSTN   ;     ; Low altitude station
           | 3-02-001 > | Pressure and pressure change
           | 3-02-003 > | Wind, temperature, humidity, visibility, weather
           | 3-02-004   | Significant cloud layer

  3-02-012 | HIALTST2   ;     ; High altitude station
           | 3-02-002 > | Pressure and pressure change
           | 3-02-003 > | Wind, temperature, humidity, visibility, weather
           | 3-02-004   | Significant cloud information

  3-02-013 | PWTHVWXC   ;     ;  
           | 3-02-006 > | Pressure and pressure change
           | 3-02-003 > | Wind, temperature, humidity, visibility, weather
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-02-005   | Cloud layer information

  3-02-021 | DPHGTWAV   ;     ;  
           | 0-22-001 > | Direction of waves
           | 0-22-011 > | Period of waves
           | 0-22-021   | Height of waves

  3-02-022 | DPHGTWWV   ;     ;  
           | 0-22-002 > | Direction of wind waves
           | 0-22-012 > | Period of wind waves
           | 0-22-022   | Height of wind waves

  3-02-023 | DPHGTSWV   ;     ;  
           | 0-22-003 > | Direction of swell waves
           | 0-22-013 > | Period of swell waves
           | 0-22-023   | Height of swell waves

  3-02-024 | WINDSWAV   ;     ;  
           | 3-02-022 > | Wind waves
           | 1-01-002 > | Replicate 1 descriptor 2 times
           | 3-02-023   | Swell waves (2 systems of swell)

  3-02-031 | PRESDATA   ;     ; Pressure information
           | 3-02-001 > | Pressure data
           | 0-10-062 > | 24-hour pressure change
           | 0-07-004 > | Pressure (standard level)
           | 0-10-009   | Geopotential height of the standard level

  3-02-032 | TEHUDATA   ;     ; Temperature and humidity data
           | 0-07-032 > | Height of sensor above local ground (for temperature and humidity measurement)
           | 0-12-101 > | Temperature/dry-bulb temperature (scale 2)
           | 0-12-103 > | Dew-point temperature (scale 2)
           | 0-13-003   | Relative humidity

  3-02-033 | VISBDATA   ;     ; Visibility data
           | 0-07-032 > | Height of sensor above local ground (for visibility measurement)
           | 0-20-001   | Horizontal visibility

  3-02-034 | PRECIP24   ;     ; Precipitation past 24 hours
           | 0-07-032 > | Height of sensor above local ground (for precipitation measurement)
           | 0-13-023   | Total precipitation past 24 hours

  3-02-035 | SYNOPINS   ;     ; Basic synoptic 'instantaneous' data
           | 3-02-032 > | Temperature and humidity data
           | 3-02-033 > | Visibility data
           | 3-02-034 > | Precipitation past 24 hours
           | 0-07-032 > | Height of sensor above local ground (set to missing to cancel the previous value)
           | 3-02-004 > | Cloud data
           | 1-01-000 > | Delayed replication
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-02-005   | Individual cloud layer or mass

  3-02-036 | CLOUDBSL   ;     ; Clouds with bases below station level
           | 1-05-000 > | Delayed replication of 5 descriptors
           | 0-31-001 > | Delayed descriptor replication factor
           | 0-08-002 > | Vertical significance
           | 0-20-011 > | Cloud amount
           | 0-20-012 > | Cloud type
           | 0-20-014 > | Height of top of cloud
           | 0-20-017   | Cloud top description

  3-02-037 | STATEGRD   ;     ; State of ground, snow depth, ground minimum temperature
           | 0-20-062 > | State of ground (with or without snow)
           | 0-13-013 > | Total snow depth
           | 0-12-113   | Ground minimum temperature (scale 2), past 12 hours

  3-02-038 | PWEATHER   ;     ; Present and past weather
           | 0-20-003 > | Present weather
           | 0-04-024 > | Time period in hours
           | 0-20-004 > | Past weather (1)
           | 0-20-005   | Past weather (2)

  3-02-039 | SUNSHIDA   ;     ; Sunshine data (from 1 hour and 24 hour period)
           | 0-04-024 > | Time period in hours
           | 0-14-031   | Total sunshine

  3-02-040 | PRECMEA2   ;     ; Precipitation measurement
           | 0-07-032 > | Height of sensor above local ground (for precipitation measurement)
           | 1-02-002 > | Replicate next 2 descriptors 2 times
           | 0-04-024 > | Time period in hours
           | 0-13-011   | Total precipitation / total water equivalent of snow

  3-02-041 | EXTRTEM2   ;     ; Extreme temperature data
           | 0-07-032 > | Height of sensor above local ground (for temperature measurement)
           | 0-04-024 > | Time period or displacement
           | 0-04-024 > | Time period or displacement
           | 0-12-111 > | Maximum temperature (scale 2) at height and over period specified
           | 0-04-024 > | Time period or displacement
           | 0-04-024 > | Time period or displacement
           | 0-12-112   | Minimum temperature (scale 2) at height and over period specified

  3-02-042 | WINDDAT2   ;     ; Wind data
           | 0-07-032 > | Height of sensor above local ground (for wind measurement)
           | 0-02-002 > | Type of instrumentation for wind measurement
           | 0-08-021 > | Time significance (= 2 (time averaged))
           | 0-04-025 > | Time period (= -10 minutes, or number of minutes after a significant change of wind)
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-08-021 > | Time significance (= missing value)
           | 1-03-002 > | Replicate next 3 descriptors 2 times
           | 0-04-025 > | Time period in minutes
           | 0-11-043 > | Maximum wind gust direction
           | 0-11-041   | Maximum wind gust speed

  3-02-043 | SYNOPPRD   ;     ; Basic synoptic 'period' data
           | 3-02-038 > | Present and past weather
           | 1-01-002 > | Replicate 1 descriptors 2 times
           | 3-02-039 > | Sunshine data (from 1 hour and 24 hour period)
           | 3-02-040 > | Precipitation measurement
           | 3-02-041 > | Extreme temperature data
           | 3-02-042 > | Wind data
           | 0-07-032   | Height of sensor above local ground (set to missing to cancel the previous value)

  3-02-044 | EVAPDATA   ;     ; Evaporation data
           | 0-04-024 > | Time period in hours
           | 0-02-004 > | Type of instrument for evaporation or crop type for evapotranspiration
           | 0-13-033   | Evaporation /evapotranspiration

  3-02-045 | RADNDATA   ;     ; Radiation data (from 1 hour and 24 hour period)
           | 0-04-024 > | Time period in hours
           | 0-14-002 > | Long-wave radiation, integrated over period specified
           | 0-14-004 > | Short-wave radiation, integrated over period specified
           | 0-14-016 > | Net radiation, integrated over period specified
           | 0-14-028 > | Global solar radiation (high accuracy), integrated over period specified
           | 0-14-029 > | Diffuse solar radiation (high accuracy), integrated over period specified
           | 0-14-030   | Direct solar radiation (high accuracy), integrated over period specified

  3-02-046 | TEMPCHNG   ;     ; Temperature change
           | 0-04-024 > | Time period or displacement
           | 0-04-024 > | Time period or displacement
           | 0-12-049   | Temperature change over period specified

  3-02-047 | DIRCLDFT   ;     ; Direction of cloud drift
           | 1-02-003 > | Replicate 2 descriptors 3 times
           | 0-08-002 > | Vertical significance
           | 0-20-054   | True direction from which clouds are moving

  3-02-048 | DIRELCLD   ;     ; Direction and elevation of cloud
           | 0-05-021 > | Bearing or azimuth
           | 0-07-021 > | Elevation angle
           | 0-20-012 > | Cloud type
           | 0-05-021 > | Bearing or azimuth ( = missing to cancel the previous value)
           | 0-07-021   | Elevation angle ( = missing to cancel the previous value)

  3-02-049 | CLINRVSD   ;     ; Cloud information reported with vertical soundings
           | 0-08-002 > | Vertical significance
           | 0-20-011 > | Cloud amount (of low or middle clouds Nh)
           | 0-20-013 > | Height of base of cloud (h)
           | 0-20-012 > | Cloud type (low clouds CL)
           | 0-20-012 > | Cloud type (middle clouds CM)
           | 0-20-012 > | Cloud type (high clouds CH)
           | 0-08-002   | Vertical significance ( = missing value)

  3-02-050 | RAOBSURF   ;     ; Radiosonde surface observation
           | 0-08-041 > | Data significance (5 = "sfc ob displacement from launch point")
           | 0-05-021 > | Bearing or azimuth
           | 0-07-005 > | Height increment
           | 2-02-130 > | Change scale
           | 0-06-021 > | Distance
           | 2-02-000 > | Cancel change scale
           | 0-08-041 > | Data significance (4 = "surface observation")
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-02-115 > | Type of surface observing equipment
           | 0-10-004 > | Pressure
           | 0-02-115 > | Type of surface observing equipment
           | 0-13-003 > | Relative humidity
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-02-115 > | Type of surface observing equipment
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-02-115 > | Type of surface observing equipment
           | 1-02-002 > | Replicate 2 descriptors 2 times
           | 0-12-101 > | Temperature/dry bulb temperature
           | 0-04-024 > | Time displacement (hour)
           | 0-02-115 > | Type of surface observing equipment
           | 0-12-103 > | Dew-point temperature
           | 0-12-102 > | Wet bulb temperature
           | 1-01-003 > | Replicate 1 descriptor 3 times
           | 0-20-012 > | Cloud type
           | 0-20-011 > | Cloud amount
           | 0-20-013 > | Height of base of cloud
           | 1-01-002 > | Replicate 1 descriptor 2 times
           | 0-20-003   | Present weather

  3-02-051 | PGTXNVPM   ;     ;  
           | 0-10-004 > | Pressure
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-07-004 > | Pressure (vertical location)
           | 0-10-003 > | Geopotential
           | 0-12-004 > | Dry-bulb temperature at 2 m
           | 0-12-051 > | Standard deviation temperature
           | 0-12-016 > | Maximum temperature at 2 m, past 24 hours
           | 0-12-017 > | Minimum temperature at 2 m, past 24 hours
           | 0-13-004 > | Vapour pressure
           | 1-02-004 > | Replicate 2 descriptors 4 times
           | 0-08-051 > | Qualifier for number of missing values in calculation of statistic
           | 0-08-020   | Total number of missing entities (with respect to accumulation or average)

  3-02-052 | TEHUDAT2   ;     ; Temperature and humidity data for ship
           | 0-07-032 > | Height of sensor above marine deck platform (for temperature and humidity measurement)
           | 0-07-033 > | Height of sensor above water surface (for temperature and humidity measurement)
           | 0-12-101 > | Temperature/dry-bulb temperature(scale.2)
           | 0-02-039 > | Method of wet-bulb temperature measurement
           | 0-12-102 > | Wet-bulb temperature (scale 2)
           | 0-12-103 > | Dew-point temperature (scale 2)
           | 0-13-003   | Relative humidity

  3-02-053 | VISBDAT2   ;     ; Visibility data for ship
           | 0-07-032 > | Height of sensor above marine deck platform (for visibility measurement)
           | 0-07-033 > | Height of sensor above water surface (for visibility measurement)
           | 0-20-001   | Horizontal visibility

  3-02-054 | SHIPINST   ;     ; Ship 'instantaneous' data
           | 3-02-052 > | Temperature and humidity data
           | 3-02-053 > | Visibility data
           | 0-07-033 > | Height of sensor above water surface (set to missing to cancel the previous value)
           | 3-02-034 > | Precipitation past 24 hours
           | 0-07-032 > | Height of sensor above marine deck platform (set to missing to cancel the previous value)
           | 3-02-004 > | Cloud data
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-02-005   | Cloud data

  3-02-055 | ICINGICE   ;     ; Icing and ice
           | 0-20-031 > | Ice deposit (thickness)
           | 0-20-032 > | Rate of ice accretion
           | 0-20-033 > | Cause of ice accretion
           | 0-20-034 > | Sea ice concentration
           | 0-20-035 > | Amount and type of ice
           | 0-20-036 > | Ice situation
           | 0-20-037 > | Ice development
           | 0-20-038   | Bearing of ice edge

  3-02-056 | SEATEMPM   ;     ; Sea/water temperature
           | 0-02-038 > | Method of sea/water temperature measurement
           | 0-07-063 > | Depth below sea/water surface (for sea surface temperature measurement)
           | 0-22-043 > | Sea/water temperature
           | 0-07-063   | Depth below sea/water surface (set to missing to cancel the previous value)

  3-02-057 | SHIPDATA   ;     ; Ship marine data
           | 3-02-056 > | Sea surface temperature, method of measurement, and depth below sea surface
           | 3-02-021 > | Waves data
           | 3-02-024   | Wind waves data

  3-02-058 | EXTRTEM3   ;     ; Ship extreme temperature data
           | 0-07-032 > | Height of sensor above marine deck platform (for temperature measurement)
           | 0-07-033 > | Height of sensor above water surface (for temperature measurement)
           | 0-04-024 > | Time period or displacement
           | 0-04-024 > | Time period or displacement
           | 0-12-111 > | Maximum temperature (scale 2) at height and over period specified
           | 0-04-024 > | Time period or displacement
           | 0-04-024 > | Time period or displacement
           | 0-12-112   | Minimum temperature (scale 2) at height and over period specified

  3-02-059 | WINDDAT3   ;     ; Ship wind data
           | 0-07-032 > | Height of sensor above marine deck platform (for wind measurement)
           | 0-07-033 > | Height of sensor above water surface (for wind measurement)
           | 0-02-002 > | Type of instrumentation for wind measurement
           | 0-08-021 > | Time significance (= 2 (time averaged))
           | 0-04-025 > | Time period (= -10 minutes, or number of minutes after a significant change of wind)
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-08-021 > | Time significance (= missing value)
           | 1-03-002 > | Replicate next 3 descriptors 2 times
           | 0-04-025 > | Time period in minutes
           | 0-11-043 > | Maximum wind gust direction
           | 0-11-041   | Maximum wind gust speed

  3-02-060 | SHIPPERD   ;     ; Ship 'period' data
           | 3-02-038 > | Present and past weather
           | 3-02-040 > | Precipitation measurement
           | 3-02-058 > | Ship extreme temperature data
           | 3-02-059   | Ship wind data

  3-02-066 | DANGERWX   ;     ; Dangerous weather phenomena
           | 0-20-023 > | Other weather phenomena
           | 0-20-024 > | Intensity of phenomena
           | 0-20-027 > | Phenomenon occurrence
           | 0-20-054 > | True direction from which a phenomenon or clouds are moving
           | 0-20-023 > | Other weather phenomena
           | 0-20-027 > | Phenomenon occurrence
           | 0-20-054 > | True direction from which a phenomenon or clouds are moving
           | 0-20-025 > | Obscuration
           | 0-20-026 > | Character of obscuration
           | 0-20-027 > | Phenomenon occurrence
           | 0-20-040 > | Evolution of drift of snow
           | 0-20-066 > | Maximum diameter of hailstones
           | 0-20-027 > | Phenomenon occurrence
           | 0-20-021 > | Type of precipitation
           | 0-20-067 > | Diameter of deposit
           | 0-20-027   | Phenomenon occurrence

  3-02-069 | VISBSEQN   ;     ; Visibility data
           | 0-07-032 > | Height of sensor above local ground
           | 0-07-033 > | Height of sensor above water surface
           | 0-33-041 > | Attribute of following value
           | 0-20-001   | Horizontal visibility

  3-02-070 | WINDDATA   ;     ; Wind data
           | 0-07-032 > | Height of sensor above local ground
           | 0-07-033 > | Height of sensor above water surface
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-11-043 > | Maximum wind gust direction
           | 0-11-041 > | Maximum wind gust speed
           | 0-11-016 > | Extreme counterclockwise wind direction of a variable wind
           | 0-11-017   | Extreme clockwise wind direction of a variable wind

  3-02-071 | WIND1HRP   ;     ; Wind data from one-hour period
           | 0-07-032 > | Height of sensor above local ground
           | 0-07-033 > | Height of sensor above water surface
           | 0-08-021 > | Time significance (= 2 (time averaged))
           | 0-04-025 > | Time period (= -10 minutes, or number of minutes after a significant change of wind, if any)
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-08-021 > | Time significance (= missing value)
           | 1-03-002 > | Replicate next 3 descriptors 2 times
           | 0-04-025 > | Time period (= -10 minutes in the first replication, = -60 minutes in the second replication)
           | 0-11-043 > | Maximum wind gust direction
           | 0-11-041 > | Maximum wind gust speed
           | 0-04-025 > | Time period (= -10 minutes)
           | 0-11-016 > | Extreme counterclockwise wind direction of a variable wind
           | 0-11-017   | Extreme clockwise wind direction of a variable wind

  3-02-072 | TEMHUMDA   ;     ; Temperature and humidity data
           | 0-07-032 > | Height of sensor above local ground
           | 0-07-033 > | Height of sensor above water surface
           | 0-12-101 > | Temperature/dry-bulb temperature (scale 2)
           | 0-12-103 > | Dew-point temperature (scale 2)
           | 0-13-003   | Relative humidity

  3-02-073 | CLOUDATA   ;     ; Cloud data
           | 0-20-010 > | Cloud cover (total)
           | 1-05-004 > | Replicate 5 descriptors 4 times
           | 0-08-002 > | Vertical significance
           | 0-20-011 > | Cloud amount
           | 0-20-012 > | Cloud type
           | 0-33-041 > | Attribute of following value
           | 0-20-013   | Height of base of cloud

  3-02-074 | PREPSTWX   ;     ; Present and past weather
           | 0-20-003 > | Present weather
           | 0-04-025 > | Time period
           | 0-20-004 > | Past weather (1)
           | 0-20-005   | Past weather (2)

  3-02-075 | IPRSPREL   ;     ; Intensity of precipitation, size of precipitation element
           | 0-08-021 > | Time significance (= 2 (time averaged))
           | 0-04-025 > | Time period (= -10 minutes)
           | 0-13-055 > | Intensity of precipitation
           | 0-13-058 > | Size of precipitation element
           | 0-08-021   | Time significance (=  missing value)

  3-02-076 | PROBSPHE   ;     ; Precipitation, obscuration and other phenomena
           | 0-20-021 > | Type of precipitation
           | 0-20-022 > | Character of precipitation
           | 0-26-020 > | Duration of precipitation
           | 0-20-023 > | Other weather phenomena
           | 0-20-024 > | Intensity of phenomena
           | 0-20-025 > | Obscuration
           | 0-20-026   | Character of obscuration

  3-02-077 | EXTRTEMP   ;     ; Extreme temperature data
           | 0-07-032 > | Height of sensor above local ground
           | 0-07-033 > | Height of sensor above water surface
           | 0-04-025 > | Time period 
           | 0-12-111 > | Maximum temperature (scale 2) at height and over period specified
           | 0-12-112 > | Minimum temperature (scale 2) at height and over period specified
           | 0-07-032 > | Height of sensor above local ground (for ground temperature)
           | 0-04-025 > | Time period
           | 0-12-112   | Minimum temperature (scale 2) at height and over period specified (for ground temperature)

  3-02-078 | STGDSNDM   ;     ; State of ground and snow depth measurement
           | 0-02-176 > | Method of state of ground measurement
           | 0-20-062 > | State of ground (with or without snow)
           | 0-02-177 > | Method of snow depth measurement
           | 0-13-013   | Total snow depth

  3-02-079 | PRECMEAS   ;     ; Precipitation measurement
           | 0-07-032 > | Height of sensor above local ground
           | 0-02-175 > | Method of precipitation measurement
           | 0-02-178 > | Method of liquid water content measurement of precipitation
           | 0-04-025 > | Time period
           | 0-13-011   | Total precipitation / total water equivalent of snow

  3-02-080 | EVAPMEAS   ;     ; Evaporation measurement
           | 0-02-185 > | Method of evaporation measurement
           | 0-04-025 > | Time period
           | 0-13-033   | Evaporation /evapotranspiration

  3-02-081 | SUNSHINE   ;     ; Total sunshine data
           | 0-04-025 > | Time period
           | 0-14-031   | Total sunshine

  3-02-082 | RADNSEQN   ;     ; Radiation data
           | 0-04-025 > | Time period 
           | 0-14-002 > | Long-wave radiation, integrated over period specified
           | 0-14-004 > | Short-wave radiation, integrated over period specified
           | 0-14-016 > | Net radiation, integrated over period specified
           | 0-14-028 > | Global solar radiation (high accuracy),  integrated over period specified
           | 0-14-029 > | Diffuse solar radiation (high accuracy),  integrated over period specified
           | 0-14-030   | Direct solar radiation (high accuracy),  integrated over period specified

  3-02-083 | FOSTPWTU   ;     ; First order statistics of P, W, T, U data
           | 0-04-025 > | Time period
           | 0-08-023 > | First order statistics
           | 0-10-004 > | Pressure
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-12-101 > | Temperature/dry-bulb temperature (scale 2)
           | 0-13-003 > | Relative humidity
           | 0-08-023   | First order statistics (= missing value)

  3-03-001 | GPWINDDS   ;     ;  
           | 0-07-003 > | Geopotential
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-002 | PRWINDDS   ;     ;  
           | 0-07-004 > | Pressure
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-003 | PRGPTMDP   ;     ;  
           | 0-07-004 > | Pressure
           | 0-10-003 > | Geopotential
           | 0-12-001 > | Temperature
           | 0-12-003   | Dew point

  3-03-004 | PRGPTMDW   ;     ;  
           | 0-07-004 > | Pressure
           | 0-10-003 > | Geopotential
           | 0-12-001 > | Temperature
           | 0-12-003 > | Dew point
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-011 | GPVSSWDS   ;     ;  
           | 0-07-003 > | Geopotential
           | 0-08-001 > | Vertical sounding significance
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-012 | PRVSSWDS   ;     ;  
           | 0-07-004 > | Pressure
           | 0-08-001 > | Vertical sounding significance
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-013 | PRVSSTRW   ;     ;  
           | 0-07-004 > | Pressure
           | 0-08-001 > | Vertical sounding significance
           | 0-10-003 > | Geopotential
           | 0-12-001 > | Temperature
           | 0-13-003 > | Relative humidity
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-014 | PRVSSTDW   ;     ;  
           | 0-07-004 > | Pressure
           | 0-08-001 > | Vertical sounding significance
           | 0-10-003 > | Geopotential
           | 0-12-001 > | Temperature
           | 0-12-003 > | Dew point
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-021 | PRESLAYR   ;     ;  
           | 0-07-004 > | Pressure (1)
           | 0-07-004 > | Pressure (2)     defines layer
           | 2-04-007 > | Add associated field of 7 bits
           | 0-31-021   | Additional field significance

  3-03-022 | LYRQPLMT   ;     ;  
           | 3-03-021 > | Layer, quality
           | 0-10-003 > | Geopotential (layer mean thickness)
           | 2-04-000   | Cancel the added associated field

  3-03-023 | LYRQTMLM   ;     ;  
           | 3-03-021 > | Layer, quality
           | 0-12-001 > | Temperature (layer mean)
           | 2-04-000   | Cancel the added associated field

  3-03-024 | LYRQUPRW   ;     ;  
           | 3-03-021 > | Layer, quality
           | 0-13-016 > | Precipitation water
           | 2-04-000   | Cancel the added associated field

  3-03-025 | SATCHNBT   ;     ;  
           | 0-02-025 > | Satellite channel
           | 2-04-007 > | Add associated field of 7 bits
           | 0-31-021 > | Additional field significance
           | 0-12-063 > | Brightness temperature
           | 2-04-000   | Cancel the added associated field

  3-03-026 | PRVSTEMP   ;     ;  
           | 0-07-004 > | Pressure
           | 0-08-003 > | Vertical significance
           | 2-04-007 > | Add associated field of 7 bits
           | 0-31-021 > | Additional field significance
           | 0-12-001 > | Temperature
           | 2-04-000   | Cancel the added associated field

  3-03-027 | PRESGEOP   ;     ;  
           | 0-07-004 > | Pressure
           | 2-04-007 > | Add associated field of 7 bits
           | 0-31-021 > | Additional field significance
           | 0-10-003 > | Geopotential
           | 2-04-000   | Cancel the added associated field

  3-03-031 | PRVSESST   ;     ;  
           | 0-07-004 > | Pressure
           | 0-08-003 > | Vertical significance (base of sounding)
           | 0-07-021 > | Elevation (local zenith)
           | 0-07-022 > | Solar elevation (solar zenith)
           | 0-08-012 > | Land/sea qualifier
           | 0-12-061   | Skin temperature

  3-03-032 | CLAMTPRT   ;     ;  
           | 0-20-011 > | Cloud amount
           | 0-20-016   | Pressure at top of cloud

  3-03-033 | CLCVRPRT   ;     ;  
           | 0-20-010 > | Cloud cover (total)
           | 0-20-016   | Pressure at the top of cloud

  3-03-040 | RAOBDURT   ;     ; Radiosonde duration of flight and termination information
           | 0-08-041 > | Data significance (7 = "flight level termination point")
           | 0-04-025 > | Time displacement (minute)
           | 0-04-026 > | Time displacement (second)
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 3-01-122 > | Date/time (to hundredths of second)
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-25-069 > | Flight level pressure correction
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-12-101 > | Temperature/dry bulb temperature
           | 0-10-009 > | Geopotential height
           | 1-02-002 > | Replicate 2 descriptors 2 times
           | 0-08-040 > | Flight level significance
           | 0-35-035   | Reason for termination

  3-03-041 | WINDSEQN   ;     ; Wind sequence
           | 0-02-152 > | Geostationary satellite instrument used
           | 0-02-023 > | Cloud motion computational method
           | 0-07-004 > | Pressure
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-02-153 > | Satellite channel centre frequency
           | 0-02-154 > | Satellite channel band width
           | 0-12-071   | Coldest cluster T

  3-03-050 | WDPLRAOB   ;     ; Wind data at a pressure level with radiosonde position
           | 0-04-086 > | Long time period or displacement (since launch time)
           | 0-08-042 > | Extended vertical sounding significance
           | 0-07-004 > | Pressure
           | 0-05-015 > | Latitude displacement since launch site (high accuracy)
           | 0-06-015 > | Longitude displacement since launch site (high accuracy)
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-051 | WSPLRAOB   ;     ; Wind shear data at a pressure level with radiosonde position
           | 0-04-086 > | Long time period or displacement (since launch time)
           | 0-08-042 > | Extended vertical sounding significance
           | 0-07-004 > | Pressure
           | 0-05-015 > | Latitude displacement since launch site (high accuracy)
           | 0-06-015 > | Longitude displacement since launch site (high accuracy)
           | 0-11-061 > | Absolute wind shear in 1 km layer below
           | 0-11-062   | Absolute wind shear in 1 km layer above

  3-03-052 | WDHLRAOB   ;     ; Wind data at a height level with radiosonde position
           | 0-04-086 > | Long time period or displacement (since launch time)
           | 0-08-042 > | Extended vertical sounding significance
           | 0-07-009 > | Geopotential height
           | 0-05-015 > | Latitude displacement since launch site (high accuracy)
           | 0-06-015 > | Longitude displacement since launch site (high accuracy)
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-03-053 | WSHLRAOB   ;     ; Wind shear data at a height level with radiosonde position
           | 0-04-086 > | Long time period or displacement (since launch time)
           | 0-08-042 > | Extended vertical sounding significance
           | 0-07-009 > | Geopotential height
           | 0-05-015 > | Latitude displacement since launch site (high accuracy)
           | 0-06-015 > | Longitude displacement since launch site (high accuracy)
           | 0-11-061 > | Absolute wind shear in 1 km layer below
           | 0-11-062   | Absolute wind shear in 1 km layer above

  3-03-054 | TDWPRAOB   ;     ; Temperature, dew-point and wind data at a pressure level with radiosonde position
           | 0-04-086 > | Long time period or displacement (since launch time)
           | 0-08-042 > | Extended vertical sounding significance
           | 0-07-004 > | Pressure
           | 0-10-009 > | Geopotential height
           | 0-05-015 > | Latitude displacement since launch site (high accuracy)
           | 0-06-015 > | Longitude displacement since launch site (high accuracy)
           | 0-12-101 > | Temperature/dry-bulb temperature (scale 2)
           | 0-12-103 > | Dew-point temperature (scale 2)
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-04-001 | VSPTWDWS   ;     ;  
           | 0-08-003 > | Vertical significance
           | 0-10-004 > | Pressure
           | 0-12-001 > | Temperature
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-04-002 | VSPRWDWS   ;     ;  
           | 0-08-003 > | Vertical significance
           | 0-10-004 > | Pressure
           | 0-11-001 > | Wind direction
           | 0-11-002   | Wind speed

  3-04-003 | VSIGTEMP   ;     ;  
           | 0-08-003 > | Vertical significance
           | 0-12-001   | Temperature

  3-04-004 | VSPRCCTM   ;     ;  
           | 0-08-003 > | Vertical significance
           | 0-10-004 > | Pressure
           | 0-20-010 > | Cloud cover (total)
           | 0-12-001   | Temperature

  3-04-005 | IMHCMPRH   ;     ;  
           | 0-02-024 > | Integrated mean humidity computational method
           | 0-07-004 > | Pressure (1)
           | 0-07-004 > | Pressure (2)    defines layer
           | 0-13-003   | Relative humidity

  3-04-006 | OILWROSW   ;     ;  
           | 0-14-001 > | Outgoing long-wave radiation
           | 0-14-001 > | Incoming long-wave radiation
           | 0-14-003   | Outgoing short-wave radiation

  3-04-011 | GOESIMIN   ;     ; GOES-I/M info
           | 0-02-163 > | Height assignment method
           | 0-02-164 > | Tracer correlation method
           | 0-08-012 > | Land/sea qualifier
           | 0-07-024 > | Satellite zenith angle
           | 0-02-057 > | Origin of first guess information
           | 0-08-021 > | Time significance
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-08-021 > | Time significance
           | 0-04-024 > | Time period or displacement
           | 1-10-004 > | Replicate 10 descriptors 4 times
           | 0-08-021 > | Time significance
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-04-006 > | Second
           | 0-08-021 > | Time significance
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-04-006 > | Second
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 1-03-010 > | Replicate 3 descriptors 10 times
           | 0-02-163 > | Height assignment method
           | 0-07-004 > | Pressure
           | 0-12-001   | Temperature

  3-04-030 | LOCPLAT    ;     ; Location of platform
           | 0-27-031 > | In direction of 0 degree longitude, distance from the Earth's centre
           | 0-28-031 > | In direction of 90 degrees East longitude, distance from the Earth's centre
           | 0-10-031   | In direction of North Pole, distance from Earth's centre

  3-04-031 | SPDPLAT    ;     ; Speed of platform
           | 0-01-041 > | Absolute platform velocity - first component
           | 0-01-042 > | Absolute platform velocity - second component
           | 0-01-043   | Absolute platform velocity - third component

  3-04-032 | CLFRASEQ   ;     ; Cloud fraction
           | 0-02-153 > | Satellite channel centre frequency
           | 0-02-154 > | Satellite channel band width
           | 0-20-081 > | Cloud amount in segment
           | 0-20-082 > | Amount segment cloud free
           | 0-20-012   | Cloud type

  3-04-033 | CSRADSEQ   ;     ; Clear sky radiance
           | 0-02-152 > | Satellite instrument used in data processing
           | 0-02-166 > | Radiance type
           | 0-02-167 > | Radiance computational method
           | 0-02-153 > | Satellite channel centre frequency
           | 0-02-154 > | Satellite channel band width
           | 0-12-075 > | Spectral radiance
           | 0-12-076 > | Radiance
           | 0-12-063   | Brightness temperature

  3-04-034 | LLSEFCPQ   ;     ;  
           | 1-02-004 > | Replicating next two descriptors 4 times
           | 0-27-001 > | Latitude (high accuracy)
           | 0-28-001 > | Longitude (high accuracy)
           | 0-07-022 > | Solar elevation
           | 0-05-043 > | Field of view number
           | 0-20-010 > | Cloud cover (total)
           | 0-20-016 > | Pressure at top of cloud
           | 0-33-003 > | Quality information table
           | 0-10-040   | Number of retrieved layers

  3-05-003 | SADCHYCO   ;     ; SADC-HYCOS measurement array definition
           | 3-01-012 > | Hour, minute of first single measurement minus increment
           | 0-04-065 > | Short time increment - time interval between measuremens
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-05-001   | Single measurement

  3-05-006 | MEDHYCOM   ;     ; MEDHYCOS measurement
           | 0-13-072 > | Downstream water level
           | 0-13-082 > | Water temperature
           | 0-13-019 > | Precipitation last hour
           | 0-12-001 > | Air temperature
           | 0-13-073 > | Maximum water height observed
           | 0-13-060   | Total accumulated precipitation

  3-05-007 | MEDHYCOR   ;     ; MEDHYCOS report
           | 3-01-029 > | Identification
           | 3-01-012 > | Hour, minute (time of first measurement)
           | 0-04-065 > | Short time increment - time interval between measurements
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-05-006   | Single measurement

  3-05-008 | AOCHYCOM   ;     ; AOCHYCOS - Chad measurement
           | 3-05-006 > | Same as MEDHYCOS type measurement
           | 0-12-030   | Soil temperature at -50 cm

  3-05-009 | AOCHYVOR   ;     ; AOCHYCOS-Chad report
           | 3-01-029 > | Identification
           | 3-01-012 > | Hour, minute (time of first measurement)
           | 0-04-065 > | Short time increment - time interval between measurements
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-05-008   | Single measurement

  3-05-011 | MEDHYCO2   ;     ; MEDHYCOS report type 2
           | 3-01-029 > | Identification
           | 3-01-012 > | Hour, minute (time of first measurement)
           | 0-04-065 > | Short time increment - time interval between measurements
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-05-010   | Single measurement

  3-05-018 | MEDHYCOQ   ;     ; MEDHYCOS report with meteorology and water quality data
           | 3-01-029 > | Identification
           | 3-01-012 > | Hour, minute (time) of first measurement
           | 0-04-065 > | Hour increment
           | 1-03-000 > | Delayed replication of 3 descriptors
           | 0-31-001 > | Replication factor
           | 3-05-008 > | Same as AOCHYCOS type measurement
           | 3-05-016 > | Meteorological parameters associated to hydrological data
           | 3-05-017   | Water quality measurement

  3-06-001 | IDDBSSST   ;     ;  
           | 0-02-032 > | Indicator for digitization
           | 1-02-000 > | Delayed replication of 2 descriptors
           | 0-31-001 > | Replication factor
           | 0-07-062 > | Depth below sea surface
           | 0-22-042   | Subsurface sea temperature

  3-06-002 | MOCMDSOC   ;     ;  
           | 0-02-031 > | Method of current measurement (duration and time)
           | 0-22-004 > | Direction of current
           | 0-22-031   | Speed of current

  3-06-003 | WIWDWSDB   ;     ;  
           | 0-02-002 > | Wind instrumentation
           | 0-11-011 > | Wind direction (10 m)
           | 0-11-012 > | Wind speed (10 m)
           | 0-12-004   | Dry-bulb temperature (2 m)

  3-06-004 | IDMSMDBS   ;     ;  
           | 0-02-032 > | Indicator for digitization
           | 0-02-033 > | Method of salinity/depth measurement
           | 1-03-000 > | Delayed replication of 3 descriptors
           | 0-31-001 > | Replication factor
           | 0-07-062 > | Depth below sea surface
           | 0-22-043 > | Subsurface sea temperature
           | 0-22-062   | Salinity

  3-06-005 | MOCMDBDS   ;     ;  
           | 0-02-031 > | Method of current measurement (duration and time)
           | 1-03-000 > | Delayed replication of 3 descriptors
           | 0-31-001 > | Replication factor
           | 0-07-062 > | Depth below sea surface
           | 0-22-004 > | Direction of current
           | 0-22-031   | Speed of current

  3-06-006 | UWSNOPTP   ;     ; Under water sounding optional parameters
           | 3-06-003 > | Surface wind and temperature
           | 3-06-002 > | Current
           | 0-22-063   | Total water depth

  3-06-007 | BUOYSPAR   ;     ; Buoy spare block parameters
           | 0-01-012 > | Direction of motion of moving observing platform
           | 0-01-014 > | Platform drift speed (high precision)
           | 3-06-008 > | Buoy instrumentation
           | 0-04-024 > | Time period
           | 0-27-003 > | Alternate latitude
           | 0-28-003   | Alternate longitude

  3-06-008 | BUOYINST   ;     ; Buoy instrumentation parameters
           | 0-02-034 > | Drogue type
           | 0-02-035 > | Cable length
           | 0-02-036   | Buoy type

  3-06-019 | TIDECKTI   ;     ; Tide report identification, water level checks, time increments
           | 0-01-075 > | Tide station alphanumeric identification
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Hour, minute
           | 0-22-042 > | Sea/water temperature
           | 0-22-120 > | Tide station automated water level check
           | 0-22-121 > | Tide station manual water level check
           | 0-04-015 > | Time increment in minutes
           | 0-04-065   | Short time increment

  3-06-023 | NLALODTP   ;     ;  
           | 0-01-015 > | Station or site name
           | 3-01-023 > | Latitude, longitude
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Hour, minute
           | 0-22-038 > | Tidal level with respect to local chart datum
           | 0-22-039 > | Meteorological residual tidal elevation
           | 0-22-120 > | Tide station automated water level check
           | 0-22-121   | Tide station manual water level check

  3-07-001 | LOALSTNH   ;     ; Low altitude station
           | 3-01-031 > | Identification, type, date/time, position (high accuracy), height
           | 3-02-011   | Basic surface report

  3-07-002 | LOALSTNC   ;     ; Low altitude station
           | 3-01-032 > | Identification, type, date/time, position (coarse accuracy), height
           | 3-02-011   | Basic surface report

  3-07-003 | LOALSTCH   ;     ; Low altitude station
           | 3-07-001 > | Location (high accuracy) and basic report
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-02-005   | Cloud layer information

  3-07-004 | LOALSTCC   ;     ; Low altitude station
           | 3-07-002 > | Location (coarse accuracy) and basic report
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-02-005   | Cloud layer information

  3-07-005 | LOALST4H   ;     ; Low altitude station
           | 3-07-001 > | Location (high accuracy) and basic report
           | 1-01-004 > | Replicate 1 descriptor 4 times
           | 3-02-005   | Cloud layer information (4 layers)

  3-07-006 | LOALST4C   ;     ; Low altitude station
           | 3-07-002 > | Location (coarse accuracy) and basic report
           | 1-01-004 > | Replicate 1 descriptor 4 times
           | 3-02-005   | Cloud layer information (4 layers)

  3-07-007 | HIALSTNH   ;     ; High altitude station
           | 3-01-031 > | Identification, type, date/time, position (high accuracy), height
           | 3-02-012   | Basic surface report

  3-07-008 | HIALSTNC   ;     ; High altitude station
           | 3-01-032 > | Identification, type, date/time, position (coarse accuracy), height
           | 3-02-012   | Basic surface report

  3-07-009 | ITDALALO   ;     ;  
           | 3-01-031 > | Identification, type, date/time, position (high accuracy), height
           | 3-02-013   | Basic surface report

  3-07-011 | METARSPE   ;     ; Main part of data for representation of METAR/SPECI code in BUFR
           | 0-01-063 > | ICAO location indicator
           | 0-02-001 > | Type of station
           | 3-01-011 > | Year, month, day (YY)
           | 3-01-012 > | GG, gg
           | 3-01-024 > | Latitude, longitude (coarse accuracy), height of station
           | 0-07-006 > | Height above station (= height of an anemometer)
           | 0-11-001 > | Wind direction
           | 0-11-016 > | Extreme counterclockwise wind direction of a variable wind
           | 0-11-017 > | Extreme clockwise wind direction of a variable wind
           | 0-11-002 > | Wind speed
           | 0-11-041 > | Maximum wind speed (gusts)
           | 0-07-006 > | Height above station (= height of a thermometer)
           | 0-12-001 > | Temperature
           | 0-12-003 > | Dew-point temperature
           | 0-10-052 > | Altimeter setting (QNH)
           | 0-20-009   | General Weather Indicator TAF/METAR

  3-07-012 | DSVWWSEQ   ;     ; DvVVVV
           | 1-03-000 > | Delayed replication of 3 descriptors
           | 0-31-001 > | Number of replication (up to 3)
           | 0-08-023 > | First order statistics
           | 0-05-021 > | Direction of visibility observed
           | 0-20-001   | Horizontal visibility

  3-07-013 | DSR2VSR4   ;     ; DRDRVRVRVRVR
           | 1-06-000 > | Delayed replication of 6 descriptors
           | 0-31-001 > | Number of replication (up to 4)
           | 0-01-064 > | Runway designator
           | 0-08-014 > | Qualification for runway visual range
           | 0-20-061 > | Runway visual range
           | 0-08-014 > | Qualification for runway visual range
           | 0-20-061 > | Runway visual range
           | 0-20-018   | Tendency of runway visual range

  3-07-014 | WPRIMEWS   ;     ; w'w' 
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Number of replication (up to 3)
           | 0-20-019   | Significant present weather

  3-07-015 | CLOUDGRP   ;     ; Clouds groups
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Number of replication
           | 3-02-005 > | (NsNsNs, CC, hshshs)
           | 0-20-002   | Vertical visibility

  3-07-016 | REWPRMEW   ;     ; REw'w'
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Number of replication (up to 3)
           | 0-20-020   | Significant recent weather phenomena

  3-07-017 | WSHRRWAY   ;     ; Wind shear on runwayss
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Number of replication
           | 0-11-070   | Runway designator of the runway affected by wind shear (including ALL)

  3-07-018 | TTYPLFST   ;     ; Trend-type landing forecast
           | 0-08-016 > | Change qualifier of a trend-type forecast or an aerodrome forecast
           | 1-02-000 > | Delayed replication of 2 descriptors
           | 0-31-001 > | Number of replication (up to 2)
           | 0-08-017 > | Qualifier of the time when the forecast change is expected (FM, TL, AT)
           | 3-01-012 > | GG, gg
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Number of replication (up to 1)
           | 0-07-006 > | Height above station
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-11-041 > | Maximum wind speed (gusts)
           | 0-20-009 > | General Weather Indicator
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Number of replication (up to 1)
           | 0-20-001 > | Horizontal visibility
           | 3-07-014   | w'w'

  3-07-020 | SMETARSP   ;     ; Short METAR/SPECI
           | 3-07-011 > | Main part of data
           | 3-07-014 > | w'w'
           | 3-07-016   | REw'w'

  3-07-021 | TMETARSP   ;     ; Total sequence for representation of METAR/SPECI code in BUFR
           | 3-07-011 > | Main part of data
           | 3-07-012 > | DvVVVV
           | 3-07-013 > | DRDRVRVRVRVR
           | 3-07-014 > | w'w'
           | 3-07-015 > | Clouds group(s)
           | 3-07-016 > | REw'w'
           | 3-07-017 > | Wind shear on runway(s)
           | 3-07-018 > | Trend-type landing forecast
           | 3-07-015   | Clouds group(s)

  3-07-022 | GBGNSSDA   ;     ; Ground-based GNSS data
           | 0-01-015 > | Station or site name
           | 3-01-011 > | Year, Month, Day
           | 3-01-012 > | Hour, Minute
           | 3-01-022 > | Latitude (high accuracy), Longitude (high accuracy), Height of station
           | 0-08-021 > | Time significance (= 23, monitoring period)
           | 0-04-025 > | Time period or displacement
           | 0-10-004 > | Pressure
           | 0-12-001 > | Temperature
           | 0-13-003 > | Relative humidity
           | 0-33-038 > | Quality flags for ground-based GNSS data
           | 0-08-022 > | Total number (Number of GNSS satellites used)
           | 1-06-025 > | Replication
           | 0-02-020 > | Satellite classification
           | 0-01-050 > | Platform transmitter Id. number
           | 0-05-021 > | Azimuth
           | 0-07-021 > | Elevation
           | 0-15-031 > | Atmospheric path delay in satellite signal
           | 0-15-032 > | Estimated error in atmospheric path delay
           | 0-08-060 > | Sample scanning mode significance (=5 for North/South)
           | 0-15-033 > | Difference in path delays for limb views at extremes of scan
           | 0-15-034 > | Estimated error in path delay difference
           | 0-08-060 > | Sample scanning mode significance (=6 for East/West)
           | 0-15-033 > | Difference in path delays for limb views at extremes of scan
           | 0-15-034 > | Estimated error in path delay difference
           | 0-15-035 > | Component of zenith path delay due to water vapour
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-13-016 > | Precipitable water
           | 2-02-000 > | Reset scale
           | 2-01-000 > | Reset data width
           | 0-15-011   | Log10 of integrated electron density

  3-07-071 | MNTHVLND   ;     ; Monthly values of a land station - CLIMAT Data of the month
           | 3-01-090 > | Surface station identification, time, horizontal and vertical co-ordinates
           | 0-04-074 > | Short time displacement (= UTC - LST)
           | 0-04-023 > | Time period ( = number of days in the month)
           | 0-08-023 > | First order statistics = 4, mean value
           | 0-10-004 > | Pressure
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-07-004 > | Pressure (standard level) (for lowland stations = missing value)
           | 0-10-009 > | Geopotential height of the standard level (for lowland stations = missing value)
           | 0-07-032 > | Height of sensor above local ground
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-02-051 > | Indicator to specify observing method for extreme temperatures
           | 0-04-051 > | Principal time of daily reading of maximum temperature
           | 0-12-118 > | Maximum temperature at height specified, past 24 hours
           | 0-04-052 > | Principal time of daily reading of minimum temperature
           | 0-12-119 > | Minimum temperature at height specified, past 24 hours
           | 0-13-004 > | Vapour pressure
           | 0-08-023 > | First order statistics (=63, missing value)
           | 0-12-151 > | Standard deviation of daily mean temperature
           | 0-07-032 > | Height of sensor above local ground (set to missing to cancel the previous value)
           | 1-02-005 > | Replicate 2 descriptors 5 times
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic.
           | 0-08-020 > | Total number of missing entities (days)
           | 0-14-032 > | Total sunshine
           | 0-14-033 > | Total sunshine
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic
           | 0-08-020 > | Total number of missing entities (days)
           | 1-02-018 > | Replicate 2 descriptors 18 times (Number of days of occurrence)
           | 0-08-052 > | Conditions for which number of days of occurrence follows
           | 0-08-022 > | Total number (of days)
           | 0-07-032 > | Height of sensor above local ground
           | 0-08-053 > | Day of occurrence qualifier  = 0 (on 1 day only), = 1 (on 2 or more days)
           | 0-04-003 > | Day
           | 0-12-152 > | Highest daily mean temperature
           | 0-08-053 > | Day of occurrence qualifier  = 0 (on 1 day only), = 1 (on 2 or more days)
           | 0-04-003 > | Day
           | 0-12-153 > | Lowest daily mean temperature
           | 0-08-053 > | Day of occurrence qualifier  = 0 (on 1 day only), = 1 (on 2 or more days)
           | 0-04-003 > | Day
           | 0-08-023 > | First order statistics ( = 2, maximum value)
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-08-053 > | Day of occurrence qualifier  = 0 (on 1 day only), = 1 (on 2 or more days)
           | 0-04-003 > | Day
           | 0-08-023 > | First order statistics (= 3, minimum value)
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-08-023 > | First order statistics (= 63, missing value)
           | 0-07-032 > | Height of sensor above local ground
           | 0-02-002 > | Type of instrumentation for wind measurement
           | 0-08-053 > | Day of occurrence qualifier = 0 (on 1 day only), = 1 (on 2 or more days)
           | 0-04-003 > | Day
           | 0-11-046 > | Maximum instantaneous wind speed
           | 0-08-053 > | Day of occurrence qualifier (set to missing = 3 to cancel the previous value)
           | 0-04-003 > | Day (= 1) (Precipitation)
           | 0-04-004 > | Hour (= 6)
           | 0-04-023 > | Time period (= number of days in the month)
           | 0-07-032 > | Height of sensor above local ground
           | 0-13-060 > | Total accumulated precipitation
           | 0-13-051 > | Frequency group, precipitation
           | 0-04-053 > | Number of days with precipitation equal to or more than 1 mm
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic, = 5 (precipitation)
           | 0-08-020 > | Total number of missing entities (days)
           | 1-02-006 > | Replicate 2 descriptors 6 times (Number of days of occurrence)
           | 0-08-052 > | Conditions for which number of days of occurrence follows
           | 0-08-022 > | Total number (of days)
           | 0-08-053 > | Day of occurrence qualifier = 0 (on 1 day only), = 1 (on 2 or more days) (Occurrence of extreme precipitation)
           | 0-04-003 > | Day
           | 0-13-052 > | Highest daily amount of precipitation
           | 0-07-032   | Height of sensor above local ground (set to missing to cancel the previous value)

  3-07-072 | MNTHNLND   ;     ; Monthly normals from a land station
           | 0-04-001 > | Year (of beginning of the reference period)
           | 0-04-001 > | Year (of ending of the reference period)
           | 0-04-002 > | Month
           | 0-04-003 > | Day  (= 1)
           | 0-04-004 > | Hour (= 0)
           | 0-04-074 > | Short time displacement (= UTC- LST)
           | 0-04-022 > | Time period (= 1)
           | 0-08-023 > | First order statistics (= 4, mean value)
           | 0-10-004 > | Pressure
           | 0-10-051 > | Pressure reduced to Mean Sea Level
           | 0-07-004 > | Pressure (standard level)
           | 0-10-009 > | Geopotential height of the standard level
           | 0-07-032 > | Height of sensor above local ground
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-02-051 > | Indicator to specify observing method for extreme temperatures
           | 0-04-051 > | Principal time of daily reading of maximum temperature
           | 0-12-118 > | Maximum temperature at height specified, past 24 h.
           | 0-04-052 > | Principal time of daily reading of minimum temperature
           | 0-12-119 > | Minimum temperature at height specified, past 24 h.
           | 0-13-004 > | Vapour pressure
           | 0-12-151 > | Standard deviation of daily mean temperature
           | 0-07-032 > | Height of sensor above local ground (set to missing to cancel the previous value)
           | 0-14-032 > | Total sunshine (Normal of sunshine duration)
           | 0-08-023 > | First order statistics (= 63, missing value)
           | 0-04-001 > | Year (of beginning of the reference period) (Normals of precipitation)
           | 0-04-001 > | Year (of ending of the reference period)
           | 0-04-002 > | Month
           | 0-04-003 > | Day (= 1)
           | 0-04-004 > | Hour (= 6)
           | 0-04-022 > | Time period (= 1)
           | 0-07-032 > | Height of sensor above local ground
           | 0-08-023 > | First order statistics (= 4, mean value)
           | 0-13-060 > | Total accumulated precipitation
           | 0-04-053 > | Number of days with precipitation equal to or more than 1 mm
           | 0-08-023 > | First order statistics (= 63, missing value)
           | 1-02-008 > | Replicate 2 descriptors 8 times
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic.
           | 0-08-020   | Total number of missing entities (years)

  3-07-073 | CLIMATML   ;     ; Representation of CLIMAT data of the actual month and for monthly normals
           | 3-07-071 > | Monthly values of a land station - CLIMAT Data of the month
           | 3-07-072   | Monthly normals from a land station

  3-07-080 | SYNFLNDS   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-07-081 | SYNFLND1   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA I
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance (= missing to cancel the previous value)
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 0-12-122 > | Ground minimum temperature of the preceding night
           | 0-13-056 > | Character and intensity of precipitation
           | 0-13-057 > | Time of beginning or end of precipitation
           | 0-20-101 > | Locust (acridian) name
           | 0-20-102 > | Locust (maturity) color
           | 0-20-103 > | Stage of development of locusts
           | 0-20-104 > | Organization state of swarm or band of locusts
           | 0-20-105 > | Size of swarm or band of locusts and duration of passage of swarm
           | 0-20-106 > | Locust population density
           | 0-20-107 > | Direction of movements of locust swarm
           | 0-20-108 > | Extent of vegetation
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-07-082 | SYNFLND2   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA II
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance (= missing to cancel the previous value)
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 0-12-121 > | Ground minimum temperature (at the time of observation)
           | 0-12-122 > | Ground minimum temperature of the preceding night
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-07-083 | SYNFLND3   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA III
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance (= missing to cancel the previous value)
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 0-12-122 > | Ground minimum temperature of the preceding night
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-07-084 | SYNFLND4   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA IV
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance (= missing to cancel the previous value)
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 0-20-055 > | State of sky in tropics
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 2-05-001 > | Character field of 1 character
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-07-086 | SYNFLND6   ;     ; Sequence for representation of synoptic reports from a fixed land station suitable for SYNOP data in compliance with reporting practices in RA VI
           | 3-01-090 > | Fixed surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 0-08-002 > | Vertical significance (= missing to cancel the previous value)
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 3-02-066 > | Dangerous weather phenomena
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045   | Radiation data (from 1 hour and/or 24 hour period)

  3-07-090 | SYNMLNDS   ;     ; Sequence for representation of synoptic reports from a mobile land station suitable for SYNOP MOBIL data
           | 3-01-092 > | Mobile surface station identification, time, horizontal and vertical coordinates
           | 3-02-031 > | Pressure data
           | 3-02-035 > | Basic synoptic 'instantaneous' data
           | 3-02-036 > | Clouds with bases below station level
           | 3-02-047 > | Direction of cloud drift
           | 0-08-002 > | Vertical significance
           | 3-02-048 > | Direction and elevation of cloud
           | 3-02-037 > | State of ground, snow depth, ground minimum temperature
           | 3-02-043 > | Basic synoptic 'period' data
           | 3-02-044 > | Evaporation data
           | 1-01-002 > | Replicate next descriptor 2 times
           | 3-02-045 > | Radiation data (from 1 hour and/or 24 hour period)
           | 3-02-046   | Temperature change

  3-08-001 | BUOYFIXH   ;     ; Buoy/platform - fixed
           | 3-01-033 > | Identification, type, date/time, position (high accuracy)
           | 3-02-011 > | Basic surface report
           | 0-22-042   | Sea-surface temperature

  3-08-002 | BUOYFIXC   ;     ; Buoy/platform - fixed
           | 3-01-034 > | Identification, type, date/time, position (coarse accuracy)
           | 3-02-011 > | Basic surface report
           | 0-22-042   | Sea-surface temperature

  3-08-003 | BUOYMOVE   ;     ; Buoy/platform - moving
           | 3-01-035 > | Identification, movement, type, date/time, position (coarse accuracy)
           | 3-02-011 > | Basic surface report
           | 0-22-042   | Sea-surface temperature

  3-08-004 | SHIPSEQ2   ;     ; Ship
           | 3-01-036 > | Identification, movement, type, date/time, position (coarse accuracy)
           | 3-02-011 > | Basic surface report
           | 0-22-042   | Sea-surface temperature

  3-08-005 | SHIPWASW   ;     ;  
           | 3-08-004 > | Basic ship report
           | 3-02-024   | Wind waves and swell waves

  3-08-006 | BUOYSEC1   ;     ; Buoy Section 1 optional parameters
           | 0-10-004 > | Pressure
           | 0-10-061 > | 3-hour pressure change
           | 0-10-063 > | Characteristic of pressure tendency
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-12-004 > | Dry-bulb temperature at 2 m
           | 0-13-003 > | Relative humidity
           | 0-22-042   | Sea temperature

  3-08-007 | IDMDLBDS   ;     ;
           | 3-01-055 > | Identification, movement type, date/time, position (high accuracy)
           | 3-02-011 > | Basic surface report
           | 0-07-062 > | Depth below sea/water surface
           | 0-22-042   | Sea/water temperature

  3-08-009 | SYNPSHIP   ;     ; Sequence for representation of synoptic reports from a sea station suitable for SHIP data
           | 3-01-093 > | Ship identification, movement, date/time, horizontal and vertical coordinates
           | 3-02-001 > | Pressure data
           | 3-02-054 > | SHIP 'instantaneous' data
           | 0-08-002 > | Vertical significance
           | 3-02-055 > | Icing and ice
           | 3-02-057 > | SHIP marine data
           | 3-02-060   | SHIP 'period' data

  3-08-010 | TRACKOBB   ;     ; TRACKOB Template
           | 0-01-011 > | Ship or mobile land station identifier
           | 1-13-000 > | Delayed replication of 13 descriptors
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021 > | Latitude/Longitude (high accuracy)
           | 0-04-080 > | Averaging period for following value
           | 0-22-049 > | Sea surface temperature
           | 0-04-080 > | Averaging period for following value
           | 0-22-059 > | Sea surface salinity
           | 0-04-080 > | Averaging period for following value
           | 0-22-005 > | Direction of sea surface current
           | 0-02-042 > | Indicator for sea surface current speed
           | 0-22-032 > | Speed of sea surface current
           | 0-02-042 > | Indicator for sea surface current speed (cancel)
           | 0-04-080   | Averaging period for following value (cancel)

  3-08-011 | MNTHVSEA   ;     ; Monthly values from an ocean weather station - CLIMAT SHIP
           | 0-01-011 > | Ship's call sign
           | 0-02-001 > | Type of station
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023 > | Latitude (coarse accuracy), Longitude (coarse accuracy)
           | 0-07-030 > | Height of station platform above mean sea level
           | 0-07-031 > | Height of barometer above mean sea level
           | 0-04-074 > | Short time displacement (= UTC - LST)
           | 0-04-023 > | Time period  (=  number of days in the month)
           | 0-08-023 > | First order statistics  (= 4, mean value)
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-07-032 > | Height of sensor above marine deck platform (for temperature measurement)
           | 0-07-033 > | Height of sensor above water surface (for temperature measurement)
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-13-004 > | Vapour pressure
           | 0-07-032 > | Height of sensor above marine deck platform (set to missing to cancel the previous value)
           | 0-07-033 > | Height of sensor above water surface (set to missing to cancel the previous value)
           | 3-02-056 > | Sea surface temperature, method of measurement, and depth below sea surface
           | 0-08-023 > | First order statistics  (= 63, missing value)
           | 0-04-003 > | Day (= 1) (Precipitation)
           | 0-04-004 > | Hour(= 6)
           | 0-04-023 > | Time period (= number of days in the month)
           | 0-07-032 > | Height of sensor above marine deck platform
           | 0-13-060 > | Total accumulated precipitation
           | 0-13-051 > | Frequency group, precipitation
           | 0-04-053 > | Number of days with precipitation equal to or more than 1 mm
           | 0-07-032   | Height of sensor above marine deck platform (set to missing to cancel the previous value)

  3-08-012 | MNTHNSEA   ;     ; Monthly normals from an ocean weather station
           | 0-04-001 > | Year (of beginning of the reference period)
           | 0-04-001 > | Year (of ending of the reference period)
           | 0-04-002 > | Month
           | 0-04-003 > | Day (= 1)
           | 0-04-004 > | Hour (= 0)
           | 0-04-074 > | Short time displacement (= UTC - LST)
           | 0-04-022 > | Time period (= 1)
           | 0-08-023 > | First order statistics (= 4, mean value)
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-07-032 > | Height of sensor above marine deck platform (for temperature measurement)
           | 0-07-033 > | Height of sensor above water surface (for temperature measurement)
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-13-004 > | Vapour pressure
           | 0-07-032 > | Height of sensor above marine deck platform (set to missing to cancel the previous value)
           | 0-07-033 > | Height of sensor above water surface (set to missing to cancel the previous value)
           | 3-02-056 > | Sea surface temperature, method of measurement, and depth below sea surface
           | 0-08-023 > | First order statistics  (= 63, missing value)
           | 0-04-001 > | Year (of beginning of the reference period)
           | 0-04-001 > | Year (of ending of the reference period)
           | 0-04-002 > | Month
           | 0-04-003 > | Day (= 1)
           | 0-04-004 > | Hour (= 6)
           | 0-04-022 > | Time period (= 1)
           | 0-07-032 > | Height of sensor above marine deck platform (for precipitation measurement)
           | 0-08-023 > | First order statistics  (= 4, mean value)
           | 0-13-060 > | Total accumulated precipitation
           | 0-04-053 > | Number of days with precipitation equal to or more than 1 mm
           | 0-08-023   | First order statistics  (= 63, missing value)

  3-08-013 | CLIMATMS   ;     ; Representation of CLIMAT SHIP data of the actual month and for monthly normals
           | 3-08-011 > | Monthly values from an ocean weather station - CLIMAT SHIP
           | 3-08-012   | Monthly normals from an ocean weather station

  3-09-001 | VRTWNLHH   ;     ; Vertical wind profile
           | 3-01-037 > | Identification, etc. (land station, high accuracy position)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-011   | Winds at heights

  3-09-002 | VRTWNDHC   ;     ; Vertical wind profile
           | 3-01-038 > | Identification, etc. (land station, coarse accuracy position)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-011   | Winds at heights

  3-09-003 | VRTWNDPH   ;     ; Vertical wind profile
           | 3-01-037 > | Identification, etc. (land station, high accuracy position)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-012   | Winds at pressure levels

  3-09-004 | VRTWNDPC   ;     ; Vertical wind profile
           | 3-01-038 > | Identification, etc. (land station, coarse accuracy position)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-012   | Winds at pressure levels

  3-09-005 | VRTSDRLH   ;     ; Vertical sounding with relative humidity
           | 3-01-037 > | Identification, etc. (land station, high accuracy position)
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-013   | Pressure, geopotential, temperature and wind data

  3-09-006 | VRTSDRHC   ;     ; Vertical sounding with relative humidity
           | 3-01-038 > | Identification, etc. (land station, coarse accuracy position)
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-013   | Pressure, geopotential, temperature and wind data

  3-09-007 | VRTSDDLH   ;     ; Vertical sounding with dew-point data
           | 3-01-037 > | Identification, etc. (land station, high accuracy position)
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-014   | Pressure, geopotential, temperature and wind data

  3-09-008 | VRTSDDPC   ;     ; Vertical sounding with dew-point data
           | 3-01-038 > | Identification, etc. (land station, coarse accuracy position)
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-014   | Pressure, geopotential, temperature and wind data

  3-09-011 | VRTWNDSH   ;     ; Vertical wind profile
           | 3-01-039 > | Ship's identification, etc.
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-011   | Winds at heights

  3-09-012 | VRTWNDSP   ;     ; Vertical wind profile
           | 3-01-039 > | Ship's identification, etc.
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-012   | Winds at pressure levels

  3-09-013 | VRTSDRHS   ;     ; Vertical sounding with relative humidity
           | 3-01-039 > | Ship's identification, etc.
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-013   | Pressure, geopotential, temperature and wind data

  3-09-014 | VRTSDDPS   ;     ; Vertical sounding with dew-point data
           | 3-01-039 > | Ship's identification, etc.
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-014   | Pressure, geopotential, temperature and wind data

  3-09-015 | VRTWNSHH   ;     ; Vertical wind profile
           | 3-01-040 > | Ship's identification, etc.
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-011   | Winds at heights

  3-09-016 | VRTWNDHP   ;     ; Vertical wind profile
           | 3-01-040 > | Ship's identification, etc.
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-012   | Winds at pressure levels

  3-09-017 | VRTSDRSH   ;     ; Vertical sounding with relative humidity
           | 3-01-040 > | Ship's identification, etc.
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-013   | Pressure, geopotential, temperature and wind data

  3-09-018 | VRTSDDSH   ;     ; Vertical sounding with dew-point data
           | 3-01-040 > | Ship's identification, etc.
           | 3-02-004 > | Significant cloud information
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-014   | Pressure, geopotential, temperature and wind data

  3-09-019 | WNPROFSD   ;     ; Wind profiler - wind data sounding
           | 3-01-031 > | Identification, etc.
           | 0-02-003 > | Type of measuring equipment used
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-03-011   | Winds at heights

  3-09-020 | WNPROFCC   ;     ; Wind profiler - Cartesian coordinates
           | 3-01-031 > | Identification, etc.
           | 0-02-003 > | Type of measuring equipment used
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Replication factor
           | 0-07-003 > | Geopotential
           | 0-11-003 > | u-component
           | 0-11-004 > | v-component
           | 0-11-005   | w-component

  3-09-030 | OZSNDFLT   ;     ; Ozone sonde flight data
           | 0-15-004 > | Ozone sounding correction factor
           | 0-15-005 > | Ozone p
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Replication factor
           | 0-04-015 > | Time increment since launch time, if needed; in minutes
           | 0-08-006 > | Ozone vertical sounding significance
           | 0-07-004 > | Pressure
           | 0-15-003   | Measured ozone partial pressure

  3-09-031 | OZONFLTD   ;     ; Ozone sonde flight data
           | 0-15-004 > | Ozone sounding correction factor
           | 0-15-005 > | Ozone p
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Replication factor
           | 0-04-025 > | Time displacement (since launch time) in minutes
           | 0-08-006 > | Ozone vertical sounding significance
           | 0-07-004 > | Pressure
           | 0-15-003   | Measured ozone partial pressure

  3-09-050 | PILOTSMP   ;     ; Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with pressure as the vertical coordinate
           | 3-01-110 > | Identification of launch site and instrumentation for wind measurements
           | 3-01-113 > | Date/time of launch
           | 3-01-114 > | Horizontal and vertical coordinates of launch site
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 3-03-050 > | Wind data at a pressure level
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-051   | Wind shear data at a pressure level

  3-09-051 | PILOTSMH   ;     ; Sequence for representation of PILOT, PILOT SHIP and PILOT MOBIL observation type data with height as the vertical coordinate
           | 3-01-110 > | Identification of launch site and instrumentation for wind measurements
           | 3-01-113 > | Date/time of launch
           | 3-01-114 > | Horizontal and vertical coordinates of launch site
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 3-03-052 > | Wind data at a height level
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-053   | Wind shear data at a height level

  3-09-052 | TEMPSHMO   ;     ; Sequence for representation of TEMP, TEMP SHIP and TEMP MOBIL observation type data
           | 3-01-111 > | Identification of launch site and instrumentation for P, T, U and wind measurements
           | 3-01-113 > | Date/time of launch
           | 3-01-114 > | Horizontal and vertical coordinates of launch site
           | 3-02-049 > | Cloud information reported with vertical soundings
           | 0-22-043 > | Sea water temperature
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 3-03-054 > | Temperature, dew-point and wind data at a pressure level
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-051   | Wind shear data at a pressure level

  3-09-053 | TEMPDROP   ;     ; Sequence for representation of TEMP DROP observation type data
           | 3-01-112 > | Identification of launch point and instrumentation of dropsonde
           | 3-01-113 > | Date/time of launch
           | 3-01-114 > | Horizontal and vertical coordinates of launch site
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 3-03-054 > | Temperature, dew-point and wind data at a pressure level
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-051   | Wind shear data at a pressure level

  3-09-054 | CLIMATTS   ;     ; Sequence for representation of CLIMAT TEMP and CLIMAT TEMP SHIP data
           | 3-01-001 > | Identification of launch site
           | 0-01-011 > | Ship's call sign
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021 > | Horizontal and vertical coordinates
           | 0-07-030 > | Height of station ground above mean sea level
           | 0-07-031 > | Height of barometer above mean sea level
           | 0-07-007 > | Height release of sonde above mean sea level
           | 0-04-023 > | Time period (= number of days in the month) (Monthly mean data)
           | 0-04-059 > | Times of observations used to compute the reported mean values
           | 1-15-000 > | Delayed replication of 15 descriptors
           | 0-31-001 > | Delayed descriptor replication factor
           | 0-08-001 > | Vertical sounding  significance
           | 0-08-023 > | First order statistics (= 4, mean value)
           | 0-07-004 > | Pressure
           | 0-10-009 > | Geopotential height
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-12-103 > | Dew-point temperature
           | 0-08-023 > | First order statistics (= 32, vector mean)
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-08-023 > | First order statistics (= 63, missing value)
           | 0-11-019 > | Steadiness of wind
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic (= 2, temperature)
           | 0-08-020 > | Total number of missing entities (days)
           | 0-08-050 > | Qualifier for number of missing values in calculation of statistic (= 9, wind)
           | 0-08-020   | Total number of missing entities (days)

  3-09-060 | RAOBRGSF   ;     ; Radiosonde complete registration and surface observation
           | 3-01-123 > | Radiosonde full header information
           | 3-01-121 > | Radiosonde launch point location
           | 3-02-050 > | Radiosonde surface observation
           | 3-03-040   | Radiosonde duration of flight and termination information

  3-09-061 | RAWPTUSQ   ;     ; Raw PTU
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second)
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-25-069 > | Flight level pressure correction
           | 0-07-004 > | Pressure
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-33-007 > | Percent confidence (for Pressure)
           | 0-33-035 > | Manual/automatic quality control (for Pressure)
           | 0-33-015 > | Data quality-check indicator (for Pressure)
           | 0-13-009 > | Relative humidity
           | 0-33-007 > | Percent confidence (for Relative humidity)
           | 0-33-035 > | Manual/automatic quality control (for Relative humidity)
           | 0-33-015 > | Data quality-check indicator (for Relative humidity)
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-12-101 > | Temperature/dry bulb temperature
           | 0-33-007 > | Percent confidence (for Temperature)
           | 0-33-035 > | Manual/automatic quality control (for Temperature)
           | 0-33-015   | Data quality-check indicator (for Temperature)

  3-09-062 | RAWGPSUS   ;     ; Raw GPS unsmoothed wind
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second)
           | 0-05-001 > | Latitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Latitude)
           | 0-33-015 > | Data quality-check indicator (for Latitude)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Longitude)
           | 0-33-015 > | Data quality-check indicator (for Longitude)
           | 0-07-007 > | Height
           | 0-33-035 > | Manual/automatic quality control (for Height)
           | 0-33-015 > | Data quality-check indicator (for Height)
           | 0-11-003 > | U-component
           | 0-33-035 > | Manual/automatic quality control (for U-component)
           | 0-33-015 > | Data quality-check indicator (for U-component)
           | 0-11-004 > | V-component
           | 0-33-035 > | Manual/automatic quality control (for V-component)
           | 0-33-015 > | Data quality-check indicator (for V-component)
           | 0-33-007   | Percent confidence (for Raw GPS unsmoothed wind)

  3-09-063 | RAWGPSSM   ;     ; Raw GPS smoothed wind
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second) sequence
           | 0-05-001 > | Latitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Latitude)
           | 0-33-015 > | Data quality-check indicator (for Latitude)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Longitude)
           | 0-33-015 > | Data quality-check indicator (for Longitude)
           | 0-07-007 > | Height
           | 0-33-035 > | Manual/automatic quality control (for Height)
           | 0-33-015 > | Data quality-check indicator (for Height)
           | 0-11-003 > | U-component
           | 0-33-035 > | Manual/automatic quality control (for U-component)
           | 0-33-015 > | Data quality-check indicator (for U-component)
           | 0-11-004 > | V-component
           | 0-33-035 > | Manual/automatic quality control (for V-component)
           | 0-33-015 > | Data quality-check indicator (for V-component)
           | 0-33-007   | Percent confidence (for Raw GPS smoothed wind)

  3-09-064 | PROCPTUS   ;     ; Processed PTU
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second)
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 1-04-002 > | Replicate 4 descriptors 2 times
           | 0-25-069 > | Flight level pressure correction
           | 0-07-004 > | Pressure
           | 0-33-035 > | Manual/automatic quality control (for Pressure)
           | 0-33-015 > | Data quality-check indicator (for Pressure)
           | 0-13-003 > | Relative humidity
           | 0-33-035 > | Manual/automatic quality control (for Relative humidity)
           | 0-33-015 > | Data quality-check indicator (for Relative humidity)
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 1-04-002 > | Replicate 4 descriptors 2 times
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-12-101 > | Temperature/dry bulb temperature
           | 0-33-035 > | Manual/automatic quality control (for Temperature)
           | 0-33-015 > | Data quality-check indicator (for Temperature)
           | 0-12-103 > | Dew-point temperature
           | 0-33-035 > | Manual/automatic quality control (for Dew-point temperature)
           | 0-33-015 > | Data quality-check indicator (for Dew-point temperature)
           | 0-10-009 > | Geopotential height
           | 0-33-035 > | Manual/automatic quality control (for Geopotential height)
           | 0-33-015   | Data quality-check indicator (for Geopotential height)

  3-09-065 | PROCGPSS   ;     ; Processed GPS
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second)
           | 0-05-001 > | Latitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Latitude)
           | 0-33-015 > | Data quality-check indicator (for Latitude)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-33-035 > | Manual/automatic quality control (for Longitude)
           | 0-33-015 > | Data quality-check indicator (for Longitude)
           | 0-07-007 > | Height
           | 0-33-035 > | Manual/automatic quality control (for Height)
           | 0-33-015 > | Data quality-check indicator (for Height)
           | 0-11-003 > | U-component
           | 0-33-035 > | Manual/automatic quality control (for U-component)
           | 0-33-015 > | Data quality-check indicator (for U-component)
           | 0-11-004 > | V-component
           | 0-33-035 > | Manual/automatic quality control (for V-component)
           | 0-33-015   | Data quality-check indicator (for V-component)

  3-09-066 | STDSIGLV   ;     ; Standard and significant levels
           | 3-01-120 > | Radiosonde abbreviated header and launch information
           | 0-08-041 > | Data significance (6 = "flight level observation" )
           | 3-01-122 > | Date/time (to hundredths of second)
           | 0-08-040 > | Flight level significance
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-25-069 > | Flight level pressure correction
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-02-013 > | Solar and infrared radiation correction
           | 0-12-101 > | Temperature/dry bulb temperature
           | 0-12-103 > | Dew-point temperature
           | 0-10-009 > | Geopotential height
           | 0-10-007 > | Height
           | 0-11-002 > | Wind speed
           | 0-11-001   | Wind direction

  3-10-001 | SATBTEMP   ;     ; Satellite - brightness temperature
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-032 > | Cloud
           | 1-01-026 > | Replicate 1 descriptor 26 times
           | 3-03-025   | Satellite channel and brightness temperature

  3-10-002 | SATLLEVL   ;     ; Satellite - low level
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-032 > | Cloud
           | 1-01-009 > | Replicate 1 descriptor 9 times
           | 3-03-023   | Layer mean temperature

  3-10-003 | SATHLEVL   ;     ; Satellite - high level
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-032 > | Cloud
           | 1-01-006 > | Replicate 1 descriptor 6 times
           | 3-03-023   | Layer mean temperature

  3-10-004 | SATPWATR   ;     ; Satellite - precipitable water
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-032 > | Cloud
           | 1-01-003 > | Replicate 1 descriptor 3 times
           | 3-03-024   | Precipitable water

  3-10-005 | IMDLSCSB   ;     ;  
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-033 > | Cloud
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-025   | Satellite channel and brightness temperature

  3-10-006 | IMDLSCLT   ;     ;  
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-033 > | Cloud
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-023   | Layer mean temperature

  3-10-007 | IMDLSCPW   ;     ;  
           | 3-01-042 > | Identification, method, date/time
           | 3-03-031 > | Significance data, land/sea, skin temperature
           | 3-03-033 > | Cloud
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-03-024   | Precipitable water

  3-10-008 | ATOVHIRS   ;     ; ATOVS HIRS report
           | 3-10-011 > | ATOVS field of view variables
           | 1-01-019 > | Replicate 1 descriptor 19 times
           | 3-10-012 > | ATOVS channel variables
           | 0-02-150 > | TOVS/ATOVS/AVHRR instrumentation channel number
           | 0-25-079 > | Albedo-radiance solar filtered irradiance for ATOVS
           | 0-25-080 > | Albedo-radiance equivalent filter width for ATOVS
           | 0-33-032 > | Channel quality flags for ATOVS
           | 0-14-045   | Channel radiance

  3-10-009 | ATOVAMUA   ;     ; ATOVS AMSU-A report
           | 3-10-011 > | ATOVS field of view variables
           | 1-01-015 > | Replicate 1 descriptor 15 times
           | 3-10-012   | ATOVS channel variables

  3-10-010 | ATOVAMUB   ;     ; ATOVS AMSU-B report
           | 3-10-011 > | ATOVS field of view variables
           | 1-01-005 > | Replicate 1 descriptor 5 times
           | 3-10-012   | ATOVS channel variables

  3-10-011 | ATFOV      ;     ; ATOVS field of view variables
           | 0-08-070 > | TOVS/ATOVS product qualifier
           | 0-01-033 > | Identification of originating/generating centre
           | 0-01-034 > | Identification of originating/generating centre
           | 0-08-070 > | TOVS/ATOVS product qualifier
           | 0-01-033 > | Identification of originating/generating centre
           | 0-01-034 > | Identification of originating/generating centre
           | 0-01-007 > | Satellite identification
           | 0-02-048 > | Satellite sensor indicator
           | 0-05-040 > | Orbit number
           | 0-25-075 > | Satellite antenna corrections version number
           | 2-01-133 > | Change width
           | 0-05-041 > | Scan line number
           | 2-01-000 > | Change width
           | 0-05-043 > | Field of view number
           | 0-25-070 > | Major frame count
           | 0-33-030 > | Scan line status flags for ATOVS
           | 0-33-031 > | Scan line quality flags for ATOVS
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 2-02-131 > | Change scale
           | 2-01-138 > | Change width
           | 0-04-006 > | Second
           | 2-01-000 > | Change width
           | 2-02-000 > | Change scale
           | 0-05-001 > | Latitude
           | 0-06-001 > | Longitude
           | 2-02-126 > | Change scale
           | 0-07-001 > | Height of station
           | 2-02-000 > | Change scale
           | 0-07-024 > | Satellite zenith angle
           | 0-05-021 > | Satellite azimuth
           | 0-07-025 > | Solar zenith angle
           | 0-05-022 > | Solar azimuth
           | 0-33-033 > | Field of view quality flags for ATOVS
           | 0-02-151 > | Radiometer identifier
           | 0-12-064 > | Instrument temperature
           | 0-02-151 > | Radiometer identifier
           | 0-12-064 > | Instrument temperature
           | 0-02-151 > | Radiometer identifier
           | 0-12-064 > | Instrument temperature
           | 0-02-151 > | Radiometer identifier
           | 0-12-064   | Instrument temperature

  3-10-012 | ATCHV      ;     ; ATOVS channel variables
           | 0-02-150 > | TOVS/ATOVS/AVHRR instrumentation channel number
           | 0-25-076 > | Log-10 of (temperature-radiance central wavenumber) for ATOVS
           | 0-25-077 > | Bandwidth correction coefficient 1 for ATOVS
           | 0-25-078 > | Bandwidth correction coefficient 2 for ATOVS
           | 0-33-032 > | Channel quality flags for ATOVS
           | 2-01-132 > | Change width
           | 2-02-129 > | Change scale
           | 0-12-063 > | Brightness temperature
           | 2-02-000 > | Change scale
           | 2-01-000   | Change width

  3-10-013 | AVHRRGAC   ;     ; AVHRR GAC report
           | 0-01-007 > | Satellite ID
           | 0-05-040 > | Orbit number
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-04-006 > | Second
           | 0-05-001 > | Latitude
           | 0-06-001 > | Longitude
           | 0-07-025 > | Solar zenith angle
           | 0-05-043 > | Field of view number
           | 0-25-085 > | Fraction of clear pixels in HIRS field of view
           | 2-01-131 > | Change width
           | 2-02-129 > | Change scale
           | 0-02-150 > | TOVS/ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 0-02-150 > | TOVS/ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 0-02-150 > | ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 0-08-072 > | Pixel(s) type
           | 0-14-027 > | Albedo
           | 2-02-000 > | Change scale
           | 2-01-000 > | Change width
           | 2-01-132 > | Change width
           | 2-02-129 > | Change scale
           | 0-02-150 > | ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-02-150 > | ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-02-150 > | ATOVS/AVHRR instrumentation channel number
           | 0-08-023 > | First order statistics
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 0-08-072 > | Pixel(s) type
           | 0-12-063 > | Brightness temperature
           | 2-02-000 > | Change scale
           | 2-01-000   | Change width

  3-10-014 | GEOSTWND   ;     ; Satellite - geostationnary wind data
           | 3-01-072 > | Satellite identification, date, time, latitude, longitude
           | 3-03-041 > | Wind sequence
           | 3-04-011   | GOES-I/M information

  3-10-015 | METEORAD   ;     ; Meteosat radiace data
           | 3-01-072 > | Satellite identification
           | 0-07-024 > | Satellite zenith angle
           | 0-10-002 > | Height
           | 3-03-041 > | Wind sequence
           | 1-01-003 > | Replicate next descriptor 3 times
           | 3-04-032 > | Cloud fraction
           | 0-02-152 > | Satellite instrument used in data processing
           | 0-02-024 > | Integrated mean humidity computational method
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 1-01-003 > | Replicate next descriptor 3 times
           | 3-04-033   | Clear sky radiance

  3-10-016 | MSGRADAT   ;     ; Meteosat Second Generation MSG radiance data
           | 3-01-072 > | Satellite identification
           | 0-07-024 > | Satellite zenith angle
           | 0-10-002 > | Height
           | 3-03-041 > | Wind sequence
           | 1-01-012 > | Replicate next descriptor 12 times
           | 3-04-032 > | Cloud fraction
           | 0-02-152 > | Satellite instrument used in data processing
           | 0-02-024 > | Integrated mean humidity computational method
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 1-01-012 > | Replicate next descriptor 12 times
           | 3-04-033   | Clear sky radiance

  3-10-019 | SBUV2OZN   ;     ; Ozone data 
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instruments (= 624 - SBUV/2)
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-023 > | Lat/long (coarse accuracy)
           | 0-07-025 > | Solar zenith angle
           | 0-08-021 > | Time significance (= 28 - start of scan)
           | 0-07-025 > | Solar zenith angle
           | 0-08-021 > | Time significance (= 29 - end of scan)
           | 0-07-025 > | Solar zenith angle
           | 0-08-021 > | Time significance (= missing to cancel the previous value)
           | 0-08-029 > | Remotely-sensed surface type
           | 0-05-040 > | Orbit number
           | 0-08-075 > | Ascending/descending orbit qualifier
           | 0-08-003 > | Vertical significance (satellite observations) (= 0 - surface)
           | 0-10-004 > | Pressure (terrain)
           | 0-08-003 > | Vertical significance (satellite observations) (= missing to cancel the previous value)
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-15-001 > | Total ozone
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-33-070 > | SBUV total ozone quality
           | 0-15-030 > | Aerosol contamination index
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-20-081 > | Cloud amount in segment (cloud fraction)
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-08-003 > | Vertical significance (satellite observations) (= 2 - cloud top)
           | 0-33-042 > | Type of limit represented by following value (= 0 - exclusive lower limit)
           | 0-07-004 > | Pressure
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-15-001 > | Total ozone (below cloud top pressure)
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-08-003 > | Vertical significance (satellite observations) (= missing to cancel the previous value)
           | 1-13-021 > | Repeat next 13 descriptors 21 times
           | 0-07-004 > | Pressure (at bottom of layer)
           | 0-07-004 > | Pressure (at top of layer)
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-08-021 > | Time significance (= 27 - first guess)
           | 0-15-005 > | Ozone p
           | 0-08-021 > | Time significance (= missing to cancel the previous value)
           | 0-15-005 > | Ozone p
           | 0-33-007 > | Percent confidence
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-08-026 > | Matrix significance (= 4 - row of averaging kernel matrix)
           | 1-01-020 > | Repeat next descriptor 20 times
           | 0-25-143 > | Linear coefficient
           | 0-08-026 > | Matrix significance (= missing to cancel the previous value)
           | 0-08-043 > | Atmospheric chemical or physical constituent type (= 0 - ozone)
           | 1-09-015 > | Repeat next 9 descriptors 15 times
           | 0-07-004 > | Pressure
           | 0-08-090 > | Decimal scale of following Table B values
           | 2-07-006 > | Increase scale, reference value and bit width
           | 0-15-008 > | Scaled mixing ratio (volumetric)
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-08-090 > | Decimal scale applying to following Table B values (= missing to cancel the previous value)
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-33-007 > | Percent confidence
           | 2-07-000 > | Cancel increase scale, reference value and bit width
           | 0-08-043 > | Atmospheric chemical or physical constituent type (= missing to cancel the previous value)
           | 0-33-071 > | SBUV profile ozone quality
           | 1-08-008 > | Repeat next 6 descriptors 8 times
           | 2-02-124 > | Decrease scale by 4
           | 2-01-107 > | Decrease bit width by 21
           | 0-02-071 > | Spectrographic wavelength
           | 2-01-000 > | Cancel decrease bit width
           | 2-02-000 > | Cancel decrease scale
           | 2-07-002 > | Increase scale, reference value and bit width
           | 0-20-081 > | Cloud amount in segment (cloud fraction)
           | 2-07-000   | Cancel increase scale, reference value and bit width

  3-10-020 | RETROZON   ;     ; Retrieved ozone data
           | 3-10-022 > | Satellite, instrument and product
           | 3-01-011 > | Year, month, day
           | 3-01-013 > | Hour, minute, second
           | 3-01-021 > | Lat., long. (high accuracy)
           | 3-04-034 > | Latitude/longitude, solar elevation, number of layers
           | 3-10-021   | Ozone layers

  3-10-021 | PRLYIODH   ;     ;  
           | 1-08-000 > | Delayed replication of 8 next descriptors
           | 0-31-001 > | Delayed descriptor replication factor
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000 > | Change data width back to Table B
           | 0-15-020 > | Integrated ozone density
           | 0-10-002   | Height

  3-10-022 | SIIDSEQ    ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instrument used
           | 0-01-033 > | Identification of originating/generating centre
           | 0-02-172   | Product type for retrieved atmospheric gases

  3-10-023 | GSRADSEQ   ;     ; Geostationary multi-channel satellite radiance data
           | 3-01-072 > | Satellite identification
           | 0-30-021 > | Number of pixels per row
           | 0-30-022 > | Number of pixels per column
           | 0-08-012 > | Land/sea qualifier
           | 0-07-024 > | Satellite zenith angle
           | 0-07-025 > | Solar zenith angle
           | 0-10-002 > | Height
           | 1-01-012 > | Replicate next descriptor 12 times
           | 3-04-032 > | Cloud fraction
           | 1-05-002 > | Replicate next 5 descriptors 2 times
           | 0-02-152 > | Satellite instrument used in data processing
           | 0-02-024 > | Integrated mean humidity computational method
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 1-01-012 > | Replicate next descriptor 12 times
           | 3-04-033   | Radiance

  3-10-024 | GS3CHRAD   ;     ; Geostationary three-channel satellite radiance data
           | 3-01-072 > | Satellite identification
           | 0-30-021 > | Number of pixels per row
           | 0-30-022 > | Number of pixels per column
           | 0-08-012 > | Land/sea qualifier
           | 0-07-024 > | Satellite zenith angle
           | 0-07-025 > | Solar zenith angle
           | 0-10-002 > | Height
           | 1-01-003 > | Replicate next descriptor 3 times
           | 3-04-032 > | Cloud fraction
           | 1-05-002 > | Replicate next 5 descriptors 2 times
           | 0-02-152 > | Satellite instrument used in data processing
           | 0-02-024 > | Integrated mean humidity computational method
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 0-13-003 > | Relative humidity
           | 1-01-003 > | Replicate next descriptor 3 times
           | 3-04-033   | Radiance

  3-10-025 | SSMISTEM   ;     ; SSMIS Temperature data record
           | 0-01-007 > | Satellite id
           | 0-08-021 > | Scan start
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 2-01-138 > | Change bit width
           | 2-02-131 > | Change scale
           | 0-04-006 > | (Milli)seconds
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change bit width
           | 2-01-132 > | Change bit width
           | 0-05-041 > | Scan number
           | 2-01-000 > | Cancel change bit width
           | 2-01-129 > | Change bit width
           | 0-05-043 > | Scene number
           | 2-01-000 > | Cancel change bit width
           | 0-05-002 > | Latitude
           | 0-06-002 > | Longitude
           | 0-13-040 > | Surface flag
           | 0-20-029 > | Rain flag
           | 1-04-024 > | Repeat next 4 descriptors 24 times
           | 0-05-042 > | Channel number
           | 0-12-163 > | Temperature
           | 0-21-083 > | Warm target calibration
           | 0-21-084 > | Cold target calibration
           | 1-15-003 > | Replicate ephemeris data (15 descriptors) 3 times
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 2-01-142 > | Change data width
           | 2-02-131 > | Change scale
           | 0-04-026 > | Ephemeris (milli)seconds
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-05-001 > | Ephemeris latitude
           | 0-06-001 > | Ephemeris longitude
           | 2-01-138 > | Change data width
           | 2-02-129 > | Change scale
           | 0-07-001 > | Ephemeris height
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-08-021 > | Orbit start
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-05-040 > | Orbit number
           | 1-01-003 > | Repeat 3 times
           | 0-12-070 > | Warm load temperature
           | 0-25-054 > | SSMIS subframe id number
           | 1-01-004 > | Repeat 4 times
           | 0-25-055 > | Multiplexer housekeeping values
           | 0-08-007 > | Dimensional significance (line)
           | 1-04-028 > | Repeat 28 times next 4 descriptors
           | 0-05-002 > | Latitude
           | 0-06-002 > | Longitude
           | 0-02-111 > | Earth angle
           | 0-05-021   | Azimuth

  3-10-026 | RAOCSEQ    ;     ; Satellite radio occultation data
           | 3-10-022 > | Satellite, instrument and product
           | 0-25-060 > | Software identification
           | 0-08-021 > | Time significance ('17' = start of phenomenon)
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Hour, minute
           | 2-01-138 > | Change width to 16 bits
           | 2-02-131 > | Change scale to 3
           | 0-04-006 > | Second
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000 > | Change width back to Table B
           | 0-33-039 > | Quality flags for Radio Occultation data
           | 0-33-007 > | Per cent confidence (for whole message)
           | 3-04-030 > | Location of platform
           | 3-04-031 > | Speed of platform
           | 0-02-020 > | Satellite classification
           | 0-01-050 > | Platform transmitter ID number
           | 2-02-127 > | Change scale to 1
           | 3-04-030 > | Location of platform
           | 2-02-000 > | Change scale back to Table B
           | 3-04-031 > | Speed of platform
           | 2-01-133 > | Change width to 18 bits
           | 2-02-131 > | Change scale to 3
           | 0-04-016 > | Time increment
           | 2-02-000 > | Change scale back to Table B.
           | 2-01-000 > | Change width back to Table B
           | 3-01-021 > | Latitude, longitude (high accuracy)
           | 3-04-030 > | Location of point
           | 0-10-035 > | Earth's local radius of curvature
           | 0-05-021 > | Bearing or azimuth
           | 0-10-036 > | Geoid undulation
           | 1-13-000 > | Delayed replication of 13 descriptors
           | 0-31-002 > | Replication factor (16 bits)
           | 3-01-021 > | Latitude, longitude (high accuracy)
           | 0-05-021 > | Bearing or azimuth
           | 1-08-000 > | Delayed replication of 8 descriptors
           | 0-31-001 > | Replication factor
           | 0-02-121 > | Mean frequency
           | 0-07-040 > | Impact parameter
           | 0-15-037 > | Bending angle
           | 0-08-023 > | First-order statistics ('13' = r.m.s.)
           | 2-01-125 > | Change width to 20 bits
           | 0-15-037 > | Bending angle
           | 2-01-000 > | Change width back to Table B
           | 0-08-023 > | First-order statistics ('63' = missing)
           | 0-33-007 > | Per cent confidence (all data for current replication
           | 1-08-000 > | Delayed replication of 8 descriptors
           | 0-31-002 > | Replication factor (16 bits)
           | 0-07-007 > | Height
           | 0-15-036 > | Atmospheric refractivity
           | 0-08-023 > | First-order statistics ('13' = r.m.s.)
           | 2-01-123 > | Change width to 14 bits
           | 0-15-036 > | Atmospheric refractivity
           | 2-01-000 > | Change width back to Table B
           | 0-08-023 > | First-order statistics ('63' = missing)
           | 0-33-007 > | Per cent confidence (all data for current height)
           | 1-16-000 > | Delayed replication of 16 descriptors
           | 0-31-002 > | Replication factor (16 bits)
           | 0-07-009 > | Geopotential height
           | 0-10-004 > | Pressure
           | 0-12-001 > | Temperature
           | 0-13-001 > | Specific humidity
           | 0-08-023 > | First-order statistics ('13' = r.m.s.)
           | 2-01-120 > | Change width to 6 bits
           | 0-10-004 > | Pressure
           | 2-01-000 > | Change width back to Table B
           | 2-01-122 > | Change width to 6 bits
           | 0-12-001 > | Temperature
           | 2-01-000 > | Change width back to Table B
           | 2-01-123 > | Change width to 9 bits
           | 0-13-001 > | Specific humidity
           | 2-01-000 > | Change width back to Table B
           | 0-08-023 > | First-order statistics ('63' = missing)
           | 0-33-007 > | Per cent confidence (all data for current height)
           | 0-08-003 > | Vertical significance ('0' = surface)
           | 0-07-009 > | Geopotential height
           | 0-10-004 > | Pressure
           | 0-08-023 > | First-order statistics ('13' = r.m.s.)
           | 2-01-120 > | Change width to 6 bits
           | 0-10-004 > | Pressure
           | 2-01-000 > | Change width back to Table B
           | 0-08-023 > | First-order statistics ('63' = missing)
           | 0-33-007   | Per cent confidence (for surface data)

  3-10-029 | LYOZHTWV   ;     ; Layer, ozone, height, temperature and water vapour
           | 1-10-000 > | Delayed replication of 10 descriptors
           | 0-31-001 > | Delayed descriptor replication factor
           | 2-01-138 > | Change data width
           | 2-02-130 > | Change scale
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 2-02-000 > | Cancel change scale
           | 2-01-000 > | Cancel change data width
           | 0-15-020 > | Integrated ozone density
           | 0-10-002 > | Height
           | 0-12-101 > | Temperature
           | 0-13-098   | Integrated water vapour density

  3-10-030 | GOMOSINS   ;     ; MIPAS or GOMOS instruments reporting
           | 3-10-022 > | Satellite identification, product type
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 3-04-034 > | Latitude/longitude, solar elevation, number of layers
           | 3-10-029   | Layer, ozone, height, temperature and water vapour

  3-10-050 | SCO1C3IN   ;     ; Satellite collocated 1C reports with 3 instruments
           | 3-10-051 > | Satellite position and instrument temperatures
           | 3-10-052 > | Satellite instrument type and position (AIRS)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 3-10-053 > | Satellite channels and brightness temperatures with expanded channel set (AIRS)
           | 1-01-004 > | Replicate 1 descriptor 4 times
           | 3-10-054 > | Satellite visible channels and albedos with expanded channel set
           | 0-20-010 > | Cloud cover (total)
           | 3-10-052 > | Satellite instrument type and position (AMSU-A)
           | 1-01-015 > | Replicate 1 descriptor 15 times
           | 3-10-053 > | Satellite channels and brightness temperatures with expanded channel set (AMSU-A)
           | 3-10-052 > | Satellite instrument type and position (HSB)
           | 1-01-005 > | Replicate 1 descriptor 5 times
           | 3-10-053   | Satellite channels and brightness temperatures with expanded channel set (HSB)

  3-10-051 | SPITSEQN   ;     ; Satellite position and instrument temperatures
           | 0-01-007 > | Satellite identifier
           | 0-05-040 > | Orbit number
           | 2-01-133 > | Change data width
           | 0-05-041 > | Scan line number
           | 2-01-000 > | Cancel change data width
           | 2-01-132 > | Change data width
           | 0-25-070 > | Major frame count
           | 2-01-000 > | Cancel change data width
           | 2-02-126 > | Change scale
           | 0-07-001 > | Height of station
           | 2-02-000 > | Cancel change scale
           | 0-07-025 > | Solar zenith angle
           | 0-05-022 > | Solar azimuth
           | 1-02-009 > | Replicate 2 descriptors 9 times
           | 0-02-151 > | Radiometer identifier
           | 0-12-064   | Instrument temperature

  3-10-052 | SITPSEQN   ;     ; Satellite instrument type and position
           | 0-02-019 > | Satellite instruments
           | 3-01-011 > | Year, month, day
           | 3-01-012 > | Hour, minute
           | 2-02-131 > | Change scale
           | 2-01-138 > | Change data width
           | 0-04-006 > | Second
           | 2-01-000 > | Cancel change data width
           | 2-02-000 > | Cancel change scale
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-07-024 > | Satellite zenith angle
           | 0-05-021 > | Bearing or azimuth
           | 0-05-043   | Field of view number

  3-10-053 | SCBTSEQN   ;     ; Satellite channels and brightness temperatures with expanded channel set
           | 2-01-134 > | Change data width
           | 0-05-042 > | Channel number
           | 2-01-000 > | Cancel change data width
           | 0-25-076 > | Log-10 of temperature-radiance central wave number for ATOVS
           | 0-33-032 > | Channel quality flags for ATOVS
           | 0-12-163   | Brightness temperature (scale 2)

  3-10-054 | SVCASEQN   ;     ; Satellite visible channels and albedos with expanded channel set
           | 2-01-134 > | Change data width
           | 0-05-042 > | Channel number
           | 2-01-000 > | Cancel change data width
           | 0-25-076 > | Log-10 of temperature-radiance central wave number for ATOVS
           | 0-33-032 > | Channel quality flags for ATOVS
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 1-02-002 > | Replicate 2 descriptors 2 times
           | 0-08-023 > | First-order statistics
           | 0-14-027 > | Albedo
           | 0-08-023 > | First-order statistics
           | 2-02-000 > | Cancel change scale
           | 2-01-000   | Cancel change data width

  3-10-055 | SATRCPRC   ;     ; Satellite radiance/channel principle components
           | 3-10-051 > | Satellite position and instrument temperatures
           | 3-10-052 > | Satellite instrument type and position (AIRS)
           | 1-02-020 > | Replicate 2 descriptors 20 times
           | 0-25-076 > | Log-10 of temperature-radiance central wave number for ATOVS
           | 0-25-052 > | Log-10 of principal components normalized fit to data
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 0-25-050   | Principal components of satellite radiance

  3-11-001 | AIRCRAFT   ;     ; Aircraft reports
           | 3-01-051 > | ASDAR aircraft flight number, navigational system, date/time, position, phase of aircraft flight
           | 0-07-002 > | Altitude
           | 0-12-001 > | Temperature
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-11-031 > | Degree of turbulence
           | 0-11-032 > | Height of base of turbulence
           | 0-11-033 > | Height of top of turbulence
           | 0-20-041   | Airframe icing

  3-11-002 | ACARSREP   ;     ; ACARS reports
           | 3-01-065 > | ACARS identification
           | 3-01-066 > | ACARS location
           | 3-11-003 > | ACARS standard reported variables
           | 3-11-004   | ACARS supplementary reported variables

  3-11-003 | ACARSV     ;     ; ACARS standard reported variables
           | 0-10-070 > | Indicated aircraft altitude
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-12-001 > | Temperature/dry-bulb temperature
           | 0-13-002   | Mixing ratio

  3-11-004 | ACARSSRV   ;     ; ACARS supplementary reported variables
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-11-034 > | Vertical gust velocity
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-11-035 > | Vertical gust acceleration
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-11-075 > | Mean turbulence intensity (eddy dissipation rate)
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-11-076 > | Peak turbulence intensity (eddy dissipation rate)
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-33-025 > | ACARS interpolated values
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-000 > | Short delayed descriptor replication factor
           | 0-33-026   | Mixing ratio quality

  3-11-005 | AMDARSTD   ;     ; Standard AMDAR reports
           | 0-01-008 > | Aircraft identification
           | 0-01-023 > | Sequence number
           | 3-01-021 > | Latitude and longitude
           | 3-01-011 > | Year, month and day
           | 3-01-013 > | Hour, minute and second
           | 0-07-010 > | Flight level
           | 0-08-009 > | Detailed phase of flight
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-11-031 > | Degree of turbulence
           | 0-11-036 > | Derived equivalent vertical gust speed
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-33-025   | ACARS interpolated values

  3-11-006 | AMDARNOL   ;     ; AMDAR data or Aircraft data for one level without latitude/longitude
           | 0-07-010 > | Flight level
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-02-064 > | Roll angle quality
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-12-103   | Dew-point temperature

  3-11-007 | ACFTLALO   ;     ; Aircraft data for one level with latitude/longitude indicated
           | 0-07-010 > | Flight level
           | 3-01-021 > | Latitude, longitude
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-02-064 > | Roll angle quality
           | 0-12-101 > | Temperature/dry-bulb temperature
           | 0-12-103   | Dew-point temperature

  3-11-008 | ASDSNOLL   ;     ; Aircraft ascent/descent profile without latitude/longitude indicated at each level
           | 0-01-008 > | Aircraft identification
           | 3-01-011 > | Year, month, day
           | 3-01-013 > | Hour, Min, second
           | 3-01-021 > | Latitude, Longitude
           | 0-08-004 > | Phase of flight
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-11-006   | Aircraft data for one level without latitude/longitude

  3-11-009 | ASDSLALO   ;     ; Aircraft ascent/descent profile with latitude/longitude given for each level
           | 0-01-008 > | Aircraft identification
           | 3-01-011 > | Year, month, day
           | 3-01-013 > | Hour, Min, second
           | 3-01-021 > | Latitude, Longitude
           | 0-08-004 > | Phase of flight
           | 1-01-000 > | Delayed replication of one descriptor
           | 0-31-001 > | Delayed descriptor replication factor
           | 3-11-007   | Aircraft data for one level with latitude/longitude indicated

  3-12-001 | SAIDCPTW   ;     ;  
           | 3-01-043 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-001   | Cloud top pressure, temperature, wind

  3-12-002 | SAIDCPWN   ;     ;  
           | 3-01-043 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-002   | Cloud top pressure, wind

  3-12-003 | SAIDSFCT   ;     ;  
           | 3-01-042 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-003   | Surface temperature

  3-12-004 | SAIDCLDC   ;     ;  
           | 3-01-042 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-004   | Cloud cover

  3-12-005 | SAIDHOCT   ;     ;  
           | 3-01-042 > | Satellite identifier, instrumentation, location, date/time
           | 0-20-014   | Height of top of cloud

  3-12-006 | SAIDLMRH   ;     ;  
           | 3-01-044 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-005   | Layer mean relative humidity

  3-12-007 | SAIDRADN   ;     ;  
           | 3-01-042 > | Satellite identifier, instrumentation, location, date/time
           | 3-04-006   | Radiation

  3-12-010 | ORBITAL1   ;     ; Orbital information, Part I
           | 0-01-007 > | Satellite identifier
           | 0-05-040 > | Orbit number
           | 0-02-021 > | Satellite instrumentation
           | 0-05-041 > | Scan line number
           | 0-04-001 > | Year
           | 0-04-043   | Day of year

  3-12-011 | ORBITAL2   ;     ; Orbital information, Part II
           | 2-02-131 > | Change scale
           | 2-01-149 > | Change width
           | 0-04-006 > | Second
           | 2-01-000 > | Change width
           | 2-02-000 > | Change scale
           | 2-02-126 > | Change scale
           | 0-10-002 > | Height
           | 2-02-000 > | Change scale
           | 0-05-043 > | Field of view number
           | 0-05-053   | Field of view number increment

  3-12-012 | HIRSB119   ;     ; HIRS brightness temperatures - channels 1-19
           | 2-02-129 > | Change scale
           | 2-01-132 > | Change width
           | 1-01-019 > | Replicate 1 descriptor 19 times
           | 0-12-063 > | Brightness temperature
           | 2-01-000 > | Change width
           | 2-02-000   | Change scale

  3-12-013 | HIRSBT20   ;     ; HIRS brightness temperatures - channel 20
           | 0-05-042 > | Channel number
           | 2-02-129 > | Change scale
           | 2-01-135 > | Change width
           | 0-12-063 > | Brightness temperature
           | 2-01-000 > | Change width
           | 2-02-000   | Change scale

  3-12-014 | HIRSDATA   ;     ; HIRS satellite data
           | 3-12-010 > | Orbital information, Part I
           | 3-12-011 > | Orbital information, Part II
           | 1-05-056 > | Replicate 5 descriptors 56 times
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-05-042 > | Channel number
           | 0-05-052 > | Channel number increment
           | 3-12-012 > | HIRS brightness temperatures - channels 1-19
           | 3-12-013   | HIRS brightness temperature - channel 20

  3-12-015 | MSUB1234   ;     ; MSU brightness temperatures - channels 1-4
           | 1-09-011 > | Replicate 9 descriptors 11 times
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-05-042 > | Channel number
           | 0-05-052 > | Channel number increment
           | 2-02-129 > | Change scale
           | 2-01-132 > | Change width
           | 1-01-004 > | Replicate 1 descriptor 4 times
           | 0-12-063 > | Brightness temperature
           | 2-02-000 > | Change scale
           | 2-01-000   | Change width

  3-12-016 | MSUSDATA   ;     ; MSU satellite data
           | 3-12-010 > | Orbital information, Part I
           | 3-12-011 > | Orbital information, Part II
           | 3-12-015   | MSU brightness temperatures - channels 1-4

  3-12-017 | SSUBT123   ;     ; SSU brightness temperatures - channels 1-3
           | 1-09-008 > | Replicate 9 descriptors 8 times
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-05-042 > | Channel number
           | 0-05-052 > | Channel number increment
           | 2-02-129 > | Change scale
           | 2-01-132 > | Change width
           | 1-01-003 > | Replicate 1 descriptor 3 times
           | 0-12-063 > | Brightness temperature
           | 2-02-000 > | Change scale
           | 2-01-000   | Change width

  3-12-018 | SSUSDATA   ;     ; SSU satellite data
           | 3-12-010 > | Orbital information, Part I
           | 3-12-011 > | Orbital information, Part II
           | 3-12-017   | SSU brightness temperatures - channels 1-3

  3-12-019 | SCATWNML   ;     ; Wave scatterometer product with width change for wave number spectral
           | 3-01-047 > | Product header
           | 3-01-048 > | Radar parameters
           | 0-15-015 > | Maximum spectrum composition before normalisation
           | 0-29-002 > | Coordinate grid type
           | 0-21-076 > | Representation of intensities
           | 1-06-012 > | Repeat next 6 descriptors 12 times
           | 2-01-129 > | Change width to 14 bits
           | 0-06-030 > | Wave number (spectral)
           | 2-01-000 > | Change width back to Table B
           | 1-02-012 > | Repeat next 2 descriptors 12 times
           | 0-05-030 > | Direction (spectral)
           | 0-21-075 > | Image spectrum intensity
           | 0-21-066   | Wave scatterometer product confidence data

  3-12-020 | SCATPRD1   ;     ; Wave scatterometer product
           | 3-01-047 > | Product header
           | 3-01-048 > | Radar parameters
           | 0-15-015 > | Maximum spectrum composition before normalization
           | 0-29-002 > | Coordinate grid type
           | 0-21-076 > | Representation of intensities
           | 1-04-012 > | Repeat next 4 descriptors 12 times
           | 0-06-030 > | Wave number (spectral)
           | 1-02-012 > | Repeat next 2 descriptors 12 times
           | 0-05-030 > | Direction (spectral)
           | 0-21-075 > | Spectral intensity
           | 0-21-066   | Wave scatterometer product confidence data

  3-12-021 | SCATPRD2   ;     ; Wind scatterometer product
           | 3-01-047 > | Product header
           | 1-01-003 > | Repeat 1 descriptor 3 times
           | 3-01-049 > | Radar beam data
           | 0-11-012 > | Wind speed at 10 m
           | 0-11-011 > | Wind direction at 10 m
           | 0-21-067   | Wind product confidence data

  3-12-022 | RALTPROD   ;     ; Radar altimeter product
           | 3-01-047 > | Product header
           | 0-08-022 > | Number in average
           | 0-11-012 > | Wind speed
           | 0-11-050 > | Standard deviation of horizontal wind speed
           | 0-22-070 > | Significant wave height
           | 0-22-026 > | Standard deviation of significant wave height
           | 3-12-041 > | Altitude
           | 0-10-050 > | Standard deviation of altitude
           | 0-21-068 > | Radar altimeter product confidence data
           | 0-21-071 > | Peakiness
           | 0-21-072 > | Altimeter calibration status
           | 0-21-073 > | Altimeter instrument mode
           | 3-12-042 > | Altitude corrections
           | 0-21-062 > | Backscatter
           | 0-15-011   | Log 10 of integrated electron density

  3-12-023 | ATSRSSTP   ;     ; ATSR sea surface temperature product
           | 3-01-047 > | Product header
           | 1-03-003 > | Repeat 3 descriptors 3 times
           | 0-08-022 > | Number in average
           | 0-12-061 > | Skin temperature
           | 0-22-050 > | Standard deviation of sea surface temperature
           | 0-21-069 > | SST product confidence data
           | 0-21-085   | ATSR sea surface temperature across-track band number

  3-12-024 | SCATPRDE   ;     ; Wave scatterometer product enhanced
           | 3-12-020 > | (Wave scatterometer product)
           | 0-08-060 > | Sample scanning mode significance - range
           | 0-08-022 > | Number in sample
           | 0-08-060 > | Sample scanning mode signification - horizontal
           | 0-08-022 > | Number in sample
           | 0-25-014 > | Azimuth clutter cut-off
           | 0-22-101 > | Total energy (wavelength > 731 m)
           | 0-22-097 > | Mean wavelength of image spectrum
           | 0-22-098 > | Wavelength spread (wavelength > 731 m)
           | 0-22-099 > | Mean direction (wavelength > 731 m)
           | 0-22-100   | Direction spread (wavelength > 731 m)

  3-12-025 | SCATWNME   ;     ; Wave scatterometer enhanced product with change of width for wave number spectral
           | 3-12-019 > | Wave scatterometer product with width change for wave number (spectral)
           | 0-08-060 > | Sample scanning mode significance - range
           | 0-08-022 > | Number in sample
           | 0-08-060 > | Sample scanning mode signification - horizontal
           | 0-08-022 > | Number in sample
           | 0-25-014 > | Azimuth clutter cut-off
           | 0-22-101 > | Total energy (wavelength > 731 m)
           | 0-22-097 > | Mean wavelength of image spectrum
           | 0-22-098 > | Wavelength spread (wavelength > 731 m)
           | 0-22-099 > | Mean direction (wavelength > 731 m)
           | 0-22-100   | Direction spread (wavelength > 731 m)

  3-12-026 | QUIKSCAT   ;     ; QUIKSCAT data
           | 3-01-046 > | Satellite ID, motion, resolution and orbit number
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-023 > | Location
           | 3-12-031 > | Model wind data
           | 1-01-004 > | Replicate 1 descriptor 4 times
           | 3-12-030 > | Wind data
           | 0-21-110 > | Number of inner-beam sigma-0 (forward of satellite)
           | 3-01-023 > | Location
           | 3-21-027 > | Radar data
           | 0-21-111 > | Number of outer-beam sigma-0 (forward of satellite)
           | 3-01-023 > | Location
           | 3-21-027 > | Radar data
           | 0-21-112 > | Number of inner-beam sigma-0 (aft of satellite)
           | 3-01-023 > | Location
           | 3-21-027 > | Radar data
           | 0-21-113 > | Number of outer-beam sigma-0 (aft of satellite)
           | 3-01-023 > | Location
           | 3-21-027   | Radar data

  3-12-027 | SADIDTD2   ;     ; ATSR SST Product SADIST-2
           | 3-01-047 > | ERS product header
           | 1-05-009 > | Repeat next 5 descriptors 9 times
           | 3-01-023 > | Location (coarse Latitude + Longitude) of 10-arcmin cell
           | 0-07-021 > | Elevation: Incidence angle Nadir view [set to zero]
           | 0-12-061 > | Skin temperature: SST [Nadir-only view]
           | 0-07-021 > | Elevation: Incidence angle Dual view [set to 'missing']
           | 0-12-061 > | Skin temperature: SST [Dual view]
           | 0-21-085 > | ATSR SST across-track band number [0-9]
           | 0-21-070   | SST product confidence data (SADIST-2) [23-bit flag]

  3-12-028 | SWNDQKST   ;     ; SEAWINDS QUIKSCAT data
           | 3-01-046 > | Satellite ID, motion, resolution and orbit number
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-023 > | Location
           | 0-08-025 > | Time difference qualifier
           | 2-01-136 > | Change data width
           | 0-04-006 > | Second
           | 2-01-000 > | Change data width back to Table B
           | 3-12-031 > | Model wind data
           | 3-12-032 > | Rain data
           | 1-01-004 > | Next descriptor replicated 4 times
           | 3-12-030 > | Wind data
           | 1-01-002 > | Next descriptor replicated 2 times
           | 3-12-033 > | Brightness temperature data
           | 0-21-110 > | Number of inner-beam sigma-0 (forward of satellite)
           | 3-01-023 > | Location
           | 3-21-028 > | Radar data
           | 0-21-111 > | Number of outer-beam sigma-0 (forward of satellite)
           | 3-01-023 > | Location
           | 3-21-028 > | Radar data
           | 0-21-112 > | Number of inner-beam sigma-0 (aft of satellite)
           | 3-01-023 > | Location
           | 3-21-028 > | Radar data
           | 0-21-113 > | Number of outer-beam sigma-0 (aft of satellite)
           | 3-01-023 > | Location
           | 3-21-028   | Radar data

  3-12-030 | WNFRMUNL   ;     ;  
           | 2-01-130 > | Change data width
           | 2-02-129 > | Change scale
           | 0-11-012 > | Wind speed at 10 m
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000 > | Change data width back to Table B
           | 0-11-052 > | Formal uncertainty in wind speed
           | 2-01-135 > | Change data width
           | 2-02-130 > | Change scale
           | 0-11-011 > | Wind direction at 10 m
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000 > | Change data width back to Table B
           | 0-11-053 > | Formal uncertainty in wind direction
           | 0-21-104   | Likelihood computed for solution

  3-12-031 | ACQMWDAI   ;     ;  
           | 0-05-034 > | Along-track row number
           | 0-06-034 > | Cross-track cell number
           | 0-21-109 > | SEAWINDS wind vector cell quality
           | 0-11-081 > | Model wind direction at 10 m
           | 0-11-082 > | Model wind speed at 10 m
           | 0-21-101 > | Number of vector ambiguities
           | 0-21-102 > | Index of selected wind vector
           | 0-21-103   | Total number of sigma-0 measurements

  3-12-032 | SEAWPROR   ;     ;  
           | 0-21-120 > | Probability of rain
           | 0-21-121 > | SEAWINDS NOF rain index
           | 0-13-055 > | Intensity of precipitation
           | 0-21-122   | Attenuation correction on sigma-0 (from tB)

  3-12-033 | ANTPBTMP   ;     ;  
           | 0-02-104 > | Antenna polarisation
           | 0-08-022 > | Total number (with respect to accumulation)
           | 0-12-063 > | Brightness temperature
           | 0-12-065   | Standard deviation brightness temperature

  3-12-041 | ALTITUDE   ;     ; Altitude
           | 2-01-141 > | Change width to 28 bits
           | 2-02-130 > | Change scale to 2
           | 0-07-001 > | Altitude
           | 2-01-000 > | Change width back to Table B
           | 2-02-000   | Change scale back to Table B

  3-12-042 | ALTCORRN   ;     ; Altitude corrections
           | 0-21-077 > | Altitude correction, ionosphere
           | 0-21-078 > | Altitude correction, dry troposphere
           | 0-21-079 > | Altitude correction, wet troposphere
           | 0-21-080 > | Altitude correction, calibration constant
           | 0-21-081 > | Open loop height-time loop calibration correction
           | 0-21-082   | Open loop automatic gain control calibration correction

  3-12-045 | AATSRSST   ;     ; AATSR sea surface temperatures
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instruments
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification and version number
           | 0-05-040 > | Orbit number
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 0-07-002 > | Height or altitude
           | 0-12-180 > | Average 12 micron BT for all clear pixels at nadir
           | 0-12-181 > | Average 11 micron BT for all clear pixels at nadir
           | 0-12-182 > | Average 3.7 micron BT for all clear pixels at nadir
           | 0-12-183 > | Average 12 micron BT for all clear pixels, forward view
           | 0-12-184 > | Average 11 micron BT for all clear pixels, forward view
           | 0-12-185 > | Average 3.7 micron BT for all clear pixels, forward view
           | 0-02-174 > | Mean across track pixel number
           | 0-21-086 > | Number of pixels in nadir only, average
           | 0-12-186 > | Mean nadir sea surface temperature
           | 0-21-087 > | Number of pixels in dual view, average
           | 0-12-187 > | Mean dual view sea surface temperature
           | 0-33-043   | ATS confidence

  3-12-050 | MERISINS   ;     ; MERIS instrument reporting
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Instrument type
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification
           | 0-05-040 > | Orbit number
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 0-07-025 > | Solar zenith angle
           | 0-05-022 > | Solar azimuth
           | 0-10-080 > | Viewing zenith angle
           | 0-27-080 > | Viewing azimuth angle
           | 0-08-003 > | Vertical significance
           | 0-07-004 > | Pressure
           | 0-13-093 > | Cloud optical thickness
           | 0-08-003 > | Vertical significance
           | 2-01-131 > | Change data width
           | 2-02-129 > | Change scale
           | 0-07-004 > | Pressure
           | 0-07-004 > | Pressure
           | 2-02-000 > | Cancel operator
           | 2-01-000 > | Cancel operator
           | 0-13-095   | Total column water vapour

  3-12-051 | OCRSPWVS   ;     ; Ocean cross spectra - WVS
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instrument type
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification
           | 0-05-040 > | Orbit number
           | 0-08-075 > | Ascending/descending orbit qualifier
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 0-01-012 > | Direction of motion of moving observing platform
           | 2-01-131 > | Change data width
           | 0-01-013 > | Speed of motion of moving observing platform
           | 2-01-000 > | Cancel operator
           | 0-10-032 > | Satellite distance to Earth centre
           | 0-10-033 > | Altitude (platform to ellipsoid)
           | 0-10-034 > | Earth radius
           | 0-07-002 > | Height
           | 0-08-012 > | Land/sea qualifier
           | 0-25-110 > | Image processing summary
           | 0-25-111 > | Number of input data gaps
           | 0-25-102 > | Number of missing lines excluding data gaps
           | 0-02-104 > | Antenna polarisation
           | 0-25-103 > | Number of directional bins
           | 0-25-104 > | Number of wave-length bins
           | 0-25-105 > | First directional bin
           | 0-25-106 > | Directional bin step
           | 0-25-107 > | First wave-length bin
           | 0-25-108 > | Last wave-length bin
           | 0-02-111 > | Radar incidence angle
           | 0-02-121 > | Mean frequency
           | 0-02-026 > | Cross track resolution
           | 0-02-027 > | Along track resolution
           | 0-21-130 > | Spectrum total energy
           | 0-21-131 > | Spectrum maximum energy
           | 0-21-132 > | Direction of spectrum max on higher resolution grid
           | 0-21-133 > | Wavelength of spectrum max on higher resolution grid
           | 0-21-064 > | Clutter noise estimate
           | 0-25-014 > | Azimuth clutter cut-off
           | 0-21-134 > | Range resolution of cross covariance spectrum
           | 1-07-018 > | Replicate next 7 descriptors 18 times
           | 0-05-030 > | Direction (spectral)
           | 1-05-024 > | Replicate 5 descriptors 24 times
           | 2-01-130 > | Change data width
           | 0-06-030 > | Wave number (spectral)
           | 2-01-000 > | Cancel operator
           | 0-21-135 > | Real part of cross spectra
           | 0-21-136 > | Imaginary part of cross spectra
           | 0-33-044   | ASAR quality

  3-12-052 | RALTIMR2   ;     ; RA2- Radar Altimeter-2
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instrument type
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification
           | 0-05-040 > | Orbit number
           | 0-25-120 > | RA2 L2 processing flag
           | 0-25-121 > | RA2 L2 processing quality
           | 0-25-124 > | MWR L2 processing flag
           | 0-25-125 > | MWR L2 processing quality
           | 0-25-122 > | Hardware configuration for RF
           | 0-25-123 > | Hardware configuration for HPA
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 0-07-002 > | Height or altitude
           | 0-02-119 > | Instrument operations
           | 0-33-047 > | Measurement confidence data
           | 0-10-081 > | Altitude of COG above reference ellipsoid
           | 0-10-082 > | Instantaneous altitude rate
           | 0-10-083 > | Squared off nadir angle of the satellite from platform data
           | 0-10-084 > | Squared off nadir angle of the satellite from waveform data
           | 0-02-116 > | Percentage of 320 MHz band processed
           | 0-02-117 > | Percentage of 80 MHz band processed
           | 0-02-118 > | Percentage of 20 MHz band processed
           | 0-02-156 > | Percentage of valid Ku ocean retracker measurements
           | 0-02-157 > | Percentage of valid S ocean retracker measurements
           | 0-14-055 > | Solar activity index
           | 0-22-150 > | Number of 18 Hz valid points for Ku band
           | 0-22-151 > | Ku band ocean range
           | 0-22-152 > | STD of 18Hz Ku band ocean range
           | 0-22-153 > | Number of 18 Hz valid points for S band
           | 0-22-154 > | S band ocean range
           | 0-22-155 > | STD of 18 Hz S band ocean range
           | 0-22-156 > | Ku band significant wave height
           | 0-22-157 > | STD of 18 Hz Ku band significant wave height
           | 0-22-158 > | S band significant wave height
           | 0-22-159 > | STD 18 Hz S band significant wave height
           | 0-21-137 > | Ku band corrected ocean backscatter coefficient
           | 0-21-138 > | STD Ku band corrected ocean backscatter coefficient
           | 0-21-139 > | Ku band net instrumental correction for AGC
           | 0-21-140 > | S band corrected ocean backscatter coefficient
           | 0-21-141 > | STD S band corrected ocean backscatter coefficient
           | 0-21-142 > | S band net instrumental correction for AGC
           | 0-10-085 > | Mean sea surface height
           | 0-10-086 > | Geoid height
           | 0-10-087 > | Ocean depth/land elevation
           | 0-10-088 > | Total geocentric ocean tide height solution 1
           | 0-10-089 > | Total geocentric ocean tide height solution 2
           | 0-10-090 > | Long period tide height
           | 0-10-091 > | Tidal loading height
           | 0-10-092 > | Solid earth tide height
           | 0-10-093 > | Geocentric pole tide height
           | 0-11-002 > | Wind speed
           | 0-25-126 > | Model dry tropospheric correction
           | 0-25-127 > | Inverted barometer correction
           | 0-25-128 > | Model wet tropospheric correction
           | 0-25-129 > | MWR derived wet tropospheric correction
           | 0-25-130 > | RA2 ionospheric correction on Ku band
           | 0-25-131 > | Ionospheric correction from Doris on Ku band
           | 0-25-132 > | Ionospheric correction from model on Ku band
           | 0-25-133 > | Sea state bias correction on Ku band
           | 0-25-134 > | RA2 ionospheric correction on S band
           | 0-25-135 > | Ionospheric correction from Doris on S band
           | 0-25-136 > | Ionospheric correction from model on S band
           | 0-25-137 > | Sea state bias correction on S band
           | 0-13-096 > | MWR water vapour content
           | 0-13-097 > | MWR liquid water content
           | 0-11-095 > | U component of model wind vector
           | 0-11-096 > | V component of model wind vector
           | 0-12-188 > | Interpolated 23.8 GHz brightness temperature from MWR
           | 0-12-189 > | Interpolated 36.5 GHz brightness temperature from MWR
           | 0-02-158 > | RA2 instrument
           | 0-02-159 > | MWR instrument
           | 0-33-052 > | S band ocean retracking quality
           | 0-33-053 > | Ku band ocean retracking quality
           | 0-21-143 > | Ku band rain attenuation
           | 0-21-144   | Altimeter rain flag

  3-12-053 | OCWAVESP   ;     ; Ocean wave spectra
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instrument type
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification and version number
           | 0-05-040 > | Orbit number
           | 0-08-075 > | Ascending/descending orbit qualifier
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude/longitude
           | 0-01-012 > | Direction of motion of moving observing platform
           | 2-01-131 > | Change data width
           | 0-01-013 > | Speed of motion of moving observing platform
           | 2-01-000 > | Cancel operator
           | 0-10-032 > | Satellite distance to Earth centre
           | 0-10-033 > | Altitude (platform to ellipsoid)
           | 0-10-034 > | Earth radius
           | 0-07-002 > | Height or altitude
           | 0-08-012 > | Land/sea qualifier
           | 0-25-110 > | Image processing summary
           | 0-25-111 > | Number of input data gaps
           | 0-25-102 > | Number of missing lines excluding data gaps
           | 0-02-104 > | Antenna polarisation
           | 0-25-103 > | Number of directional bins
           | 0-25-104 > | Number of wave-length bins
           | 0-25-105 > | First directional bin
           | 0-25-106 > | Directional bin step
           | 0-25-107 > | First wave-length bin
           | 0-25-108 > | Last wave-length bin
           | 0-11-001 > | Wind direction
           | 0-11-002 > | Wind speed
           | 0-22-160 > | Normalized inverse wave age
           | 0-25-138 > | Average signal to noise ratio
           | 2-01-130 > | Change data width
           | 2-02-129 > | Change scale
           | 0-22-021 > | Height of waves
           | 2-02-000 > | Cancel operator
           | 2-01-000 > | Cancel operator
           | 0-33-048 > | Confidence measure for SAR inversion
           | 0-33-049 > | Confidence measure for wind retrieval
           | 0-02-026 > | Cross track resolution
           | 0-02-027 > | Along track resolution
           | 0-21-130 > | Spectrum total energy
           | 0-21-131 > | Spectrum max energy
           | 0-21-132 > | Direction of spectrum max
           | 0-21-133 > | Wave-length of spectrum max
           | 0-25-014 > | Azimuth clutter cut-off
           | 1-06-036 > | Replicate 6 descriptors 36 times
           | 0-05-030 > | Direction (spectral)
           | 1-04-024 > | Replicate 4 descriptors 24 times
           | 2-01-130 > | Change data width
           | 0-06-030 > | Wave number (spectral)
           | 2-01-000 > | Cancel operator
           | 0-22-161 > | Wave spectra
           | 0-33-044   | ASAR quality

  3-12-055 | ASCAT1BC   ;     ; ASCAT level 1b cell information
           | 0-05-033 > | Pixel size on horizontal-1
           | 0-05-040 > | Orbit number
           | 0-06-034 > | Cross track cell number
           | 0-10-095 > | Height of atmosphere used
           | 0-21-157   | Loss per unit length of atmosphere used

  3-12-056 | SCATWNDC   ;     ; Scatterometer wind cell information
           | 0-25-060 > | Software identification
           | 0-01-032 > | Generating application
           | 0-11-082 > | Model wind speed at 10 m
           | 0-11-081 > | Model wind direction at 10 m
           | 0-20-095 > | Ice probability
           | 0-20-096 > | Ice age (a-parameter)
           | 0-21-155 > | Wind vector cell quality
           | 2-01-133 > | Increase data width by 5 bits
           | 0-21-101 > | Number of vector ambiguities
           | 0-21-102 > | Index of selected wind vector
           | 2-01-000   | Cancel change data width

  3-12-057 | AMBIGWND   ;     ; Ambiguous wind data
           | 2-01-130 > | Increase data width by 2 bits
           | 2-02-129 > | Increase scaling by 101
           | 0-11-012 > | Wind speed at 10 m
           | 2-02-000 > | Cancel change scaling
           | 2-01-000 > | Cancel change data width
           | 2-01-131 > | Increase data width by 3 bits
           | 2-02-129 > | Increase scaling by 101
           | 0-11-011 > | Wind direction at 10 m
           | 2-02-000 > | Cancel change scaling
           | 2-01-000 > | Cancel change data width
           | 0-21-156 > | Backscatter distance
           | 0-21-104   | Likelihood computed for solution

  3-12-058 | ASCAT1BD   ;     ; ASCAT level 1b data
           | 3-01-125 > | ASCAT header information
           | 3-01-011 > | Date information
           | 3-01-013 > | Time information
           | 3-01-021 > | Position information
           | 3-12-055 > | ASCAT level 1b cell information
           | 0-21-150 > | Beam co-location
           | 1-01-003 > | Repeat next 1 descriptor 3 times
           | 3-21-030   | ASCAT sigma-0 information

  3-12-059 | SCATWNDD   ;     ; Scatterometer wind data
           | 3-12-056 > | Scatterometer wind cell information
           | 1-01-000 > | Delayed replication of next 1 descriptor
           | 0-31-001 > | Delayed replication factor
           | 3-12-057   | Ambiguous wind data

  3-12-060 | SCATSMST   ;     ; Scatterometer soil moisture data
           | 0-25-060 > | Software identification
           | 0-25-062 > | Database identification
           | 0-40-001 > | Surface soil moisture (ms)
           | 0-40-002 > | Estimated error in surface soil moisture
           | 0-21-062 > | Extrapolated backscatter at 40deg incidence angle (sigma0_40)
           | 0-21-151 > | Estimated error in sigma0 at 40deg incidence angle
           | 0-21-152 > | Slope at 40deg incidence angle
           | 0-21-153 > | Estimated error in slope at 40deg incidence angle
           | 0-21-154 > | Soil moisture sensitivity
           | 0-21-062 > | Dry backscatter
           | 0-21-088 > | Wet backscatter
           | 0-40-003 > | Mean surface soil moisture
           | 0-40-004 > | Rain fall detection
           | 0-40-005 > | Soil moisture correction flag
           | 0-40-006 > | Soil moisture processing flag
           | 0-40-007 > | Soil moisture quality
           | 0-20-065 > | Snow cover
           | 0-40-008 > | Frozen land surface fraction
           | 0-40-009 > | Inundation and wetland fraction
           | 0-40-010   | Topographic complexity

  3-12-061 | ASCAT1B2   ;     ; ASCAT Level 1b and level 2 data
           | 3-12-058 > | ASCAT level 1b data
           | 3-12-060 > | Scatterometer soil moisture data
           | 3-12-059   | Scatterometer wind data

  3-12-070 | SMOSDATA   ;     ; SMOS data
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instruments
           | 0-01-144 > | Snapshot identifier
           | 0-01-124 > | Gridpoint identifier
           | 0-30-010 > | Number of grid points
           | 3-01-011 > | Date
           | 3-01-013 > | Time
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-07-012 > | Gridpoint altitude
           | 0-15-012 > | Total electron count per square meter
           | 0-12-165 > | Direct sun brightness temperature
           | 0-12-166 > | Snapshot accuracy
           | 0-12-167 > | Radiometric accuracy (pure polarisation)
           | 0-12-168 > | Radiometric accuracy (cross polarisation)
           | 0-27-010 > | Footprint axis 1
           | 0-28-010 > | Footprint axis 2
           | 0-02-099 > | Polarization
           | 0-13-048 > | Water fraction
           | 0-25-081 > | Incidence angle
           | 0-25-082 > | Azimuth angle
           | 0-25-083 > | Faraday rotational angle
           | 0-25-084 > | Geometric rotational angle
           | 0-12-080 > | Brightness temperature real part
           | 0-12-081 > | Brightness temperature imaginary part
           | 0-12-082 > | Pixel radiometric accuracy
           | 0-25-174 > | SMOS information flag
           | 0-33-028   | Snapshot overall quality

  3-13-009 | RADARREF   ;     ; Radar reflectivity values
           | 0-21-001 > | Horizontal reflectivity
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 0-21-001   | Horizontal reflectivity

  3-13-010 | RADARAIN   ;     ; Radar rainfall intensities
           | 0-21-036 > | Radar rainfall intensity
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 0-21-036   | Radar rainfall intensity

  3-13-031 | NRLERPXV   ;     ; Non run-length encoded row for Pixel value 4 bits
           | 0-06-002 > | First longitude location minus one increment
           | 0-06-012 > | Longitude increment
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended replication factor
           | 0-30-001   | Pixel value (4 bits)

  3-13-032 | NRLEPPXV   ;     ; Non run-length encoded picture data for Pixel value 4 bits
           | 0-05-002 > | First latitude location minus one increment
           | 0-05-012 > | Latitude increment (signed value so cannot cross pole)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended replication factor
           | 3-13-031   | Non run-length encoded row

  3-13-041 | RLGERPXV   ;     ; Run-length encoded row for Pixel value 4 bits
           | 0-06-002 > | First longitude location minus one increment
           | 1-10-000 > | Delayed replication of 10 descriptors
           | 0-31-001 > | Replication factor
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Replication factor
           | 0-06-012 > | Longitude increment
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-012 > | Repetition factor
           | 0-30-001 > | Pixel value (4 bits)
           | 0-06-012 > | Longitude increment
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 0-30-001   | Pixel value (4 bits)

  3-13-042 | RLGEPPXV   ;     ; Run-length encoded picture data for Pixel value 4 bits
           | 0-05-002 > | First latitude location minus one increment
           | 0-05-012 > | Latitude increment (signed value so cannot cross pole)
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-002 > | Extended replication factor
           | 3-13-041   | Run-length encoded row

  3-13-043 | RLGEPPXR   ;     ; Run-length encoded picture data for Pixel value 4 bits, regular grid
           | 0-06-002 > | First longitude location minus one increment
           | 0-05-002 > | First latitude location minus one increment
           | 0-05-012 > | Latitude increment
           | 1-12-000 > | Delayed replication of 12 descriptors
           | 0-31-001 > | Replication factor
           | 1-10-000 > | Delayed replication of 10 descriptors
           | 0-31-001 > | Replication factor
           | 1-04-000 > | Delayed replication of 4 descriptors
           | 0-31-001 > | Replication factor
           | 0-06-012 > | Longitude increment
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-011 > | Repetition factor
           | 0-30-001 > | Pixel value (4 bits)
           | 0-06-012 > | Longitude increment
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 0-30-001   | Pixel value (4 bits)

  3-15-001 | TUSWODTM   ;     ; Typically reported underwater sounding without optional fields
           | 0-01-011 > | Ship's call sign
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 3-06-001   | Depth, temperature

  3-15-002 | TUSWODTS   ;     ; Typically reported underwater sounding without optional fields
           | 0-01-011 > | Ship's call sign
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 3-06-004   | Depth, temperature, salinity

  3-15-003 | TEMSALFL   ;     ; Temperature and salinity profile observed by profile floats
           | 0-01-087 > | WMO Marine observing platform extended identifier
           | 0-01-085 > | Observing platform manufacturers model
           | 0-01-086 > | Observing platform manufacturers serial number
           | 0-02-036 > | Buoy type
           | 0-02-148 > | Data collection and/or location system
           | 0-02-149 > | Type of data buoy
           | 0-22-055 > | Float cycle number
           | 0-22-056 > | Direction of profile
           | 0-22-067 > | Instrument type for water temperature profile measurement
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 3-01-021 > | Latitude and longitude (high accuracy)
           | 0-08-080 > | Qualifier for quality class
           | 0-33-050 > | GTSPP quality class
           | 1-09-000 > | Delayed replication of 9 descriptors
           | 0-31-002 > | Extended delayed descriptor replication factor
           | 0-07-065 > | Water pressure
           | 0-08-080 > | Qualifier for quality class
           | 0-33-050 > | GTSPP quality class
           | 0-22-045 > | Subsurface sea temperature
           | 0-08-080 > | Qualifier for quality class
           | 0-33-050 > | GTSPP quality class
           | 0-22-064 > | Salinity
           | 0-08-080 > | Qualifier for quality class
           | 0-33-050   | GTSPP quality class

  3-16-001 | DLIMTPRT   ;     ;  
           | 3-01-011 > | Year, month, day
           | 0-04-004 > | Hour
           | 3-01-023 > | Latitude and longitude (coarse accuracy)
           | 0-01-021 > | Synoptic feature identifier
           | 0-02-041 > | Method for estimating reports related to synoptic features
           | 0-19-001 > | Type of synoptic feature
           | 0-10-051 > | Pressure reduced to mean sea level
           | 0-19-002 > | Effective radius of feature
           | 0-19-003 > | Wind speed threshold (15 m s-1 typically)
           | 0-19-004   | Effective radius with respect to wind speeds above threshold

  3-16-002 | HEADRSEQ   ;     ; Header
           | 0-08-021 > | Data time (analysis)
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-01-033 > | Originating/generating centre
           | 0-08-021 > | Validity time (fcst)
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-07-002 > | Flight level (altitude) (base of chart layer)
           | 0-07-002   | Flight level (altitude) (top of chart layer)

  3-16-003 | JTSTREAM   ;     ; Jet stream
           | 1-10-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (jet stream value)
           | 0-08-007 > | Dimensional significance (value for line)
           | 1-04-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-10-002 > | Flight level (altitude)
           | 0-11-002 > | Wind speed
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-004 | TURBLNCE   ;     ; Turbulence
           | 1-11-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (value for turbulence)
           | 0-08-007 > | Dimensional significance (value for area)
           | 0-07-002 > | Flight level (altitude) (base of layer)
           | 0-07-002 > | Flight level (altitude) (top of layer)
           | 1-02-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-11-031 > | Degree of turbulence
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-005 | STORMSEQ   ;     ; Storm
           | 1-08-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-005 > | Meteorological attribute significance (storm centre)
           | 0-08-007 > | Dimensional significance (value for point)
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-01-026 > | WMO storm name (use "UNKNOWN" for a sandstorm)
           | 0-19-001 > | Synoptic features (value for type of storm)
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-005   | Meteorological attribute significance (cancel/end of object)

  3-16-006 | CLOUDSQ2   ;     ; Cloud
           | 1-12-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (value for cloud)
           | 0-08-007 > | Dimensional significance (value for area)
           | 0-07-002 > | Flight level (altitude) (base of layer)
           | 0-07-002 > | Flight level (altitude) (top of layer)
           | 1-02-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-20-011 > | Cloud amount
           | 0-20-012 > | Cloud type
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-007 | FRONTSEQ   ;     ; Front
           | 1-10-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (value for type of front)
           | 0-08-007 > | Dimensional significance (value for line)
           | 1-04-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-19-005 > | Direction of feature
           | 0-19-006 > | Speed of feature
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-008 | TROPAUSE   ;     ; Tropopause
           | 1-11-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-001 > | Vertical significance (bit 3 set for tropopause)
           | 0-08-007 > | Dimensional significance (value for point)
           | 0-08-023 > | Statistic (type of tropopause value)
           | 1-03-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-10-002 > | Height/altitude
           | 0-08-023 > | Statistic (cancel)
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-001   | Vertical significance (cancel/end of object)

  3-16-009 | AFRMICEA   ;     ; Airframe icing area
           | 1-11-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (value for airframe icing)
           | 0-08-007 > | Dimensional significance (value for area)
           | 0-07-002 > | Flight level (altitude) (base of layer)
           | 0-07-002 > | Flight level (altitude) (top of layer)
           | 1-02-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-20-041 > | Airframe icing (type of airframe icing)
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-010 | NAMEFEAT   ;     ; Name of feature
           | 1-07-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature
           | 0-08-007 > | Dimensional significance (value for point)
           | 0-01-022 > | Name of feature
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-011 | VCNOERPT   ;     ; Volcano erupting
           | 1-17-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-08-011 > | Meteorological feature (value for special clouds)
           | 0-01-022 > | Name of feature (volcano name)
           | 0-08-007 > | Dimensional significance (value for point)
           | 1-02-000 > | Delayed replication
           | 0-31-001 > | Replication
           | 0-05-002 > | Latitude (coarse)
           | 0-06-002 > | Longitude (coarse)
           | 0-08-021 > | Time significance (eruption starting time)
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-20-090 > | Special clouds (clouds from volcanic eruptions)
           | 0-08-021 > | Time significance (cancel)
           | 0-08-007 > | Dimensional significance (cancel)
           | 0-08-011   | Meteorological feature (cancel/end of object)

  3-16-022 | FORECAST   ;     ; Forecast data
           | 0-01-032 > | Generating application (NWP model name, etc. code table defined by originating/generating centre)
           | 0-02-041 > | Method for estimating reports related to synoptic feature
           | 0-19-001 > | Type of synoptic feature
           | 0-19-010 > | Method for tracing of the centre of synoptic feature
           | 1-18-000 > | Delayed replication of 18 descriptors
           | 0-31-001 > | Replication factor
           | 0-08-021 > | Time significance (forecast)
           | 0-04-014 > | Time increment (hour)
           | 0-08-005 > | Surface synoptic feature significance
           | 3-01-023 > | Latitude (coarse accuracy), longitude (coarse accuracy)
           | 0-19-005 > | Direction of motion of feature
           | 0-19-006 > | Speed of motion of feature
           | 0-10-004 > | Pressure
           | 0-11-041 > | Maximum wind speed (gust: e.g. used in US)
           | 0-08-021 > | Time significance (forecast time averaged)
           | 0-04-075 > | Time period (minutes)
           | 0-11-040 > | Maximum wind speed (mean wind)
           | 0-19-008 > | Vertical extent of feature
           | 1-05-004 > | Replicate 5 descriptors 4 times
           | 0-05-021 > | Starting bearing or azimuth
           | 0-05-021 > | Ending bearing or azimuth
           | 1-02-002 > | Replicate 2 descriptors 2 times
           | 0-19-003 > | Wind speed threshold
           | 0-19-004   | Effective radius with respect to wind speed above threshold

  3-16-030 | SIGMETHD   ;     ; SIGMET header
           | 3-01-014 > | Time period (for which SIGMET is valid)
           | 0-01-037 > | SIGMET sequence identifier
           | 0-10-064 > | SIGMET cruising level
           | 0-08-019 > | Qualifier for location identifier, 1=ATS unit serving FIR
           | 0-01-062 > | Short ICAO location identifier
           | 0-08-019 > | Qualifier for location identifier, 2=FIR, 3=UIR, 4=CTA
           | 0-01-065 > | ICAO region identifier
           | 0-08-019 > | Qualifier for location identifier, 6=MWO
           | 0-01-062 > | Short ICAO location identifier
           | 0-08-019   | Qualifier for location identifier, Missing=Cancel

  3-16-031 | SIGMETOF   ;     ; SIGMET, Observed or forecast location and motion
           | 0-08-021 > | Time Significance, 16=Analysis, 4=Forecast
           | 3-01-011 > | Year, Month, Day
           | 3-01-012 > | Hour, Minute
           | 3-01-027 > | Description of feature
           | 0-19-005 > | Direction of motion
           | 0-19-006 > | Speed of motion
           | 0-20-028 > | Expected change in intensity
           | 0-08-021   | Time significance, Missing=Cancel

  3-16-032 | SIGMETFC   ;     ; SIGMET, Forecast position
           | 0-08-021 > | Time Significance, 4=Forecast
           | 3-01-011 > | Year, Month, Day
           | 3-01-012 > | Hour, Minute
           | 3-01-027 > | Description of feature
           | 0-08-021   | Time significance, Missing=Cancel

  3-16-033 | SIGMETOU   ;     ; SIGMET, Outlook
           | 0-08-021 > | Time Significance, 4=Forecast
           | 3-01-011 > | Year, Month, Day
           | 3-01-012 > | Hour, Minute
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-01-027 > | Description of feature
           | 0-08-021   | Time significance, Missing=Cancel

  3-16-034 | SIGMETVA   ;     ; Volcanic Ash SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 17=Volcano
           | 0-01-022 > | Name of feature
           | 0-08-007 > | Dimensional significance, 0=Point
           | 3-01-023 > | Location
           | 0-08-007 > | Dimensional significance, Missing=Cancel
           | 0-20-090 > | Special Clouds, 5=Clouds from volcanic eruptions
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-000 > | Short replication factor
           | 3-16-032 > | SIGMET Forecast position
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-16-033 > | SIGMET Outlook
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-035 | SIGMETTH   ;     ; Thunderstorm SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 21=Thunderstorm
           | 0-20-023 > | Other weather phenomenon, bit 2=Squalls or all 18 bits = Missing
           | 0-20-021 > | Type of precipitation, bit 14=Hail or all 30 bits=Missing
           | 0-20-008 > | Cloud distribution 15=OBSC, 16=EMBD, 12=FRQ, 31=Missing
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-036 | SIGMETTC   ;     ; Tropical Cyclone SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 22=Tropical Cyclone
           | 0-01-027 > | WMO long storm name
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-000 > | Short replication factor
           | 3-16-032 > | SIGMET Forecast position
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-16-033 > | SIGMET Outlook
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-037 | SIGMETTU   ;     ; Turbulence SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 13=Turbulence
           | 0-11-031 > | Degree of turbulence, 10=Moderate, 11=Severe
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-038 | SIGMETIC   ;     ; Icing SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 15=Airframe Icing
           | 0-20-041 > | Airframe icing, 7=Severe
           | 0-20-021 > | Type of precipitation, bit 3=Liquid freezing or all 30 bits = Missing
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-039 | SIGMETMT   ;     ; Mountain Wave, Duststorm or Sandstorm SIGMET
           | 0-08-079 > | Product status, 0=Normal Issue, 1=Correction
           | 3-16-030 > | SIGMET Header
           | 0-08-011 > | Meteorological feature, 23=MountainWave, 24=Duststorm, 25=Sandstorm
           | 0-20-024 > | Intensity of phenomena, 3=Heavy, 5=Severe
           | 3-16-031 > | SIGMET Observed or forecast location and motion
           | 0-08-011 > | Meteorological feature, Missing=Cancel
           | 0-08-079   | Product status, Missing=Cancel

  3-16-040 | SIGMETCA   ;     ; Cancellation of SIGMET
           | 3-16-030 > | SIGMET header
           | 0-08-079 > | Product status, 4=Cancellation
           | 3-01-014 > | Time period (of the SIGMET to be cancelled)
           | 0-01-037 > | SIGMET sequence identifier (of the SIGMET to be cancelled)
           | 0-10-064 > | SIGMET cruising level (of the SIGMET to be cancelled)
           | 0-08-079   | Product status, Missing=Cancel

  3-16-050 | RADOBPTA   ;     ; RADOB Template (part A: Information on tropical cyclone)
           | 3-01-001 > | WMO block and station number
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 0-02-160 > | Wave length of the radar
           | 0-08-005 > | Meteorological attribute significance (=1)
           | 0-05-002 > | Latitude (coarse accuracy)
           | 0-06-002 > | Longitude (coarse accuracy)
           | 0-08-005 > | Cancel Meteorological attribute significance
           | 0-19-100 > | Time interval to calculate the movement of the tropical cyclone
           | 0-19-005 > | Direction of motion of feature
           | 0-19-006 > | Speed of motion of feature
           | 0-19-101 > | Accuracy of the position of the centre of the tropical cyclone
           | 0-19-102 > | Shape and definition of the eye of the tropical cyclone
           | 0-19-103 > | Diameter of major axis of the eye of the tropical cyclone
           | 0-19-104 > | Change in character of the eye during the 30 minutes
           | 0-19-105   | Distance between the end of spiral band and the centre

  3-16-052 | SAREPPTA   ;     ; SAREP Template (part A: Information on tropical cyclone)
           | 3-01-005 > | Originating centre/sub-centre
           | 3-01-011 > | Date
           | 3-01-012 > | Time
           | 0-01-007 > | Satellite identifier
           | 0-25-150 > | Method of tropical cyclone intensity analysis using satellite data
           | 1-22-000 > | Delayed replication of 22 descriptors
           | 0-31-001 > | Delayed descriptor replication facto
           | 0-01-027 > | WMO long storm name
           | 0-19-150 > | Typhoon International Common Number (Typhoon Committee)
           | 0-19-106 > | Identification number of tropical cyclone
           | 0-08-005 > | Meteorological attribute significance (=1)
           | 0-05-002 > | Latitude (coarse accuracy)
           | 0-06-002 > | Longitude (coarse accuracy)
           | 0-08-005 > | Cancel Meteorological attribute significance
           | 0-19-107 > | Time interval of the tropical cyclone analysis
           | 0-19-005 > | Direction of motion of feature
           | 0-19-006 > | Speed of motion of feature
           | 0-19-108 > | Accuracy of geographical position of the tropical cyclone
           | 0-19-109 > | Mean diameter of the overcast cloud of the tropical cyclone
           | 0-19-110 > | Apparent 24-hour change in intensity of the tropical cyclone
           | 0-19-111 > | Current Intensity (CI) number of the tropical cyclone
           | 0-19-112 > | Data tropical (DT) number of the tropical cyclone
           | 0-19-113 > | Cloud pattern type of the DT-number
           | 0-19-114 > | Model Expected tropical (MET) number of the tropical cyclone
           | 0-19-115 > | Trend of the past 24-hour change (+: Developed, -: Weakened)
           | 0-19-116 > | Pattern tropical (PT) number of the tropical cyclone
           | 0-19-117 > | Cloud picture type of the PT-number
           | 0-19-118 > | Final tropical (T) number of the tropical cyclone
           | 0-19-119   | Type of the final T-number

  3-18-001 | LALODOSE   ;     ;  
           | 3-01-025 > | Latitude and longitude (coarse accuracy), day and time
           | 0-24-011   | Dose

  3-18-003 | LALOTPER   ;     ;  
           | 3-01-026 > | Latitude and longitude (high accuracy), time periods in days, hours and minutes
           | 0-24-005 > | Isotope mass
           | 0-24-004 > | Element name
           | 0-24-021   | Air concentration

  3-18-004 | LALODISP   ;     ; Air concentration
           | 3-01-025 > | Latitude and longitude (coarse accuracy), day and time
           | 0-04-023 > | Time period or displacement
           | 0-13-011 > | Total precipitation/total water equivalent
           | 0-24-005 > | Isotope mass
           | 0-24-004 > | Element name
           | 0-24-022   | Concentration in precipitation

  3-21-001 | WNPROFAN   ;     ; Wind profiler - antenna characteristics
           | 0-02-101 > | Type of antenna
           | 0-02-114 > | Antenna effective surface area
           | 0-02-105 > | Maximum antenna gain
           | 0-02-106 > | 3-dB beamwidth
           | 0-02-107 > | Sidelobe suppression
           | 0-02-121   | Mean frequency

  3-21-003 | WNPROFMD   ;     ; Wind profiler - moment data
           | 0-21-051 > | Signal power above 1 mW
           | 0-21-014 > | Doppler mean velocity (radial)
           | 0-21-017 > | Doppler velocity spectral width
           | 0-21-030   | Signal to noise ratio

  3-21-004 | WNPROFMS   ;     ; Wind profiler - moment data sounding
           | 3-01-031 > | Identification, type, date/time, position (high accuracy), height
           | 0-02-003 > | Type of measuring equipment used
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 3-21-003   | Wind profiler - moment data

  3-21-005 | TRANRECV   ;     ; Transmitter-receiver characteristics
           | 0-25-004 > | Echo processing
           | 0-02-121 > | Mean frequency
           | 0-02-122 > | Frequency agility range
           | 0-02-123 > | Peak power
           | 0-02-124 > | Average power
           | 0-02-125 > | Pulse repetition frequency
           | 0-02-126 > | Pulse width
           | 0-02-127 > | Receiver intermediate frequency
           | 0-02-128 > | Intermediate frequency bandwidth
           | 0-02-129 > | Minimum detectable signal
           | 0-02-130 > | Dynamic range
           | 0-02-131   | Sensitivity time control

  3-21-006 | INTGCHAR   ;     ; Integration characteristics
           | 0-25-001 > | Range-gate length
           | 0-25-002 > | Number of gates averaged
           | 0-25-003 > | Number of integrated pulses
           | 0-25-005   | Echo integration

  3-21-007 | CORRECTS   ;     ; Corrections
           | 0-25-009 > | Calibration method
           | 0-25-010 > | Clutter treatment
           | 0-25-011 > | Ground occultation correction
           | 0-25-012 > | Range attenuation correction
           | 0-25-013 > | Bright-band correction
           | 0-25-015 > | Radome attenuation correction
           | 0-25-016 > | Clear-air attenuation correction
           | 0-25-017   | Precipitation attenuation correction

  3-21-008 | Z2RCONVR   ;     ; Z to R conversion
           | 0-25-006 > | Z to R conversion
           | 0-25-007 > | Z to R conversion factor
           | 0-25-008   | Z to R conversion exponent

  3-21-009 | A2ZLAWSQ   ;     ; A to Z law
           | 0-25-018 > | A to Z law for attenuation factor
           | 0-25-019   | A to Z law for attenuation exponent

  3-21-010 | ANTACHAR   ;     ; Antenna characteristics
           | 0-02-101 > | Type of antenna
           | 0-07-002 > | Altitude of the tower base
           | 0-02-102 > | Antenna height above tower base
           | 0-02-103 > | Radome
           | 0-02-104 > | Antenna polarisation
           | 0-02-105 > | Maximum antenna gain
           | 0-02-106 > | 3-dB beamwidth
           | 0-02-107 > | Sidelobe suppression
           | 0-02-108 > | Crosspol discrimination (on axis)
           | 0-02-109 > | Antenna speed (azimuth)
           | 0-02-110 > | Antenna speed (elevation)
           | 0-02-132 > | Azimuth pointing accuracy
           | 0-02-133   | Elevation pointing accuracy

  3-21-011 | GNRLCHAR   ;     ; General characteristics
           | 0-30-031 > | Picture type
           | 0-30-032 > | Combination with other data
           | 0-29-002   | Coordinate grid type

  3-21-012 | ANTAELEV   ;     ; Antenna elevations
           | 1-01-000 > | Delayed replication of 1 descriptor
           | 0-31-001 > | Replication factor
           | 0-02-135   | Antenna elevation

  3-21-021 | PROFRASS   ;     ; Basic information System/site header on Wind profiler/RASS
           | 0-02-003 > | Type of measuring equipment used
           | 0-02-101 > | Type of antenna
           | 2-01-130 > | Change width to 8 bits
           | 0-02-106 > | 3-dB beamwidth
           | 2-01-000 > | Change width back to Table B
           | 2-01-132 > | Change width to 11 bits
           | 2-02-130 > | Change scale to -6
           | 0-02-121 > | Mean frequency
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000 > | Change width back to Table B
           | 2-01-133 > | Change width to 11 bits
           | 2-02-129 > | Change scale to 0 
           | 0-25-001 > | Range-gate length
           | 2-02-000 > | Change scale back to Table B
           | 2-01-000   | Change width back to Table B

  3-21-022 | WNPROFPW   ;     ; Wind profiler: Processed-data winds
           | 0-07-007 > | Height
           | 2-04-001 > | Add associated field of 1 bit in length
           | 0-31-021 > | Associated field significance
           | 0-11-001 > | Wind direction
           | 2-04-000 > | Cancel add associated field
           | 0-11-002 > | Wind speed
           | 2-04-001 > | Add associated field of 1 bit in length
           | 0-31-021 > | Associated field significance
           | 0-11-006 > | w-component
           | 2-04-000 > | Cancel add associated field
           | 0-21-030   | Signal to noise ratio

  3-21-023 | WNPROFRW   ;     ; Wind profiler: Raw-data winds
           | 0-07-007 > | Height
           | 0-21-091 > | Radar signal Doppler spectrum 0th moment
           | 0-21-030 > | Signal to noise ratio
           | 2-02-129 > | Change scale to 2
           | 0-21-014 > | Doppler mean velocity (radial)
           | 2-01-129 > | Change width to 9 bits
           | 0-21-017 > | Doppler velocity spectral width
           | 2-02-000 > | Change scale back to table B
           | 2-01-000   | Change width back to table B

  3-21-024 | RASSPROC   ;     ; RASS-Mode: Processed-data RASS
           | 0-07-007 > | Height
           | 2-04-001 > | Add associated field of 1 bit in length
           | 0-31-021 > | Associated field significance
           | 0-12-007 > | Virtual temperature
           | 0-11-006 > | w-component
           | 2-04-000 > | Cancel add associated field
           | 0-21-030   | Signal to noise ratio

  3-21-025 | RASSRAWD   ;     ; RASS-Mode: Raw-data RASS
           | 0-07-007 > | Height
           | 0-21-091 > | Radar signal Doppler spectrum 0th moment
           | 0-21-030 > | Signal to noise ratio
           | 2-02-129 > | Change scale to 2
           | 0-21-014 > | Doppler mean velocity (radial)
           | 2-01-129 > | Change width to 9 bits
           | 0-21-017 > | Doppler velocity spectral width
           | 2-02-000 > | Change scale back to table B
           | 2-01-000 > | Change width back to table B
           | 0-21-092 > | RASS signal Doppler spectrum 0th moment, referring to RASS signal
           | 0-21-030 > | Signal to noise ratio, referring to RASS signal
           | 0-25-092 > | Acoustic propagation velocity
           | 2-01-129 > | Change width to 9 bits
           | 2-02-129 > | Change scale to 2
           | 0-21-017 > | Doppler velocity spectral width, referring to RASS signal
           | 2-02-000 > | Change scale back to table B
           | 2-01-000   | Change width back to table B

  3-21-026 | RASSFLUX   ;     ; RASS data - fluxes
           | 0-07-007 > | Height
           | 2-04-001 > | Add associated field of 1 bit in length
           | 0-31-021 > | Associated field significance
           | 0-12-007 > | Virtual temperature
           | 0-25-091 > | Structure constant of the refraction index (Cn2)
           | 0-11-071 > | Turbulent vertical momentum flux
           | 0-11-072 > | Turbulent vertical buoyancy flux
           | 0-11-073 > | Turbulent kinetic energy
           | 0-11-074 > | Dissipation energy
           | 2-04-000   | Cancel add associated field

  3-21-027 | SIGMA0PR   ;     ;  
           | 0-21-118 > | Attenuation correction on sigma-0
           | 2-02-129 > | Change scale
           | 2-01-132 > | Change data width
           | 0-02-112 > | Radar look angle
           | 2-01-000 > | Change data width back to Table B
           | 2-01-131 > | Change data width
           | 0-02-111 > | Radar incidence angle
           | 2-01-000 > | Change data width back to Table B
           | 2-02-000 > | Change scale back to Table B
           | 0-02-104 > | Antenna polarization
           | 0-21-105 > | Normalized radar cross-section
           | 0-21-106 > | Kp variance coefficient (alpha)
           | 0-21-107 > | Kp variance coefficient (beta)
           | 0-21-114 > | Kp variance coefficient (gamma)
           | 0-21-115 > | SEAWINDS sigma-0 quality
           | 0-21-116 > | SEAWINDS sigma-0 mode
           | 0-08-018 > | SEAWINDS land/ice surface type
           | 0-21-117   | Sigma-0 variance quality control

  3-21-028 | SIGMA0FL   ;     ;  
           | 0-21-118 > | Attenuation correction on sigma-0
           | 2-02-129 > | Change scale
           | 2-01-132 > | Change data width
           | 0-02-112 > | Radar look angle
           | 2-01-000 > | Data width back to Table B
           | 2-01-131 > | Change data width
           | 0-02-111 > | Radar incidence angle
           | 2-01-000 > | Data width back to Table B
           | 2-02-000 > | Scale back  to table B
           | 0-02-104 > | Antenna polarization
           | 0-21-123 > | SEAWINDS normalized radar cross section
           | 0-21-106 > | Kp variance coefficient (alpha)
           | 0-21-107 > | Kp variance coefficient (beta)
           | 0-21-114 > | Kp variance coefficient (gamma)
           | 0-21-115 > | SEAWINDS sigma-0 quality flag
           | 0-21-116 > | SEAWINDS sigma-0 mode flag
           | 0-08-018 > | SEAWINDS land/ice surface flag
           | 0-21-117   | Sigma-0 variance quality control

  3-21-030 | ASCATSG0   ;     ; ASCAT sigma-0 information
           | 0-08-085 > | Beam identifier
           | 2-02-129 > | Increase scaling by 10^1
           | 2-01-131 > | Increase data width by 3 bits
           | 0-02-111 > | Radar incidence angle
           | 2-01-000 > | Cancel change data width
           | 2-02-000 > | Cancel change scaling
           | 0-02-134 > | Antenna beam azimuth
           | 0-21-062 > | Backscatter
           | 0-21-063 > | Radiometric resolution (noise value)
           | 0-21-158 > | ASCAT kp estimate quality
           | 0-21-159 > | ASCAT sigma-0 usability
           | 0-21-160 > | ASCAT synthetic data quality
           | 0-21-161 > | ASCAT synthetic data quantity
           | 0-21-162 > | ASCAT satellite orbit and attitude quality
           | 0-21-163 > | ASCAT solar array reflection contamination
           | 0-21-164 > | ASCAT telemetry presence and quality
           | 0-21-165 > | ASCAT extrapolated reference function
           | 0-21-166   | Land fraction

  3-40-001 | IASIL1CD   ;     ; IASI Level 1c data
           | 0-01-007 > | Satellite identifier
           | 0-01-031 > | Identification of originating/generating centre
           | 0-02-019 > | Satellite instruments
           | 0-02-020 > | Satellite classification
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 2-02-131 > | Add 3 to scale
           | 2-01-138 > | Add 10 to width
           | 0-04-006 > | Second
           | 2-01-000 > | Reset width
           | 2-02-000 > | Reset scale
           | 0-05-001 > | Latitude (high accuracy)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-07-024 > | Satellite zenith angle
           | 0-05-021 > | Bearing or azimuth
           | 0-07-025 > | Solar zenith angle
           | 0-05-022 > | Solar azimuth
           | 0-05-043 > | Field of view number
           | 0-05-040 > | Orbit number
           | 2-01-133 > | Add 5 to width
           | 0-05-041 > | Scan line number
           | 2-01-000 > | Reset width
           | 2-01-132 > | Add 4 to width
           | 0-25-070 > | Major frame count
           | 2-01-000 > | Reset width
           | 2-02-126 > | Subtract 2 from scale
           | 0-07-001 > | Height of station
           | 2-02-000 > | Reset scale
           | 0-33-060 > | Individual IASI-system quality flag
           | 0-33-061 > | Indicator for instrument noise performance (contributions from spectral and radiometric)
           | 0-33-062 > | Indicator for geometric quality index
           | 0-33-063 > | Indicator for instrument noise performance (contributions from radiometric calibration)
           | 0-33-064 > | Indicator for instrument noise performance (contributions from spectral calibration)
           | 0-33-065 > | Output of system TEC (Technical Expertise Center) quality function
           | 1-01-010 > | Repeat next 1 descriptor 10 times
           | 3-40-002 > | IASI Level 1c band description
           | 1-01-087 > | Repeat next 1 descriptor 87 times
           | 3-40-003 > | IASI Level 1c 100 channel sequence
           | 0-02-019 > | Satellite instruments
           | 0-25-051 > | AVHRR channel combination
           | 1-01-007 > | Repeat next 1 descriptor 7 times
           | 3-40-004   | IASI Level 1c AVHRR single scene sequence

  3-40-002 | IASIL1CB   ;     ; IASI Level 1c band description
           | 0-25-140 > | Start channel
           | 0-25-141 > | End channel
           | 0-25-142   | Channel scale factor

  3-40-003 | IASIL1CC   ;     ; IASI Level 1c 100 channel
           | 1-04-100 > | Repeat next 4 descriptor 100 times
           | 2-01-136 > | Add 8 to width
           | 0-05-042 > | Channel number
           | 2-01-000 > | Reset width
           | 0-14-046   | Scaled IASI radiance

  3-40-004 | IASIL1CS   ;     ; IASI Level 1c AVHRR single scene
           | 0-05-060 > | Y angular position from centre of gravity
           | 0-05-061 > | Z angular position from centre of gravity
           | 0-25-085 > | Fraction of clear pixels in HIRS FOV
           | 1-05-006 > | Repeat next 5 descriptor 6 times
           | 0-05-042 > | Channel number
           | 0-25-142 > | Channel scale factor
           | 0-14-047 > | Scaled mean AVHRR radiance
           | 0-25-142 > | Channel scale factor
           | 0-14-048   | Scaled std dev AVHRR radiance

  3-40-005 | JASNOGDR   ;     ;  
           | 0-01-007 > | Satellite identifier
           | 0-02-019 > | Satellite instrument used
           | 0-01-096 > | Station acquisition
           | 0-25-061 > | Software identification
           | 0-05-044 > | Satellite cycle number
           | 0-05-040 > | Orbit number
           | 0-01-030 > | Numerical model identifier
           | 0-04-001 > | Year
           | 0-04-002 > | Month
           | 0-04-003 > | Day
           | 0-04-004 > | Hour
           | 0-04-005 > | Minute
           | 0-04-007 > | Second within a minute (microsecond accuracy)
           | 0-05-001 > | Latitude (high accuracy)
           | 0-06-001 > | Longitude (high accuracy)
           | 0-08-029 > | Remotely sensed surface type
           | 0-08-074 > | Altimeter echo type
           | 0-08-077 > | Radiometer sensed surface type
           | 0-40-011 > | Interpolation flag
           | 0-25-097 > | Three-dimensional error estimate of the navigator orbit
           | 0-25-095 > | Altimeter state flag
           | 0-25-098 > | Altimeter data quality flag
           | 0-25-099 > | Altimeter correction quality flag
           | 0-21-144 > | Altimeter rain flag
           | 0-25-096 > | Radiometer state flag
           | 0-40-012 > | Radiometer data quality flag
           | 0-40-013 > | Radiometer brightness temperature interpretation flag
           | 0-21-169 > | Ice presence indicator
           | 0-22-151 > | Ku band ocean range
           | 0-22-162 > | RMS of 20 Hz Ku band ocean range
           | 0-22-163 > | Number of 20 Hz valid points for Ku band
           | 0-25-160 > | Ku band net instrumental correction
           | 0-25-133 > | Sea state bias correction on Ku band
           | 0-22-156 > | Ku band significant wave height
           | 0-22-164 > | RMS 20 Hz Ku band significant wave height
           | 0-22-165 > | Number of 20 Hz valid points for Ku band significant wave height
           | 0-22-166 > | Ku band net instrumental correction for significant wave height
           | 0-21-137 > | Ku band corrected ocean backscatter coefficient
           | 0-21-138 > | STD Ku band corrected ocean backscatter coefficient
           | 0-22-167 > | Number of valid points for Ku band backscatter
           | 0-21-139 > | Ku band net instrumental correction for AGC
           | 0-21-118 > | Attenuation correction on sigma-0
           | 0-21-145 > | Ku band automatic gain control
           | 0-21-146 > | RMS Ku band automatic gain control
           | 0-21-147 > | Number of valid points for Ku band automatic gain control 
           | 0-22-168 > | C band ocean range
           | 0-22-169 > | RMS of C band ocean range
           | 0-22-170 > | Number of 20 Hz valid points for C band
           | 0-25-161 > | C band net instrumental correction
           | 0-25-162 > | Sea state bias correction on C band
           | 0-22-171 > | C band significant wave height
           | 0-22-172 > | RMS 20 Hz C band significant wave height
           | 0-22-173 > | Number of 20 Hz valid points for C band significant wave height
           | 0-22-174 > | C band net instrumental correction for significant wave height
           | 0-21-170 > | C band corrected ocean backscatter coefficient
           | 0-21-171 > | RMS C band corrected ocean backscatter coefficient
           | 0-22-175 > | Number of valid points for C band backscatter
           | 0-21-172 > | C band net instrumental correction for AGC
           | 0-21-118 > | Attenuation correction on sigma-0
           | 0-21-173 > | C band automatic gain control
           | 0-21-174 > | RMS C band automatic gain control
           | 0-21-175 > | Number of valid points for C band automatic gain control
           | 0-02-153 > | Satellite channel center frequency
           | 0-12-063 > | Brightness temperature
           | 0-02-153 > | Satellite channel center frequency
           | 0-12-063 > | Brightness temperature
           | 0-02-153 > | Satellite channel center frequency
           | 0-12-063 > | Brightness temperature
           | 0-13-090 > | Radiometer water vapor content
           | 0-13-091 > | Radiometer liquid content
           | 0-07-002 > | Height or altitude
           | 0-11-097 > | Wind speed from altimeter
           | 0-11-098 > | Wind speed from radiometer
           | 0-07-002 > | Height or altitude
           | 0-11-095 > | U component of model wind vector
           | 0-11-096 > | V component of model wind vector
           | 0-10-096 > | Mean dynamic topography
           | 0-10-081 > | Altitude of COG above reference ellipsoid
           | 0-10-082 > | Instantaneous altitude rate
           | 0-10-083 > | Squared off nadir angle of the satellite from platform data
           | 0-10-101 > | Squared off nadir angle of the satellite from waveform data
           | 0-25-132 > | Ionospheric correction from model on Ku band
           | 0-25-163 > | Altimeter ionospheric correction on Ku band
           | 0-25-126 > | Model dry tropospheric correction
           | 0-25-128 > | Model wet tropospheric correction
           | 0-25-164 > | Radiometer wet tropospheric correction
           | 0-10-085 > | Mean sea surface height
           | 0-10-097 > | Mean sea surface height from altimeter only
           | 0-10-086 > | Geoid height
           | 0-10-087 > | Ocean depth/land elevation
           | 0-10-092 > | Solid earth tide height
           | 0-10-088 > | Total geocentric ocean tide height solution 1
           | 0-10-089 > | Total geocentric ocean tide height solution 2
           | 0-10-098 > | Loading tide height geocentric ocean tide solution 1
           | 0-10-099 > | Loading tide height geocentric ocean tide solution 2
           | 0-10-090 > | Long period tide height
           | 0-10-100 > | Non-equilibrium long period tide height
           | 0-10-093 > | Geocentric pole tide height
           | 0-25-127 > | Inverted barometer correction
           | 0-40-014   | High frequency fluctuations of the sea surface topography correction

END
