#
# BUFR Table B - Classification of Elements
#
#                                       Data
#F      X       Y       Scale   RefVal  Width   Units           Element Name
  0;    0;      1;      0;           0;   24;    CCITT_IA5; TABLE A ENTRY
  0;    0;      2;      0;           0;  256;    CCITT_IA5; TABLE A  DATA CATEGORY DESCRIPTIO
  0;    0;      3;      0;           0;  256;    CCITT_IA5; TABLE A DATA CATEGORY DESCRIPTION
  0;    0;      5;      0;           0;   24;    CCITT_IA5; BUFR EDITION NUMBER
  0;    0;     10;      0;           0;    8;    CCITT_IA5; F DESCRIPTOR TO BE ADDED OR DEFIN
  0;    0;     11;      0;           0;   16;    CCITT_IA5; X DESCRIPTOR TO BE ADDED OR DEFIN
  0;    0;     12;      0;           0;   24;    CCITT_IA5; Y DESCRIPTOR TO BE ADDED OR DEFIN
  0;    0;     13;      0;           0;  256;    CCITT_IA5; ELEMENT NAME LN 1
  0;    0;     14;      0;           0;  256;    CCITT_IA5; ELEMENT NAME LN 2
  0;    0;     15;      0;           0;  192;    CCITT_IA5; UNITS NAME
  0;    0;     16;      0;           0;    8;    CCITT_IA5; UNITS SCALE SIGN
  0;    0;     17;      0;           0;   24;    CCITT_IA5; UNITS SCALE
  0;    0;     18;      0;           0;    8;    CCITT_IA5; UNITS REFERENCE SIGN
  0;    0;     19;      0;           0;   80;    CCITT_IA5; UNITS REFERENCE VALUE
  0;    0;     20;      0;           0;   24;    CCITT_IA5; ELEMENT DATA WIDTH
  0;    0;     30;      0;           0;   48;    CCITT_IA5; DESCRIPTOR DEFINING SEQUENCE
  0;    1;      1;      0;           0;    7;      NUMERIC; WMO BLOCK NUMBER
  0;    1;      2;      0;           0;   10;      NUMERIC; WMO STATION NUMBER
  0;    1;      3;      0;           0;    3;      NUMERIC; WMO REGION NUMBER
  0;    1;      4;      0;           0;    3;      NUMERIC; WMO REGION SUB-AREA
  0;    1;      5;      0;           0;   17;      NUMERIC; BUOY/PLATFORM IDENTIFIER
  0;    1;      6;      0;           0;   64;    CCITT_IA5; AIRCRAFT IDENTIFIER (FLIGHT NUMBE
  0;    1;      7;      0;           0;   10;   CODE_TABLE; SATELLITE IDENTIFIER
  0;    1;      8;      0;           0;   64;    CCITT_IA5; AIRCRAFT REGISTRATION NUMBER (TAI
  0;    1;      9;      0;           0;   64;    CCITT_IA5; TYPE OF COMMERCIAL ACFT
  0;    1;     10;      0;           0;   64;    CCITT_IA5; STATIONARY BOUY PLATFORM IDENTIFI
  0;    1;     11;      0;           0;   72;    CCITT_IA5; SHIP CALL SIGN
  0;    1;     12;      0;           0;    9; DEGREES_TRUE; DIRECTION OF MOTION OBSERVING PLA
  0;    1;     13;      0;           0;   10; METER/SECOND; SPEED OF MOTION OF OBSERVING PLAT
  0;    1;     14;      2;           0;   10; METER/SECOND; PLATFORM DRIFT SPEED (HIGH PRECIS
  0;    1;     15;      0;           0;    4;   CODE_TABLE; TRUE DIR OF MOVING PLATFORM PAST
  0;    1;     16;      0;           0;    4;   CODE_TABLE; AVG SPD MOVING PLATFORM PAST 3 HO
  0;    1;     18;      0;           0;   40;    CCITT_IA5; SHORT STATION OR SITE NAME
  0;    1;     19;      0;           0;  256;    CCITT_IA5; LONG STATION OR SITE NAME
  0;    1;     20;      0;           0;    4;      NUMERIC; WMO REGION SUB-AREA
  0;    1;     21;      0;           0;   14;      NUMERIC; SYNOPTIC FEATURE ID
  0;    1;     25;      0;           0;   24;    CCITT_IA5; STORM IDENTIFIER
  0;    1;     26;      0;           0;   64;    CCITT_IA5; WMO STORM NAME
  0;    1;     31;      0;           0;   16;   CODE_TABLE; GENERATING CENTER
  0;    1;     32;      0;           0;    8;   CODE_TABLE; GENERATING APPLICATION
  0;    1;     50;      0;           0;   48;    CCITT_IA5; NMC REPORT IDENTIFIER
  0;    1;     62;      0;           0;   40;    CCITT_IA5; NAT'L ASSIGNED STATION IDENTIFIER
  0;    1;     63;      0;           0;   64;    CCITT_IA5; ICAO LOCATION IDENTIFIER
  0;    1;    192;      0;           0;    4;    CCITT_IA5; RADIOSONDE REPORT PART
  0;    1;    193;      0;           0;   64;    CCITT_IA5; SATELLITE IDENTIFIER
  0;    1;    194;      0;           0;   64;    CCITT_IA5; BULLETIN HEADER
  0;    1;    195;      0;           0;   48;    CCITT_IA5; NMC REPORT IDENTIFIER
  0;    1;    196;      0;           0;   96;    CCITT_IA5; ALPHANUMERIC IDENTIFIER
  0;    1;    197;      0;           0;   64;    CCITT_IA5; RADIOSONDE SHIP OR MOBILE LND STN
  0;    2;      1;      0;           0;    2;   CODE_TABLE; TYPE OF STATION
  0;    2;      2;      0;           0;    4;   FLAG_TABLE; TYPE OF INSTR. FOR WIND MEASUREME
  0;    2;      3;      0;           0;    4;   CODE_TABLE; TYPE OF MEASURING INSTRUMENT USED
  0;    2;      4;      0;           0;    4;   CODE_TABLE; TYPE OF INSTR/CROP FOR EVAP/EVAPO
  0;    2;      5;      2;           0;    7;      DEGREES; PRECISION OF TEMPERATURE OBS.
  0;    2;     11;      0;           0;    8;   CODE_TABLE; RADIOSONDE TYPE
  0;    2;     12;      0;           0;    4;   CODE_TABLE; RADIOSONDE COMPUTATIONAL METHOD
  0;    2;     13;      0;           0;    4;   CODE_TABLE; SOLAR AND INFRARED RADIATION CORR
  0;    2;     14;      0;           0;    7;   CODE_TABLE; TRACKING TECHNIQUE/STATUS OF SYST
  0;    2;     15;      0;           0;    4;   CODE_TABLE; RADIOSONDE COMPLETENESS
  0;    2;     21;      0;           0;    9;   FLAG_TABLE; SATELLITE INSTRUMENT DATA USED IN
  0;    2;     22;      0;           0;    8;   FLAG_TABLE; SATELLITE DATA PROCESSING TECHNIQ
  0;    2;     23;      0;           0;    4;   CODE_TABLE; SATELLITE DERIVED WIND COMPUTATIO
  0;    2;     24;      0;           0;    4;   CODE_TABLE; INT. MEAN HUMIDITY COMPUTATIONAL
  0;    2;     25;      0;           0;   25;   FLAG_TABLE; SATELLITE CHANNEL(S) USED IN COMP
  0;    2;     26;      2;           0;   12;       METERS; CROSS TRACK RESOLUTION
  0;    2;     27;      2;           0;   12;       METERS; ALONG TRACK RESOLUTION
  0;    2;     28;      0;           0;   32;   FLAG_TABLE; GEOSTAT. SOUNDER SATELL CHAN'LS U
  0;    2;     29;      0;           0;    8;   FLAG_TABLE; GEOSTAT. SOUNDER SATELL CHAN'LS U
  0;    2;     30;      0;           0;    3;   CODE_TABLE; METH OF CURRENT MEASUREMENT
  0;    2;     31;      0;           0;    5;   CODE_TABLE; DURATION & TIME OF CURRENT CODE M
  0;    2;     32;      0;           0;    2;   CODE_TABLE; INDICATOR FOR DIGITIZATION
  0;    2;     33;      0;           0;    3;   CODE_TABLE; METHOD OF SALINITY/DEPTH MEASUREM
  0;    2;     34;      0;           0;    5;   CODE_TABLE; DROGUE TYPE
  0;    2;     35;      0;           0;    9;       METERS; CABLE LENGTH
  0;    2;     36;      0;           0;    2;   CODE_TABLE; BUOY TYPE
  0;    2;     37;      0;           0;    3;   CODE_TABLE; METHOD OF TIDAL OBSERVATION
  0;    2;     38;      0;           0;    3;   CODE_TABLE; METH OF SEA SURFACE TEMPERATURE M
  0;    2;     39;      0;           0;    3;   CODE_TABLE; METH OF WET BULB TEMPERATURE MEAS
  0;    2;     40;      0;           0;    4;   CODE_TABLE; METH RMV CODE VELOC & MOTION OF P
  0;    2;     41;      0;           0;    6;   CODE_TABLE; METH FOR EST RPTS OF SYNOP FEATUR
  0;    2;     42;      0;           0;    6;   CODE_TABLE; METHOD OF REPORT CONSTRUCTION
  0;    2;     43;      0;           0;    6;   CODE_TABLE; PRECISION OF LAT/LON REPORT
  0;    2;     51;      0;           0;    4;   CODE_TABLE; INDIC TO SPECIFY OBS METH EXTRM T
  0;    2;     61;      0;           0;    3;   CODE_TABLE; AIRCRAFT NAVIGATION   SYSTEM
  0;    2;     62;      0;           0;    4;   CODE_TABLE; TYPE OF AIRCRAFT DATA RELAY SYSTE
  0;    2;     63;      2;      -18000;   16;      DEGREES; AIRCRAFT ROLL ANGLE
  0;    2;     70;      0;           0;    4;   CODE_TABLE; ORIGINAL SPECIFICATION OF LAT/LON
  0;    2;    101;      0;           0;    4;   CODE_TABLE; TYPE OF ANTENNA
  0;    2;    102;      0;           0;    8;       METERS; ANTENNA HGT ABOVE TOWER
  0;    2;    103;      0;           0;    2;        FLAGE; TABLE     RADOME
  0;    2;    104;      0;           0;    4;   CODE_TABLE; ANTENNA POLARIZATION
  0;    2;    105;      0;           0;    6;           DB; MAXIMUM ANTENNA GAIN
  0;    2;    106;      1;           0;    6;      DEGREES; 3 - DB BANDWIDTH
  0;    2;    107;      0;           0;    6;           DB; SIDELOBE SUPRESSION
  0;    2;    108;      0;           0;    6;           DB; CROSSPOL DISCRI. (ON AXIS)
  0;    2;    109;      2;           0;   12; DEGREES/SECOND; ANTENNA SPEED (AZIMUTH)
  0;    2;    110;      2;           0;   12; DEGREES/SECOND; ANTENNA SPEED (ELEVATION)
  0;    2;    111;      1;           0;   10;      DEGREES; RADAR INCIDENCE ANGLE
  0;    2;    112;      1;           0;   12;      DEGREES; RADAR AZIMUTH ANGLE
  0;    2;    113;      0;           0;    4;     NUMERICS; NO. OF AZIMUTH LOOKS
  0;    2;    114;      0;           0;   15;         M**2; ANTENNA EFFECTIVE SURFACE AREA
  0;    2;    121;      8;           0;    7;           HZ; MEAN FREQUENCY
  0;    2;    122;      6;        -128;    8;           HZ; FREQUENCY AGILITY RANGE
  0;    2;    123;      4;           0;    7;        WATTS; PEAK POWER
  0;    2;    124;      1;           0;    7;        WATTS; AVERAGE POWER
  0;    2;    125;      1;           0;    8;           HZ; PULSE REPETITION FREQUENCY
  0;    2;    126;      7;           0;    6;       SECOND; PULSE WIDTH
  0;    2;    127;      6;           0;    7;           HZ; RECEIVER INTERMEDIATE FREQUENCY
  0;    2;    128;      5;           0;    6;           HZ; INTERMEDIATE FREQUENCY BANDWIDTH
  0;    2;    129;      0;        -150;    5;           DB; MINIMUM DETECTABLE SIGNAL
  0;    2;    130;      0;           0;    7;           DB; DYNAMIC RANGE
  0;    2;    131;      0;           0;    2;   FLAG_TABLE; SENSITIVITY TIME CONTROL
  0;    2;    132;      2;           0;    6;      DEGREES; AZIMUTH POINTING ACCURACY
  0;    2;    133;      2;           0;    6;      DEGREES; ELEVATION POINTING ACCURACY
  0;    2;    134;      2;           0;   16;      DEGREES; ANTENNA BEAM AZIMUTH
  0;    2;    135;      2;       -9000;   15;      DEGREES; ANTENNA ELEVATION
  0;    2;    140;      0;           0;    9;      DEGREES; SATELLITE RADAR BEAM AZIMUTH ANGL
  0;    2;    141;      0;           0;   24;    CCITT_IA5; MEAS.TYPE SERIAL NBR/IDENT
  0;    2;    142;      0;           0;   32;    CCITT_IA5; OZONE INSTRUMENT
  0;    2;    143;      0;           0;    7;      NUMERIC; INSTRUMENT TYPE
  0;    2;    183;      0;           0;    1;   CODE_TABLE; QUALITY OF PRESSURE MEASUREMENT
  0;    2;    184;      0;           0;    1;   CODE_TABLE; QUALITY OF WATER SFC TEMP MEASURE
  0;    2;    185;      0;           0;    1;   CODE_TABLE; QUALITY OF AIR TEMP MEASUREMENT
  0;    2;    186;      0;           0;    3;   CODE_TABLE; QUAL CONTROL INDIC FOR FOLLOWING
  0;    2;    187;      0;           0;    1;   CODE_TABLE; QUALITY OF BUOY SATELLIT TRANSMIS
  0;    2;    188;      0;           0;    3;   CODE_TABLE; QUAL CONTROL INDICATOR FOR BUOY L
  0;    2;    189;      0;           0;    3;   CODE_TABLE; QUAL CONTROL INDIC FOR BUOY TIME
  0;    2;    190;      0;           0;    8;   CODE_TABLE; U, V QUALITY INDICATOR
  0;    2;    191;      0;           0;    4;   CODE_TABLE; W QUALITY INDICATOR
  0;    2;    192;      0;           0;    6;   CODE_TABLE; RADIOSONDE CORRECTION TYPE APPLIE
  0;    2;    193;      0;           0;    3;   CODE_TABLE; IND TYPE OF STN OPERATION PAST/PR
  0;    2;    200;      0;           0;    4;   CODE_TABLE; OBJECTIVE FORECAST TECHNIQUE USED
  0;    2;    206;      0;           0;    4;        MONTH; MONTH  - RELEASE TIME
  0;    2;    207;      0;           0;    6;          DAY; DAY    - RELEASE TIME
  0;    2;    208;      0;           0;    5;         HOUR; HOUR   - RELEASE TIME
  0;    2;    209;      0;           0;    6;       MINUTE; MINUTE - RELEASE TIME
  0;    2;    210;      0;           0;    3;   FLAG_TABLE; STATION/SEA LEVEL COMPARISON
  0;    4;      1;      0;           0;   12;         YEAR; YEAR
  0;    4;      2;      0;           0;    4;        MONTH; MONTH
  0;    4;      3;      0;           0;    6;          DAY; DAY
  0;    4;      4;      0;           0;    5;         HOUR; HOUR
  0;    4;      5;      0;           0;    6;       MINUTE; MINUTE
  0;    4;      6;      0;           0;    6;       SECOND; SECOND
  0;    4;     11;      0;       -1024;   11;        YEARS; TIME INCREMENT
  0;    4;     12;      0;       -1024;   11;       MONTHS; TIME INCREMENT
  0;    4;     13;      0;       -1024;   11;         DAYS; TIME INCREMENT
  0;    4;     14;      0;       -1024;   11;        HOURS; TIME INCREMENT
  0;    4;     15;      0;       -2048;   12;      MINUTES; TIME INCREMENT
  0;    4;     16;      0;       -4096;   13;      SECONDS; TIME INCREMENT
  0;    4;     21;      0;       -1024;   11;        YEARS; TIME PERIOD OR DISPLACEMENT
  0;    4;     22;      0;       -1024;   11;       MONTHS; TIME PERIOD OR DISPLACEMENT
  0;    4;     23;      0;       -1024;   11;         DAYS; TIME PERIOD OR DISPLACEMENT
  0;    4;     24;      0;       -2048;   12;        HOURS; TIME PERIOD OR DISPLACEMENT
  0;    4;     25;      0;       -2048;   12;      MINUTES; TIME PERIOD OR DISPLACEMENT
  0;    4;     26;      0;       -4096;   13;      SECONDS; TIME PERIOD OR DISPLACEMENT
  0;    4;     31;      0;           0;    8;         HOUR; DUR OF TIME REL TO FOLLOWING VALU
  0;    4;     41;      0;       -1440;   12;       MINUTE; TIME DIFFERENCE UTC - LMT
  0;    4;     43;      0;           0;    9;          DAY; DAY OF THE YEAR
  0;    4;     44;      0;           0;    3;   CODE_TABLE; DAY OF THE WEEK
  0;    4;     53;      0;           0;    6;      NUMERIC; NUMBER OF DAYS WITH PRECIP => 1MM
  0;    4;    192;      0;           0;   12;        HOURS; RECIEPT TIME - REPORT TIME
  0;    4;    193;      0;           0;   31;      MINUTES; RECIEPT TIME - REPORT TIME
  0;    4;    194;      0;           0;   12;        HOURS; RELEASE TIME OF SONDE
  0;    4;    195;      0;           0;    5;         HOUR; FORECAST CYCLE HOUR
  0;    4;    200;      0;           0;   12;         YEAR; YEAR   - TIME OF RECEIPT
  0;    4;    201;      0;           0;    4;        MONTH; MONTH  - TIME OF RECEIPT
  0;    4;    202;      0;           0;    6;          DAY; DAY    - TIME OF RECEIPT
  0;    4;    203;      0;           0;    5;         HOUR; HOUR   - TIME OF RECEIPT
  0;    4;    204;      0;           0;    6;       MINUTE; MINUTE - TIME OF RECEIPT
  0;    4;    205;      0;           0;    6;       SECOND; SECOND - TIME OF RECEIPT
  0;    4;    206;      0;           0;   32;       SECOND; DATA BASE INGEST TIME FROM 1 JAN
  0;    4;    207;      0;           0;    5;         HOUR; HOUR - TIME OF MAX WIND (GUST)
  0;    4;    208;      0;           0;    6;       MINUTE; MINUTE - TIME OF NAX WIND (GUST)
  0;    5;      1;      5;    -9000000;   25;      DEGREES; LATITUDE(HIGH ACCURACY)
  0;    5;      2;      2;       -9000;   15;      DEGREES; LATITUDE(COARSE ACCURACY)
  0;    5;      3;      2;       -9000;   15;      DEGREES; ALTERNATE LATITUDE
  0;    5;     11;      5;    -9000000;   25;      DEGREES; LATITUDE INCREMENT(HIGH ACCURACY)
  0;    5;     12;      2;       -9000;   15;      DEGREES; LATITUDE INCREMENT(COARSE ACCURAC
  0;    5;     21;      2;           0;   16; DEGREES_TRUE; BEARING OR AZIMUTH
  0;    5;     22;      2;           0;   16; DEGREES_TRUE; SOLAR AZIMUTH
  0;    5;     30;      0;           0;   12;      DEGREES; DIRECTION (SPECTRAL)
  0;    5;     31;      0;           0;   12;      NUMERIC; ROW NUMBER
  0;    5;     33;      1;           0;   16;       METERS; PIXEL SIZE ON HORIZONTAL-1
  0;    5;     34;      0;           0;   11;      NUMERIC; ALONG TRACK ROW NUMBER
  0;    5;     40;      0;           0;   24;      NUMERIC; ORBIT NUMBER
  0;    5;     41;      0;           0;    8;      NUMERIC; SCAN LINE NUMBER
  0;    5;     42;      0;           0;    6;      NUMERIC; CHANNEL NUMBER
  0;    5;     43;      0;           0;    8;      NUMERIC; FIELD OF VIEW NUMBER
  0;    5;     50;      5;           0;   17;      NUMERIC; SIGMA LEVEL
  0;    5;     52;      0;           0;    5;      NUMERIC; CHANNEL NUMBER INCREMENT
  0;    5;     53;      0;           0;    5;      NUMERIC; FIELD OF VIEW NUMBER INCREMENT
  0;    6;      1;      5;   -18000000;   26;      DEGREES; LONGITUDE (HIGH ACCURACY)
  0;    6;      2;      2;      -18000;   16;      DEGREES; LONGITUDE (COARSE ACCURACY)
  0;    6;      3;      2;      -18000;   16;      DEGREES; ALTERNATE LONGITUDE
  0;    6;     11;      5;   -18000000;   26;      DEGREES; LONGITUDE INCREMENT (HIGH ACCURAC
  0;    6;     12;      2;      -18000;   16;      DEGREES; LONGITUDE INCREMENT (COARSE ACCUR
  0;    6;     21;      1;           0;   13;       METERS; DISTANCE
  0;    6;     30;      5;           0;   13;        RAD/M; WAVENUMBER (SPECTRAL)
  0;    6;     31;      0;           0;   12;      NUMERIC; COLUMN NUMBER
  0;    6;     33;      1;           0;   16;       METERS; PIXEL SIZE ON HORIZONTAL-2
  0;    6;     34;      0;           0;    7;      NUMERIC; CROSS-TRACK CELL NUMBER
  0;    7;      1;      0;        -400;   15;       METERS; HEIGHT OF STATION
  0;    7;      2;      1;         -40;   16;       METERS; HEIGHT OR ALTITUDE
  0;    7;      3;      1;        -400;   17;    M**2/S**2; GEOPOTENTIAL
  0;    7;      4;      1;           0;   14;      PASCALS; PRESSURE
  0;    7;      5;      0;        -400;   12;       METERS; HEIGHT INCREMENT
  0;    7;      6;      0;           0;   15;       METERS; HEIGHT ABOVE STATION
  0;    7;      7;      0;       -1000;   17;            M; HEIGHT
  0;    7;      8;      0;      -10000;   20;    M**2/S**2; GEOPOTENTIAL
  0;    7;     21;      2;       -9000;   15;      DEGREES; ELEVATION
  0;    7;     22;      2;       -9000;   15;      DEGREES; SOLAR ELEVATION
  0;    7;     61;      2;           0;   14;       METERS; DEPTH BELOW LAND SURFACE
  0;    7;     62;      1;           0;   17;       METERS; DEPTH BELOW SEA SURFACE
  0;    7;    190;      0;           0;   12;       METERS; HEIGHT INCREMENT
  0;    7;    192;      0;        -400;   17;          GPM; FLIGHT LEVEL (PRESSURE ALTITUDE)
  0;    7;    193;      0;        -400;   17;         GPDM; FLIGHT LEVEL (PRESSURE ALTITUDE)
  0;    7;    194;      0;        -400;   15;            M; HEIGHT OR ALTITUDE ABOVE MSL
  0;    8;      1;      0;           0;    7;   FLAG_TABLE; VERTICAL SOUNDING SIGNIFICANCE
  0;    8;      2;      0;           0;    6;   CODE_TABLE; VERT. SIGNIFICANCE (SFC OBSERVATI
  0;    8;      3;      0;           0;    6;   CODE_TABLE; VERT. SIGNIFICANCE (SAT OBSERVATI
  0;    8;      4;      0;           0;    3;   CODE_TABLE; PHASE OF AIRCRAFT FLIGHT
  0;    8;      5;      0;           0;    4;   CODE_TABLE; SURFACE SYNOPTIC FEATURE SIGNIFIC
  0;    8;     10;      0;           0;    4;   CODE_TABLE; VERT SIGNIFICANCE(FORECAST SOUNDI
  0;    8;     11;      0;           0;    6;   CODE_TABLE; HORIZONTAL SIGNIFICANCE
  0;    8;     12;      0;           0;    2;   CODE_TABLE; LAND/SEA QUALIFIER
  0;    8;     13;      0;           0;    2;   CODE_TABLE; DAY/NIGHT QUALIFIER
  0;    8;     20;      0;           0;   16;      NUMERIC; TOTAL NR MISG ENTITIES W/RES TO A
  0;    8;     21;      0;           0;    5;   CODE_TABLE; TIME SIGNIFICANCE
  0;    8;     22;      0;           0;   16;      NUMERIC; TOTAL NUMBER(W/RESPECT TO ACCUM O
  0;    8;     23;      0;           0;    7;   CODE_TABLE; FIRST ORDER STATISTICS
  0;    8;     24;      0;           0;    7;   CODE_TABLE; DIFFERENCE STATISTICS
  0;    8;     31;      0;           0;    8;         BUFR; TABLE A    DATA CATEGORY
  0;    8;     32;      0;           0;   14;   CODE_TABLE; DATA SIGNIF-INTERACTIVE RETRIEVAL
  0;    8;     51;      0;           0;    3;   CODE_TABLE; QUALIFIER-NR MISG VALUES IN CALC
  0;    8;     52;      0;           0;    5;   CODE_TABLE; COND. FOR  WHICH NR OF DAYS OF OC
  0;    8;     53;      0;           0;    2;   CODE_TABLE; DAY OF OCCURRENCE QUALIFIER
  0;    8;     77;      0:           0;    7;   CODE_TABLE: RADIOMETER SENSED SURFACE TYPE
  0;    8;    192;      0;           0;   16;      NUMERIC; UPDATE SEQUENCE NUMBER
  0;    8;    193;      0;           0;   16;      NUMERIC; OBSERVATION DATABASE KEY
  0;    8;    194;      0;           0;    6;   CODE_TABLE; CORRECTION INDICATOR
  0;    8;    195;      0;           0;    6;   CODE_TABLE; QUALITY CONTROL TYPE
  0;    8;    196;      0;           0;    6;   CODE_TABLE; QUALITY CONTROL DECISION
  0;    8;    197;      0;           0;    5;   CODE_TABLE; RECORD TEMPERATURE KEY
  0;    8;    198;      0;           0;    4;   CODE_TABLE; TIME SIGNIFICANCE
  0;    8;    199;      0;           0;    3;   CODE_TABLE; SOURCE UNITS OF WIND SPEED
  0;    8;    200;      0;           0;    4;      NUMERIC; NMC QUALITY MARK
  0;    8;    232;      0;           0;   14;   CODE_TABLE; DATA SIGNIF-INTERACTIVE RETRIEVAL
  0;    9;      6;      3;           0;   10;      SECONDS; TIME OF ASCENDING NODE
  0;   10;      1;      0;        -400;   15;       METERS; HEIGHT OF LAND SURFACE
  0;   10;      2;      1;         -40;   16;       METERS; HEIGHT
  0;   10;      3;      1;        -400;   17;    M**2/S**2; GEOPOTENTIAL
  0;   10;      4;      1;           0;   14;      PASCALS; PRESSURE
  0;   10;      7;      0;       -1000;   17;       METERS; HEIGHT
  0;   10;      8;      0;      -10000;   20;    M**2/S**2; GEOPOTENTIAL
  0;   10;      9;      0;       -1000;   17;          GPM; GEOPOTENTIAL HEIGHT
  0;   10;     10;     -1;           0;   14;      PASCALS; MIN PRESSURE REDUCED TO MSL
  0;   10;     11;     -1;           0;   14;      PASCALS; MAX PRESSURE REDUCED TO MSL
  0;   10;     31;      2; -1073741824;   31;       METERS; DIR OF NORTH POLE, DIST FROM EART
  0;   10;     32;      1;           0;   27;       METERS; SATELLITE DIST TO EARTH CENTER
  0;   10;     33;      1;           0;   27;       METERS; ALTITUDE (PLATFORM TO ELLIPSOID)
  0;   10;     50;      2;           0;   16;       METERS; STD. DEV. ALTITUDE
  0;   10;     51;      1;           0;   14;      PASCALS; PRESSURE REDUCED TO MSL
  0;   10;     52;      1;           0;   14;      PASCALS; ALTIMETER SETTING (QNH)
  0;   10;     60;      1;       -1024;   11;      PASCALS; PRESSURE CHANGE
  0;   10;     61;      1;        -500;   10;      PASCALS; 3 HOUR PRESSURE CHANGE
  0;   10;     62;      1;       -1000;   11;      PASCALS; 24 HOUR PRESSURE CHANGE
  0;   10;     63;      0;           0;    4;   CODE_TABLE; CHARACTERISTIC OF PRESSURE TENDEN
  0;   10;     64;      0;           0;    3;   CODE_TABLE; SIGMET CRUISING LEVEL
  0;   10;     70;      0;        -400;   16;       METERS; INDICATED AIRCRAFT ALTITUDE
  0;   10;     80;      2;       -9000;   15;      DEGREES; VIEWING ZENITH ANGLE
  0;   10;     81;      3;           0;   31;       METERS; ALTITUDE OF COG ABOVE REF ELLIPSO
  0;   10;     82;      3;      -65536;   17; METERS/SECOND; INSTANTANEOUS ALTITUDE RATE
  0;   10;     83;      2;           0;   26;       DEG**2; SQUARED OFF NADIR ANGLE OF THE SA
  0;   10;     84;      2;           0;   26;       DEG**2; SQUARED OFF NADIR ANGLE OF THE SA
  0;   10;     85;      3;     -131072;   18;       METERS; MEAN SEA SURFACE HEIGHT
  0;   10;     86;      3;     -131072;   18;       METERS; GEOID'S HEIGHT 
  0;   10;     87;      3;     -131072;   18;       METERS; OCEAN DEPTH/LAND ELEVATION
  0;   10;     88;      3;      -32768;   16;       METERS; TOTAL GEOCENTRIC OCEAN TIDE HEIGH
  0;   10;     89;      3;      -32768;   16;       METERS; TOTAL GEOCENTRIC OCEAN TIDE HEIGH
  0;   10;     90;      3;      -32768;   16;       METERS; LONG PERIOD TIDE HEIGHT 
  0;   10;     91;      3;      -32768;   16;       METERS; TIDAL LOADING HEIGHT
  0;   10;     92;      3;      -32768;   16;       METERS; SOLID EARTH TIDE HEIGHT
  0;   10;     93;      3;      -32768;   16;       METERS; GEOCENTRIC POLE TIDE HEIGHT 
  0;   10;     95;      0;           0;   16;       METERS; HEIGHT OF ATMOSPHERE USED 
  0;   10;     96;      3;     -131072;   18;       METERS; MEAN DYNAMIC TOPOGRAPHY 
  0;   10;     97;      3;     -131072;   18;       METERS; MEAN SEA SURFACE HEIGHT FROM ALTI
  0;   10;     98;      4;       -2000;   12;       METERS; LOADING TIDE HEIGHT GEOCENTRIC OC
  0;   10;     99;      4;       -2000;   12;       METERS; LOADING TIDE HEIGHT GEOCENTRIC OC
  0;   10;    100;      4;       -2000;   12;       METERS; NON-EQUILIBRIUM LONG PERIOD TIDE 
  0;   10;    101;      2;      -32768;   16;       DEG**2; SQUARED OFF NADIR ANGLE OF THE SA
  0;   10;    102;      3;      -32768;   16;       METERS; SEA SURFACE HEIGHT ANOMALY
  0;   10;    192;      0;        -400;   17;          GPM; GEOPOTENTIAL HEIGHT
  0;   10;    193;      0;        -400;   17;         GPDM; GEOPOTENTIAL HEIGHT
  0;   10;    194;      0;       -2000;   17;          GPM; DEPARTURE FROM ICAO STD ATMOSPHER
  0;   10;    195;      0;        -400;   17;           DM; GEOMETRIC HEIGHT
  0;   11;      1;      0;           0;    9; DEGREES_TRUE; WIND DIRECTION
  0;   11;      2;      1;           0;   12; METERS/SECOND; WIND SPEED
  0;   11;      3;      1;       -4096;   13; METERS/SECOND; U-COMPONENT
  0;   11;      4;      1;       -4096;   13; METERS/SECOND; V-COMPONENT
  0;   11;      5;      1;        -512;   10; PASCALS/SECOND; W-COMPONENT
  0;   11;      6;      2;       -4096;   13; METERS/SECOND; W-COMPONENT
  0;   11;     11;      0;           0;    9; DEGREES_TRUE; WIND DIRECTION AT 10 METERS
  0;   11;     12;      1;           0;   12; METERS/SECOND; WIND SPEED AT 10 METERS
  0;   11;     13;      0;           0;    9; DEGREES_TRUE; WIND DIRECTION AT 5 METERS
  0;   11;     14;      1;           0;   12; METERS/SECOND; WIND SPEED AT 5 METERS
  0;   11;     21;      9;      -65536;   17;   SECOND**-1; RELATIVE VORTICITY
  0;   11;     22;      9;      -65536;   17;   SECOND**-1; DIVERGENCE
  0;   11;     23;      2;      -65536;   17;  M**2/SECOND; VELOCITY POTENTIAL
  0;   11;     31;      0;           0;    4;   CODE_TABLE; DEGREE OF TURBULENCE
  0;   11;     32;      1;         -40;   16;       METERS; HEIGHT OF BASE OF TURBULENCE
  0;   11;     33;      1;         -40;   16;       METERS; HEIGHT OF TOP OF TURBULENCE
  0;   11;     34;      1;       -1024;   11; METERS/SECOND; VERTICAL GUST VELOCITY
  0;   11;     35;      2;       -8192;   14; METERS/SECOND**2VERTICAL; GUST ACCELERATION
  0;   11;     36;      1;           0;   10; METERS/SECOND; MAXIMUM DERIVED EQUIVALENT VERTIC
  0;   11;     41;      1;           0;   12; METERS/SECOND; MAX WIND SPEED (GUSTS)
  0;   11;     42;      1;           0;   12; METERS/SECOND; MAX WIND SPEED(10 MIN MEAN WIND)
  0;   11;     43;      0;           0;    9; DEGREES_TRUE; MAXIMUM WIND GUST DIRECTION
  0;   11;     44;      0;           0;    9; DEGREES_TRUE; SFC-5000FT MEAN LYR WIND DIRECTIO
  0;   11;     49;      0;           0;    9; DEGREES_TRUE; STD. DEV. OF WIND DIRECTION
  0;   11;     50;      1;           0;   12; METERS/SECOND; STD. DEV. HORIZ WIND SPEED
  0;   11;     51;      1;           0;    8; METERS/SECOND; STD DEV VERT WIND COMPONENT
  0;   11;     61;      1;           0;   12; METERS/SECOND; ABSOLUTE WIND SHEAR(1KM LAYER BEL
  0;   11;     62;      1;           0;   12; METERS/SECOND; ABSOLUTE WIND SHEAR(1KM LAYER ABO
  0;   11;    192;      1;       -1024;   11; METERS/SECOND; MEAN U-COMPONENT
  0;   11;    193;      1;       -1024;   11; METERS/SECOND; MEAN V-COMPONENT
  0;   11;    194;      1;        -128;    8; METERS/SECOND; MEAN W-COMPONENT
  0;   11;    195;      1;           0;    9; METERS/SECOND; STANDARD DEVIATION U
  0;   11;    196;      1;           0;    9; METERS/SECOND; STANDARD DEVIATION V
  0;   11;    197;      1;           0;    6; METERS/SECOND; STANDARD DEVIATION W
  0;   11;    198;      1;           0;   12; METERS/SECOND; WIND SPEED 10000FT (EXTRAPLOATED)
  0;   11;    199;      1;           0;   12; METERS/SECOND; WIND SPEED 20000FT (EXTRAPOLATED)
  0;   11;    200;      1;           0;   12; METERS/SECOND; INFLATED WIND SPEED (MOS)
  0;   11;    201;      1;           0;   12; METERS/SECOND; MEAN WIND SPEED PAST 12 HRS
  0;   11;    210;      1;           0;   12; METERS/SECOND; ROOT MEAN SQUARE VECTOR WIND ERRO
  0;   11;    221;      0;           0;    9; DEGREES_TRUE; MEAN WIND DIR 5000FT-10000FT
  0;   11;    222;      1;           0;   12; METERS/SECOND; MEAN WIND SPEED 5000FT-10000FT
  0;   11;    223;      1;           0;   12; METERS/SECOND; 10 METER EXTRAPOLATED WIND SPEED
  0;   11;    224;      1;           0;   12; METERS/SECOND; 20 METER EXTRAPOLATED WIND SPEED
  0;   12;      1;      1;           0;   12; DEGREES_KELVIN; TEMPERATURE/DRY BULB TEMPERATURE
  0;   12;      2;      1;           0;   12; DEGREES_KELVIN; WET BULB TEMPERATURE
  0;   12;      3;      1;           0;   12; DEGREES_KELVIN; DEW POINT TEMPERATURE
  0;   12;      4;      1;           0;   12; DEGREES_KELVIN; DRY BULB TEMPERATURE AT 2 METERS
  0;   12;      5;      1;           0;   12; DEGREES_KELVIN; WET BULB TEMPERATURE AT 2 METERS
  0;   12;      6;      1;           0;   12; DEGREES_KELVIN; DEW POINT TEMPERATURE AT 2 METERS
  0;   12;      7;      1;           0;   12; DEGREES_KELVIN; VIRTUAL TEMPERATURE
  0;   12;     11;      1;           0;   12; DEGREES_KELVIN; MAXIMUM TEMPERATURE
  0;   12;     12;      1;           0;   12; DEGREES_KELVIN; MINIMUM TEMPERATURE
  0;   12;     13;      1;           0;   12; DEGREES_KELVIN; GROUND MINIMUM TEMPERATURE PAST 1
  0;   12;     14;      1;           0;   12; DEGREES_KELVIN; MAXIMUM TEMPERATURE AT 2MTRS,PAST
  0;   12;     15;      1;           0;   12; DEGREES_KELVIN; MINIMUM TEMPERATURE AT 2MTRS,PAST
  0;   12;     16;      1;           0;   12; DEGREES_KELVIN; MAXIMUM TEMPERATURE AT 2MTRS,PAST
  0;   12;     17;      1;           0;   12; DEGREES_KELVIN; MINIMUM TEMPERATURE AT 2MTRS,PAST
  0;   12;     20;      2;       -2000;   12;          DEG; K/DAY       RADIATIVE HEATING PROFILE
  0;   12;     30;      1;           0;   12; DEGREES_KELVIN; SOIL TEMPERATURE
  0;   12;     40;      3;       -2048;   12; WATTS/METER**2; SENSIBLE HEAT FLUX
  0;   12;     51;      1;           0;   10; DEGREES_KELVIN; STANDARD DEVIATION TEMPERATURE
  0;   12;     52;      1;           0;   12; DEGREES_KELVIN; HIGHEST DAILY MEAN TEMPERATURE
  0;   12;     53;      1;           0;   12; DEGREES_KELVIN; LOWEST DAILY MEAN TEMPERATURE
  0;   12;     61;      1;           0;   12; DEGREES_KELVIN; SKIN TEMPERATURE
  0;   12;     62;      1;           0;   12; DEGREES_KELVIN; EQUIVALENT BLACK BODY TEMPERATURE
  0;   12;     63;      1;           0;   12; DEGREES_KELVIN; BRIGHTNESS TEMPERATURE
  0;   12;     65;      1;           0;   12; DEGREES_KELVIN; STANDARD DEVIATION BRIGHTNESS TEMPERATURE
  0;   12;    192;      0;           0;    6;   CODE_TABLE; PRECISION OF AIRCRAFT TEMPERATURE
  0;   12;    193;      1;           0;   12; DEGREES_KELVIN; TEMPERATURE (CITY)
  0;   12;    194;      1;           0;   12; DEGREES_KELVIN; MAXIMUM TEMPERATURE (CITY)
  0;   12;    195;      1;           0;   12; DEGREES_KELVIN; MINIMUM TEMPERATURE (CITY)
  0;   12;    200;      1;           0;   12; DEGREES_KELVIN; DAYTIME MAX TEMPERATURE
  0;   12;    201;      1;           0;   12; DEGREES_KELVIN; NIGHTTIME MIN TEMPERATURE (MOS)
  0;   13;      1;      5;           0;   14;        KG/KG; SPECIFIC HUMIDITY
  0;   13;      2;      5;           0;   14;        KG/KG; MIXING RATIO
  0;   13;      3;      0;           0;    7;            %; RELATIVE HUMIDITY
  0;   13;      4;      1;           0;   10;      PASCALS; VAPOR PRESSURE
  0;   13;      5;      3;           0;    7;  KG/METER**3; VAPOR DENSITY
  0;   13;      6;      1;         -40;   16;       METERS; MIXING HEIGHTS
  0;   13;     11;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION/TOTAL WATER E
  0;   13;     12;      2;          -2;   12;       METERS; DEPTH OF FRESH SNOW
  0;   13;     13;      2;          -2;   16;       METERS; TOTAL SNOW DEPTH
  0;   13;     14;      4;           0;   12; KG/METER**2/SEC; RAINFALL/WATER EQUIV OF SNOW(AVG
  0;   13;     15;      7;           0;   12; METERS/SECOND; SNOWFALL (AVERAGED RATE)
  0;   13;     16;      0;           0;    7;  KG/METER**2; PRECIPITABLE WATER
  0;   13;     19;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION PAST 1 HOUR
  0;   13;     20;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION PAST 3 HOURS
  0;   13;     21;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION PAST 6 HOURS
  0;   13;     22;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION PAST 12 HOURS
  0;   13;     23;      1;          -1;   14;  KG/METER**2; TOTAL PRECIPITATION PAST 24 HOURS
  0;   13;     31;      0;           0;    7;  KG/METER**2; EVAPOTRANSPIRATION
  0;   13;     32;      1;           0;    8;  KG/METER**2; EVAP/EVAPOTRANSPIRATION
  0;   13;     40;      3;       -2048;   12; WATTS/METER**2; LATENT HEAT FLUX
  0;   13;     41;      0;           0;    4;   CODE_TABLE; PASQUELL-GIFFORD STAB
  0;   13;     42;      0;         -20;    6; DEGREES_KELVIN; PARCEL LIFTED INDEX (TO 500 HPA)
  0;   13;     43;      0;         -20;    6; DEGREES_KELVIN; BEST LIFTED INDEX (TO 500 HPA)
  0;   13;     51;      0;           0;    4;   CODE_TABLE; FREQ GRP, PRECIPITATION
  0;   13;     52;      1;          -1;   14;          KG/; M**2        HIGHEST DAILY AMT OF PRECIPITATIO
  0;   13;     55;      4;           0;    8;    KG/M**2/S; INTENSITY OF PRECIPITATION
  0;   13;    192;      0;           0;    6;   CODE_TABLE; PRECIPITABLE WATER QUALITY
  0;   13;    193;      4;          -1;   14;     KGM/M**2; 24 HR PRECIPITATION (CITY)
  0;   13;    194;      0;           0;    3;   CODE_TABLE; INDIC INCLUSION/OMISSION OF PRECI
  0;   14;      1;      3;       -2048;   12; JOULES/METER**2; LONGWAVE RADIATION. INTEGRATED 24
  0;   14;      2;      3;       -2048;   12; JOULES/METER**2; LONGWAVE RAD. INTEGRATED SPEC.PER
  0;   14;      3;      3;       -2048;   12; JOULES/METER**2; SHORTWAVE RAD. INTEGRATED 24 HOUR
  0;   14;      4;      3;       -2048;   12; JOULES/METER**2; SHORTWAVE RAD. INTEGRATED SPEC PE
  0;   14;     11;      3;       -2048;   12; JOULES/METER**2; NET LONGWAVE RAD. INTEG. 24 HOURS
  0;   14;     12;      3;       -2048;   12; JOULES/METER**2; NET LONGWAVE RAD. INT SPEC PERIOD
  0;   14;     13;      3;       -2048;   12; JOULES/METER**2; NET SHORTWAVE RAD. INTEG 24 HOURS
  0;   14;     14;      3;       -2048;   12; JOULES/METER**2; NET SHORTWAVE RAD. INTEG SPEC PER
  0;   14;     15;      4;      -16384;   15; JOULES/METER**2; NET RAD INTEGRATED OVER 24 HOURS
  0;   14;     16;      4;      -16384;   15; JOULES/METER**2; NET RADIATION INTEG OVR PD SPECIF
  0;   14;     17;      3;       -2048;   12; WATTS/METER**2; INSTANTANEOUS LONG WAVE RADIATION
  0;   14;     18;      3;       -2048;   12; WATTS/METER**2; INSTANTANEOUS SHORT WAVE RADIATIO
  0;   14;     19;      0;           0;    7;            %; SURFACE ALBEDO
  0;   14;     20;      4;           0;   15; JOULES/METER**2; GLOBAL SOLAR RAD INTEG OVER  24 H
  0;   14;     21;      4;           0;   15; JOULES/METER**2; GLOBAL RADIATION INTEG OVER PD SP
  0;   14;     22;      4;           0;   15; JOULES/METER**2; DIFFUSE SOLAR RAD INTEG OVER  24
  0;   14;     23;      4;           0;   15; JOULES/METER**2; DIFFUSE SOLAR RAD INTEG OVER PD S
  0;   14;     24;      4;           0;   15; JOULES/METER**2; DIRECT SOLAR RAD INTEG OVER  24 H
  0;   14;     25;      4;           0;   15; JOULES/METER**2; DIRECT SOLAR RAD INTEG OVER PD SP
  0;   14;     31;      0;           0;   11;      MINUTES; TOTAL SUNSHINE
  0;   14;     32;      0;           0;   10;        HOURS; TOTAL SUNSHINE
  0;   14;     33;      0;           0;    9;            %; TOTAL SUNSHINE(PERCENTAGE)
  0;   14;     41;      0;           0;    7;            %; SHORT WAVE ALBEDO
  0;   14;     42;      0;           0;    7;            %; BI-DIRECTIONAL REFLECTANCE
  0;   14;    200;      0;           0;    7;            %; PERCENT OF POSSIBLE SUNSHINE
  0;   15;      1;      0;           0;   10;       DOBSON; UNITS    OZONE
  0;   15;      2;      2;           0;   10;      NUMERIC; AIR-MASS (SLANT PATH AT 22KM)
  0;   15;     11;      3;       14000;   12;     LOG/M**2; LOG_E OF INTEGRATED ELECTRON DENS
  0;   19;      1;      0;           0;    6;   CODE_TABLE; TYPE OF SYNOPTIC FEATURE
  0;   19;      2;      2;           0;   12;       METERS; EFFECTIVE RADIUS OF FEATURE
  0;   19;      3;      0;           0;    8; METERS/SECOND; WIND SPEED THRESHOLD
  0;   19;      4;      2;           0;   12;       METERS; EFF RAD OF FEAT W/RESP TO WINDS A
  0;   19;      5;      0;           0;    9;          DEG; TRUE        DIRECTION OF MOTION OF FEATURE
  0;   19;      6;      2;           0;   14; METERS/SECOND; SPEED OF MOTION OF FEATURE
  0;   19;      7;      3;           0;   12;       METERS; EFFECTIVE RADIUS OF FEATURE
  0;   19;      8;      0;           0;    3;   CODE_TABLE; VERTICAL EXTENT OF CIRCULATION
  0;   19;      9;      3;           0;   12;       METERS; EFF. RAD. W/RESPECT TO FFF ABV TH
  0;   20;      1;      1;           0;   13;       METERS; HORIZONTAL VISIBILITY
  0;   20;      2;      1;           0;    7;       METERS; VERTICAL VISIBILITY
  0;   20;      3;      0;           0;    9;   CODE_TABLE; PRESENT WEATHER
  0;   20;      4;      0;           0;    5;   CODE_TABLE; PAST WEATHER (1)
  0;   20;      5;      0;           0;    5;   CODE_TABLE; PAST WEATHER (2)
  0;   20;      9;      1;         -40;   11;       METERS; CEILING
  0;   20;     10;      0;           0;    7;            %; CLOUD COVER (TOTAL)
  0;   20;     11;      0;           0;    4;   CODE_TABLE; CLOUD AMOUNT
  0;   20;     12;      0;           0;    6;   CODE_TABLE; CLOUD TYPE
  0;   20;     13;      1;         -40;   11;       METERS; HEIGHT OF BASE OF CLOUD
  0;   20;     14;      1;         -40;   11;       METERS; HEIGHT OF TOP OF CLOUD
  0;   20;     15;      1;           0;   14;      PASCALS; PRESSURE AT THE BASE OF CLOUD
  0;   20;     16;      1;           0;   14;      PASCALS; PRESSURE AT THE TOP OF CLOUD
  0;   20;     17;      0;           0;    4;   CODE_TABLE; CLOUD TOP DESCRIPTION
  0;   20;     18;      1;          40;   11;       METERS; LOWEST HGT OF CLD TOP
  0;   20;     19;      1;          40;   11;       METERS; HIGHEST HGT OF CLD TOP
  0;   20;     20;      0;           0;    4; CODE_TABLE(02001LOW; CLOUD AMOUNT
  0;   20;     21;      0;           0;    4; CODE_TABLE(02001MIDDLE; CLOUD AMOUNT
  0;   20;     22;      0;           0;    4; CODE_TABLE(02001HIGH; CLOUD AMOUNT
  0;   20;     23;      0;           0;    7;            %; SATELLITE SENSED EFF CLOUD AMOUNT
  0;   20;     31;      2;           0;    7;       METERS; ICE DEPOSIT (THICKNESS)
  0;   20;     32;      0;           0;    3;   CODE_TABLE; RATE OF ICE ACCRETION
  0;   20;     33;      0;           0;    4;   FLAG_TABLE; CAUSE OF ICE ACCRETION
  0;   20;     34;      0;           0;    5;   CODE_TABLE; SEA ICE CONCENTRATION
  0;   20;     35;      0;           0;    4;   CODE_TABLE; AMOUNT AND TYPE OF ICE
  0;   20;     36;      0;           0;    5;   CODE_TABLE; ICE SITUATION
  0;   20;     37;      0;           0;    5;   CODE_TABLE; ICE DEVELOPMENT
  0;   20;     38;      0;           0;   12; DEGREES_TRUE; BEARING OF ICE EDGE
  0;   20;     39;      1;           0;   13;       METERS; ICE DISTANCE
  0;   20;     41;      0;           0;    4;   CODE_TABLE; AIRFRAME ICING
  0;   20;     51;      0;           0;    7;            %; AMOUNT OF LOW CLOUDS
  0;   20;     52;      0;           0;    7;            %; AMOUNT OF MIDDLE CLOUDS
  0;   20;     53;      0;           0;    7;            %; AMOUNT OF HIGH CLOUDS
  0;   20;     61;      0;           0;   12;       METERS; RUNWAY VISUAL RANGE (RVR)
  0;   20;     62;      0;           0;    5;   CODE_TABLE; STATE OF GROUND(W /WO SNOW)
  0;   20;     63;      0;           0;   10;   CODE_TABLE; SPECIAL PHENOMENA
  0;   20;    192;      0;           0;    7;   CODE_TABLE; VISIBILITY TOWARDS SEA(WMO TABLE
  0;   20;    200;      0;           0;    7;            %; MEAN CLD COVER (OPAQUE) PAST 12 H
  0;   21;      1;      0;         -64;    7;           DB; HORIZONTAL REFLECTIVITY
  0;   21;      2;      0;         -64;    7;           DB; VERTICAL REFLECTIVITY
  0;   21;      3;      1;          -5;    7;           DB; DIFFERENTIAL REFLECTIVITY
  0;   21;      5;      0;         -65;    6;           DB; LINEAR DEPOLARIZATION RATIO
  0;   21;      6;      0;         -65;    6;           DB; CIRCULAR DEPOLARIZATION RATIO
  0;   21;     11;      0;        -128;    8; METERS/SECOND; DOPPLER MEAN VELOCITY IN X DIRECT
  0;   21;     12;      0;        -128;    8; METERS/SECOND; DOPPLER MEAN VELOCITY IN Y DIRECT
  0;   21;     13;      0;        -128;    8; METERS/SECOND; DOPPLER MEAN VELOCITY IN Z DIRECT
  0;   21;     14;      1;       -4096;   13; METERS/SECOND; DOPPLER MEAN VELOCITY (RADIAL)
  0;   21;     17;      1;           0;    8; METERS/SECOND; DOPPLER VELOCITY SPECTRAL WIDTH
  0;   21;     21;      3;           0;    4;       METERS; ECHO TOPS
  0;   21;     30;      0;         -32;    8;           DB; SIGNAL TO NOISE RATIO
  0;   21;     31;      0;           0;    7; KILOGRAMS/METER*VERT.; INTEGRATED LIQ. WATER CONTE
  0;   21;     36;      7;           0;   12; METERS/SECOND; RADAR RAINFALL INTENSITY
  0;   21;     41;      2;           0;    8;       METERS; BRIGHT BAND HEIGHT
  0;   21;     51;      0;        -256;    8;           DB; SIGNAL POWER ABOVE 1MW
  0;   21;     62;      2;       -5000;   13;     DECIBELS; BACKSCATTER
  0;   21;     63;      0;           0;    7;            %; NOISE FIGURE
  0;   21;     64;      0;           0;   10;      NUMERIC; CLUTTER NOISE ESTIMATE
  0;   21;     65;      0;        -127;    8;      NUMERIC; MISSING PACKET COUNTER
  0;   21;     66;      0;           0;   12;   FLAG_TABLE; WAVE SCATTEROMETER PRODUCT CONFID
  0;   21;     67;      0;           0;   12;   FLAG_TABLE; WIND SCATTEROMETER PRODUCT CONFID
  0;   21;     68;      0;           0;    8;   FLAG_TABLE; RADAR ALTIMETER PRODUCT CONFIDENC
  0;   21;     69;      0;           0;    7;   FLAG_TABLE; ATSR SEA SFC TEMP QUAL ANALYSIS T
  0;   21;     70;      0;           0;   15;   FLAG_TABLE; REPROCESSED WIND SCATTEROMETER PR
  0;   21;     71;      0;           0;   16;      NUMERIC; PEAKINESS
  0;   21;     72;      0;           0;    4;   FLAG_TABLE; SATELLITE ALTIMETER CALIBRATION S
  0;   21;     73;      0;           0;    9;   FLAG_TABLE; SATELLITE ALTIMETER INSTRUMENT MO
  0;   21;     74;      2;        -512;   10; DEGREES_KELVIN; MULTI/SINGLE VIEW DIFFERENCE
  0;   21;     75;      0;           0;    8;      NUMERIC; SPECTRAL INTENSITY
  0;   21;     76;      0;           0;    3;   CODE_TABLE; REPRESENTATION OF INTENSITIES
  0;   21;     77;      3;           0;   14;       METERS; ALTITUDE CORRECTION (IONOSPHERE)
  0;   21;     78;      3;           0;    9;       METERS; ALTITUDE CORRECTION (DRY TROPOSPH
  0;   21;     79;      3;        2000;   10;       METERS; ALTITUDE CORRECTION (WET TROPOSPH
  0;   21;     80;      3;           0;   11;       METERS; ALTITUDE CORRECTION (CALIB. CONST
  0;   21;     81;      3;           0;   10;       METERS; OPEN LOOP CORRECTION (HGT-TIME LO
  0;   21;     82;      3;       -3000;   14;     DECIBELS; OPEN LOOP CORRECTION (AUTO GAIN C
  0;   21;     83;      0;           0;    7;            %; AMBIGUITY REMOVAL CONFIDENCE
  0;   21;     84;      0;           0;    3;   CODE_TABLE; ATSR SEA SFC TEMP QUALITY SUMMARY
  0;   21;     85;      0;           0;    4;      NUMERIC; ATSR SEA SFC TEMP ACROSS TRACK BA
  0;   21;    101;      0;           0;    3;      NUMERIC; NUMBER OF VECTOR AMBIGUITIES
  0;   21;    102;      0;           0;    3;      NUMERIC; INDEX OF SELECTED WIND VECTOR
  0;   21;    104;      3;      -30000;   15;      NUMERIC; WIND LIKELIHOOD
  0;   21;    109;      0;           0;   17;   FLAG_TABLE; WIND VECTOR CELL QUALITY
  0;   21;    120;      3;           0;   10;      NUMERIC; PROBABILITY OF RAIN
  0;   21;    121;      0;           0;    8;      NUMERIC; SEAWINDS NOF RAIN INDEX
  0;   21;    192;      0;           0;    7;           DB; SPECTRAL PEAK POWER 0TH MOMENT
  0;   21;    193;      1;       -4096;   13; METERS/SECOND; SPECTRAL PEAK POWER 1ST MOMENT
  0;   21;    194;      1;           0;    8; METERS/SECOND; SPECTRAL PEAK POWER 2ND MOMENT
  0;   22;      1;      0;           0;    9; DEGREES_TRUE; DIRECTION OF WAVES
  0;   22;      2;      0;           0;    9; DEGREES_TRUE; DIRECTION OF WIND WAVES
  0;   22;      3;      0;           0;    9; DEGREES_TRUE; DIRECTION OF SWELL WAVES
  0;   22;      4;      0;           0;    9; DEGREES_TRUE; DIRECTION OF CURRENT WAVES
  0;   22;     11;      0;           0;    6;      SECONDS; PERIOD OF WAVES
  0;   22;     12;      0;           0;    6;      SECONDS; PERIOD OF WIND WAVES
  0;   22;     13;      0;           0;    6;      SECONDS; PERIOD OF SWELL WAVES
  0;   22;     21;      1;           0;   10;       METERS; HEIGHT OF WAVES
  0;   22;     22;      1;           0;   10;       METERS; HEIGHT OF WIND WAVES
  0;   22;     23;      1;           0;   10;       METERS; HEIGHT OF SWELL WAVES
  0;   22;     25;      2;           0;   10;       METERS; STANDARD DEVIATION WAVE
  0;   22;     26;      2;           0;   10;       METERS; STANDARD DEVIATION SIG WAVE HEIGH
  0;   22;     31;      2;           0;   13; METERS/SECOND; SPEED OF CURRENT
  0;   22;     37;      3;      -10000;   15;       METERS; TIDAL ELEV WITH RESPECT TO LAND D
  0;   22;     38;      3;      -10000;   15;       METERS; TIDAL ELEV WITH RESPECT TO CHART
  0;   22;     39;      3;       -5000;   12;       METERS; MET RESIDUAL TIDAL ELEV (SURGE OR
  0;   22;     41;      1;           0;   12; DEGREES_KELVIN; SEA SFC TEM (15 DAY RUNNING MEAN)
  0;   22;     42;      1;           0;   12; DEGREES_KELVIN; SEA TEMPERATURE
  0;   22;     43;      2;           0;   15; DEGREES_KELVIN; SEA TEMPERATURE
  0;   22;     44;      1;           0;   14; METERS/SECOND; SOUND VELOCITY
  0;   22;     49;      2;           0;   15; DEGREES_KELVIN: SEA SURFACE TEMPERATURE
  0;   22;     50;      2;           0;    8;            K; STD DEV SEA-SURFACE TEMPERATURE
  0;   22;     61;      0;           0;    4;   CODE_TABLE; STATE OF SEA
  0;   22;     62;      2;           0;   12;   PARTS/1000; SALINITY
  0;   22;     63;      0;           0;   14;       METERS; TOTAL WATER DEPTH
  0;   22;    105;      1;           0;    6; DEGREES_TRUE; DIRECTION OF WAVES
  0;   22;    143;      2;        2650;   13; DEGREES_KELVIN; SEA TEMPERATURE
  0;   22;    192;      0;           0;    4;   CODE_TABLE; TIDE INDICATOR
  0;   22;    193;      1;           0;   10;       METERS; ABS VALUE DEPT OF TIDE FROM PRED
  0;   22;    194;      3;        -305;   12;       METERS; DEPT OF TIDE FROM MEAN LOWER LOW
  0;   23;      1;      0;           0;    3;   CODE_TABLE; ACCIDENT EARLY NOTIFICATION ART.A
  0;   23;      2;      0;           0;    5;   CODE_TABLE; ACTIVITY OR FACILITY INVOLVED IN
  0;   23;      3;      0;           0;    3;   CODE_TABLE; TYPE OF RELEASE
  0;   23;      4;      0;           0;    3;   CODE_TABLE; COUNTERMEASURES TAKEN NR BORDER
  0;   23;      5;      0;           0;    2;   CODE_TABLE; CAUSE  OF INCIDENT
  0;   23;      6;      0;           0;    3;   CODE_TABLE; INCIDENT SITUATION
  0;   23;      7;      0;           0;    3;   CODE_TABLE; CHARACTERISTIC OF RELEASE
  0;   23;      8;      0;           0;    2;   CODE_TABLE; STATE OF CURRENT RELEASE
  0;   23;      9;      0;           0;    2;   CODE_TABLE; STATE OF EXPECTED RELEASE
  0;   23;     16;      0;           0;    2;   CODE_TABLE; POSS. OF SIG CHEM.TOXIC HEALTH EF
  0;   23;     17;      6;           0;   20; METER**3/SECOND; FLOW DISCHARGE OF MAJ. RECIPIENT
  0;   23;     18;      0;           0;    3;   CODE_TABLE; RELEASE BEHAVIOR OVER TIME
  0;   23;     19;      0;      -15000;   17;       METERS; ACTUAL RELEASE HEIGHT
  0;   23;     21;      0;      -15000;   17;       METERS; EFFECTIVE RELEASE HEIGHT
  0;   23;     22;      0;           0;   24;       METERS; DIST. OF REL PT OR SITE OF INCIDE
  0;   23;     23;      1;           0;   12; METERS/SECOND; MAIN TRANSPORT SPEED IN ATMOSPHER
  0;   23;     24;      2;           0;   13; METERS/SECOND; MAIN TRANSPORT SPEED IN WATER
  0;   23;     25;      2;           0;   13; METERS/SECOND; MAIN TRANSPORT SPEED IN GROUND WA
  0;   23;     27;      0;           0;    9; DEGREES_TRUE; MAIN TRANSPORT DIR IN ATMOSPHERE
  0;   23;     28;      0;           0;    9; DEGREES_TRUE; MAIN TRANSPORT DIR IN WATER
  0;   23;     29;      0;           0;    9; DEGREES_TRUE; MAIN TRANSPORT DIR IN GROUND WATE
  0;   23;     31;      0;           0;    2;   CODE_TABLE; POSS PLUME/PRECIP ENCOUNTER
  0;   23;     32;      0;           0;    2;   CODE_TABLE; PLUME ENCOUNTER DIR/SPD CHANGE
  0;   24;      1;      1;           0;   28;           BQ; EST. OF RADIOACTIVITY REL.TO SPEC
  0;   24;      2;      1;           0;   28;           BQ; EST MAXIMUM POTENTIAL RELEASE
  0;   24;      3;      0;           0;    5;   CODE_TABLE; COMPOSITION OF RELEASE
  0;   24;      4;      0;           0;   16;    CCITT_IA5; ELEMENT NAME
  0;   24;      5;      0;           0;    9;      NUMERIC; ISOTOPE MASS
  0;   24;     11;      2;           0;   32;          MSV; DOSE
  0;   24;     12;      2;           0;   32;          MSV; TRAJ DOSE(DEF LOC & EXP TIME OF A
  0;   24;     13;      2;           0;   32;          MSV; GAMMA DOSE IN AIR ALG MAIN TRAN P
  0;   24;     21;      2;           0;   32;  BQ/METER**3; AIR CONC.(NAMED ISOTOPE INC GROSS
  0;   24;     22;      2;           0;   32;         BQ/L; CONC IN PRECIP(OF NAMED ISOTOPE T
  0;   25;      1;      1;           0;    6;       METERS; RANGE GATE LENGTH
  0;   25;      2;      0;           0;    4;      NUMERIC; NR OF GATES AVERAGED
  0;   25;      3;      0;           0;    8;      NUMERIC; NR. OF INTEGRATED PULSES
  0;   25;      4;      0;           0;    2;   CODE_TABLE; ECHO PROCESSING
  0;   25;      5;      0;           0;    2;   CODE_TABLE; ECHO INTEGRATION
  0;   25;      6;      0;           0;    3;   CODE_TABLE; Z TO R CONVERSION
  0;   25;      7;      0;           0;   12;      NUMERIC; Z TO R CONVERSION FACTOR
  0;   25;      8;      2;           0;    9;      NUMERIC; Z TO R CONVERSION EXPONENT
  0;   25;      9;      0;           0;    4;   FLAG_TABLE; CALIBRATION METHOD
  0;   25;     10;      0;           0;    4;   CODE_TABLE; CLUTTER TREATMENT
  0;   25;     11;      0;           0;    2;   CODE_TABLE; GND. OCCULTATION CORR. (SCREENING
  0;   25;     12;      0;           0;    2;   CODE_TABLE; RANGE ATTENUATION CORRECTION
  0;   25;     13;      0;           0;    2;   FLAG_TABLE; BRIGHT BAND CORRECTION
  0;   25;     15;      0;           0;    2;   FLAG_TABLE; RADOME ATTENUATION CORRECTION
  0;   25;     16;      5;           0;    6;     DB/METER; CLEAR AIR ATTENUATION CORRECTION
  0;   25;     17;      0;           0;    2;   FLAG_TABLE; PRECIPITATION ATTENUATION CORRECT
  0;   25;     18;      7;           0;    6;      NUMERIC; A TO Z LAW FOR ATTENUATION FACTOR
  0;   25;     19;      2;           0;    7;      NUMERIC; A TO Z LAW FOR ATTENUATION EXPONE
  0;   25;     20;      0;           0;    2;   CODE_TABLE; MEAN SPEED ESTIMATION
  0;   25;     21;      0;           0;    8;   FLAG_TABLE; WIND COMPUTATION ENHANCEMENT
  0;   25;     30;      0;           0;    2;   CODE_TABLE; SST USAGE
  0;   25;     31;      0;           0;    2;   CODE_TABLE; 15 DAY SST AVAILABILITY
  0;   25;     32;      0;           0;    2;   CODE_TABLE; NOAA WIND PROFILER HIGH/LOW MODE
  0;   25;     33;      0;           0;    2;   CODE_TABLE; NOAA WIND PROFILER SUBMODE
  0;   25;     34;      0;           0;    4;   CODE_TABLE; NOAA WIND PROFILER Q/C TEST RESUL
  0;   25;     35;      0;           0;    3;   CODE_TABLE; FIRST GUESS ADJUSTMENT
  0;   25;     36;      3;       -5000;   14;      NUMERIC; NSTAR AVERAGE VALUE
  0;   25;     37;      0;           0;    2;   CODE_TABLE; HIRS-8 SFC AIR TEMP
  0;   25;     38;      0;           0;    3;   CODE_TABLE; TOVS FILTER FLAGS
  0;   25;     71;      0;           0;    5;      NUMERIC; FRAME COUNT
  0;   25;     81;      3;           0;   17;      DEGREES; INCIDENCE ANGLE
  0;   25;     82;      3;           0;   19;      DEGREES; AZIMUTH ANGLE
  0;   25;    202;      0;           0;    4;   FLAG_TABLE; TEMPERATURE CHANNEL SELECTION FLA
  0;   25;    204;      0;           0;    8;   FLAG_TABLE; MATCHUP QUALITY TEST FLAGS
  0;   25;    205;      0;           0;    8;   FLAG_TABLE; RETRIEVAL/DPI QUALITY TEST FLAGS
  0;   25;    209;      3;           0;   12; DECIMAL_HOURS; DPI TIME DIFFERENCE (READ AS MINU
  0;   25;    210;      3;           0;   19;       METERS; DPI DISTANCE
  0;   25;    211;      3;           0;   12; DECIMAL_HOURS; QUANTITATIVE RETRIEVAL TIME DIFFE
  0;   25;    212;      3;           0;   19;       METERS; QUANTITATIVE RETRIEVAL DISTANCE
  0;   26;      1;      1;           0;   12;         HOUR; PCPL TIME OF DAILY RDG IN UTC MAX
  0;   26;      2;      1;           0;   12;         HOUR; PCPL TIME OF DAILY RDG IN UTC MIN
  0;   26;     31;      2;  -107341824;   31;       METERS; DIST FM EARTH CENTER IN DIR NORTH
  0;   26;     32;      2;  -107341824;   31;       METERS; DIST FM EARTH CENTER IN DIR NORTH
  0;   26;     41;      5;  -107341824;   31; METERS/SECOND; VEL W/RESP EARTH CTR IN DIR NORTH
  0;   27;      1;      5;    -9000000;   25;      DEGREES; LATITUDE (HIGH ACCURACY)
  0;   27;      2;      2;       -9000;   15;      DEGREES; LATITUDE (COARSE ACCURACY)
  0;   27;      3;      2;       -9000;   15;      DEGREES; ALTERNATE LATITUDE
  0;   27;     20;      0;           0;   16;      NUMERIC; SATELLITE LOCATION COUNTER
  0;   27;     21;      0;           0;   16;      NUMERIC; SATELLITE SUB-LOCATION DIMENSIONS
  0;   27;     31;      2;  -107341824;   31;       METERS; DIST FM EARTH CENTER IN DIR 0 DEG
  0;   27;     41;      5;  -107341824;   31; METERS/SECOND; VEL W/RESP EARTH CTR N DIR 0 DEG
  0;   28;      1;      5;   -18000000;   26;      DEGREES; LONGITUDE (HIGH ACCURACY)
  0;   28;      2;      2;      -18000;   16;      DEGREES; LONGITUDE (COARSE ACCURACY)
  0;   28;      3;      2;      -18000;   16;      DEGREES; ALTERNATE LONGITUDE
  0;   28;     31;      2;  -107341824;   31;       METERS; DIST FMEARTH CENTER IN DIR 90 DEG
  0;   28;     41;      5;  -107341824;   31; METERS/SECOND; VEL W/RESP EARTH CTR IN DIR 90 DE
  0;   29;      1;      0;           0;    3;   CODE_TABLE; PROJECTION TYPE
  0;   29;      2;      0;           0;    3;   CODE_TABLE; COORDINATE GRID TYPE
  0;   30;      1;      0;           0;    4;      NUMERIC; PIXEL VALUE (4 BITS)
  0;   30;     21;      0;           0;   12;      NUMERIC; NUMBER OF PIXELS PER ROW
  0;   30;     22;      0;           0;   12;      NUMERIC; NUMBER OF PIXELS PER COLUMN
  0;   30;     31;      0;           0;    4;   CODE_TABLE; PICTURE TYPE
  0;   30;     32;      0;           0;   16;   FLAG_TABLE; COMBINED PICTURE
  0;   31;      0;      0;           0;    1;   FLAG_TABLE; DELAYED REPLICATION SWITCH
  0;   31;      1;      0;           0;    8;      NUMERIC; DELAYED DESCRIPTOR REPLICATION FA
  0;   31;      2;      0;           0;   16;      NUMERIC; EXT DELAYED DESCRIPTOR REPLICAT.
  0;   31;     11;      0;           0;    8;      NUMERIC; DELAYED DESC. & DATA REPITIT. FAC
  0;   31;     12;      0;           0;   16;      NUMERIC; EXT DELAYED DESC. & DATA REPITIT.
  0;   31;     21;      0;           0;    6;   CODE_TABLE; ASSOCIATED FIELD SIGNIFICANCE
  0;   31;     31;      0;           0;    1;   FLAG_TABLE; DATA PRESENT INDICATOR
  0;   31;    192;      0;           0;    9;   CODE_TABLE; NOAA WIND PROFILER HIGH/LOW MODE
  0;   31;    193;      0;           0;    2;   CODE_TABLE; NOAA WIND PROFILER SUBMODE
  0;   31;    194;      0;           0;    4;   CODE_TABLE; NOAA WIND PROFILER Q/C TEST RESUL
  0;   33;      2;      0;           0;    2;   CODE_TABLE; QUALITY INFORMATION
  0;   33;      3;      0;           0;    3;   CODE_TABLE; QUALITY INFORMATION
  0;   33;      4;      0;           0;    7;            %; % CONFIDENCE
  0;   50;      1;      0;           0;   17;      NUMERIC; REPORT SEQUENCE NUMBER
  0;   50;     20;      0;           0;    4;   CODE_TABLE; DATA QUALITY INDICATOR
  0;   55;      6;      0;           0;   10;   CODE_TABLE; NMC REPORT TYPE
  0;   58;      1;      0;           0;   48;    CCITT_IA5; BULLETIN HEADING
  0;   58;      2;      0;           0;   80;    CCITT_IA5; AIRCRAFT TYPE
  0;   58;      3;      0;        -400;   17;          GPM; ICING BASE
  0;   58;      4;      0;        -400;   17;          GPM; ICING TOP
  0;   58;      5;      0;           0;  224;    CCITT_IA5; COMPLETE BULLETIN HEADER
  0;   60;      1;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .01 INCH PAS
  0;   60;      2;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .01 INCH PAS
  0;   60;      3;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .01 INCH PAS
  0;   60;      4;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .10 INCH PAS
  0;   60;      5;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .10 INCH PAS
  0;   60;      6;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .10 INCH PAS
  0;   60;      7;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .25 INCH PAS
  0;   60;      8;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .25 INCH PAS
  0;   60;      9;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .25 INCH PAS
  0;   60;     10;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .50 INCH PAS
  0;   60;     11;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .50 INCH PAS
  0;   60;     12;      0;           0;    7;            %; PROB. OF LIQ PCPN GE .50 INCH PAS
  0;   60;     13;      0;           0;    7;            %; PROB. OF LIQ PCP GE 1.00 INCH PAS
  0;   60;     14;      0;           0;    7;            %; PROB. OF LIQ PCP GE 1.00 INCH PAS
  0;   60;     15;      0;           0;    7;            %; PROB. OF LIQ PCP GE 1.00 INCH PAS
  0;   60;     16;      0;           0;    7;            %; PROB. OF LIQ PCP GE 2.00 INCH PAS
  0;   60;     17;      0;           0;    7;            %; PROB. OF LIQ PCP GE 2.00 INCH PAS
  0;   60;     18;      0;           0;    7;            %; REL FRQ GE .01 LQ EQV PCP PAST 12
  0;   60;     19;      0;           0;    7;            %; REL FRQ GE .01 LQ EQV PCP PAST 24
  0;   60;     20;      0;           0;    7;            %; COND PROB PCP TYPE FREEZING
  0;   60;     21;      0;           0;    7;            %; COND PROB PCP TYPE SNOW
  0;   60;     22;      0;           0;    7;            %; COND PROB PCP TYPE LIQUID
  0;   60;     23;      0;           0;    7;            %; COND PROB PCP TYPE DRIZZLE
  0;   60;     24;      0;           0;    7;            %; COND PROB PCP TYPE CONTINUOUS
  0;   60;     25;      0;           0;    7;            %; COND PROB PCP TYPE SHOWERS
  0;   60;     26;      0;           0;    7;            %; PROB SNOW AMT GE TRACE PAST 6HRS
  0;   60;     27;      0;           0;    7;            %; PROB SNOW AMT GE TRACE PAST 12HRS
  0;   60;     28;      0;           0;    7;            %; PROB SNOW AMT GE TRACE PAST 24HRS
  0;   60;     29;      0;           0;    7;            %; PROB SNOW AMT GE 2.0IN PAST 6HRS
  0;   60;     30;      0;           0;    7;            %; PROB SNOW AMT GE 2.0IN PAST 12HRS
  0;   60;     31;      0;           0;    7;            %; PROB SNOW AMT GE 2.0IN PAST 24HRS
  0;   60;     32;      0;           0;    7;            %; PROB SNOW AMT GE 4.0IN PAST 12HRS
  0;   60;     33;      0;           0;    7;            %; PROB SNOW AMT GE 4.0IN PAST 24HRS
  0;   60;     34;      0;           0;    7;            %; PROB SNOW AMT GE 6.0IN PAST 12HRS
  0;   60;     35;      0;           0;    7;            %; PROB SNOW AMT GE 6.0IN PAST 24HRS
  0;   60;     36;      0;           0;    7;            %; COND PROB SNOW PAST 12 HRS
  0;   60;     37;      0;           0;    7;            %; COND REL FRQ PROB SNOW PAST 12 HR
  0;   60;     38;      0;           0;    7;            %; PROB OPAQUE SKY COVER  CLEAR
  0;   60;     39;      0;           0;    7;            %; PROB OPAQUE SKY COVER  SCATTERED
  0;   60;     40;      0;           0;    7;            %; PROB OPAQUE SKY COVER  BROKEN
  0;   60;     41;      0;           0;    7;            %; PROB OPAQUE SKY COVER  OVERCAST
  0;   60;     42;      0;           0;    7;            %; PROB CIG HGT < 200 FT
  0;   60;     43;      0;           0;    7;            %; PROB CIG HGT 200-400 FT
  0;   60;     44;      0;           0;    7;            %; PROB CIG HGT 500-900 FT
  0;   60;     45;      0;           0;    7;            %; PROB CIG HGT 1000-3000 FT
  0;   60;     46;      0;           0;    7;            %; PROB CIG HGT 3100-6500 FT
  0;   60;     47;      0;           0;    7;            %; PROB CIG HGT 6600-12000 FT
  0;   60;     48;      0;           0;    7;            %; PROB CIG HGT GT 12000 FT
  0;   60;     49;      0;           0;    7;            %; PROB VSBY < 0/2 MILES
  0;   60;     50;      0;           0;    7;            %; PROB VSBY < 0/2 - 7/8 MILES
  0;   60;     51;      0;           0;    7;            %; PROB VSBY < 0 - 2 3/4 MILES
  0;   60;     52;      0;           0;    7;            %; PROB VSBY < 3 - 5 MILES
  0;   60;     53;      0;           0;    7;            %; PROB VSBY > 5   MILES
  0;   60;     54;      0;           0;    7;            %; PROB OBS TO VISION  BLOWING PHENO
  0;   60;     55;      0;           0;    7;            %; PROB OBS TO VISION  HAZE
  0;   60;     56;      0;           0;    7;            %; PROB OBS TO VISION  FOG
  0;   60;     57;      0;           0;    7;            %; PROB OBS TO VISION  NONE
  0;   60;     58;      0;           0;    7;            %; PROB TSTM PAST 6 HRS
  0;   60;     59;      0;           0;    7;            %; PROB TSTM PAST 12HRS
  0;   60;     60;      0;           0;    7;            %; PROB TSTM PAST 24HRS
  0;   60;     61;      0;           0;    7;            %; PROB SVR WX PAST 6 HRS
  0;   60;     62;      0;           0;    7;            %; PROB SVR WX PAST 12HRS
  0;   60;     63;      0;           0;    7;            %; PROB SVR WX PAST 24HRS
  0;   60;     64;      0;           0;    7;            %; CLIM AVG CLD COVER (OPAQUE)
  0;   60;     65;      1;           0;   12; METERS/SECOND; CLIMATIC WIND SPEED
  0;   60;     66;      1;           0;   12; DEGREES_KELVIN; CLIMATIC(NORMAL) DAY MAX TEMP
  0;   60;     67;      1;           0;   12; DEGREES_KELVIN; CLIMATIC(NORMAL) NIGHT MIN TEMP
  0;   60;     90;      0;           0;    4;   CODE_TABLE; QUANT PCP FCST (CATEGORIES)
  0;   60;     91;      0;           0;    3;   CODE_TABLE; COND PCP TYPE FCST (CATS)
  0;   60;     92;      0;           0;    3;   CODE_TABLE; COND PCP CHARACTER FCST (CATS)
  0;   60;     93;      0;           0;    3;   CODE_TABLE; QUANT SNOW AMT FCST (CATS)
  0;   60;     94;      0;           0;    4;   CODE_TABLE; CIG HEIGHT FCST (CATS)
  0;   60;     95;      0;           0;    3;   CODE_TABLE; VISIBILITY FCST (CATS)
  0;   60;     96;      0;           0;    3;   CODE_TABLE; OBSTRUCT TO VISION FCST (CATS)
  0;   60;     97;      0;           0;    2;   CODE_TABLE; THUNDERSTORM FCST (CATS)
  0;   60;     98;      0;           0;    2;   CODE_TABLE; SEVERE WEATHER FCST (CATS)
  0;   63;    255;      0;           0;    1;      NUMERIC; FILL BIT
