# Autoplotter Help

measurements within this range are considered valid. This field may be changed to exclude outliers or data that has not automatically been detected as fill.

### fill value

This value is used to identify invalid data that should not be plotted.

### # Invalid

# Invalid field indicates the number of measurements and invalid measurements for reference.

### Cadence

Cadence is the expected distance between successive measurements. If two measurements are much further than the cadence, then a connector is not drawn.