 000001 TABLE A: ENTRY                                                   CCITTIA5                   0            0  24 CHARACTER                 0         3
 000002 TABLE A: DATA CATEGORY DESCRIPTION, LINE 1                       CCITTIA5                   0            0 256 CHARACTER                 0        32
 000003 TABLE A: DATA CATEGORY DESCRIPTION, LINE 2                       CCITTIA5                   0            0 256 CHARACTER                 0        32
 000004 BUFR/CREX MASTER TABLE                                           CCITTIA5                   0            0  16 CHARACTER                 0         2
 000005 BUFR/CREX EDITION NUMBER                                         CCITTIA5                   0            0  24 CHARACTER                 0         3
 000006 BUFR MASTER TABLE VERSION NUMBER                                 CCITTIA5                   0            0  16 CHARACTER                 0         2
 000007 CREX MASTER TABLE VERSION NUMBER                                 CCITTIA5                   0            0  16 CHARACTER                 0         2
 000008 BUFR LOCAL TABLE VERSION NUMBER                                  CCITTIA5                   0            0  16 CHARACTER                 0         2
 000010 F DESCRIPTOR TO BE ADDED OR DEFINED                              CCITTIA5                   0            0   8 CHARACTER                 0         1
 000011 X DESCRIPTOR TO BE ADDED OR DEFINED                              CCITTIA5                   0            0  16 CHARACTER                 0         2
 000012 Y DESCRIPTOR TO BE ADDED OR DEFINED                              CCITTIA5                   0            0  24 CHARACTER                 0         3
 000013 ELEMENT NAME, LINE 1                                             CCITTIA5                   0            0 256 CHARACTER                 0        32
 000014 ELEMENT NAME, LINE 2                                             CCITTIA5                   0            0 256 CHARACTER                 0        32
 000015 UNITS NAME                                                       CCITTIA5                   0            0 192 CHARACTER                 0        24
 000016 UNITS SCALE SIGN                                                 CCITTIA5                   0            0   8 CHARACTER                 0         1
 000017 UNITS SCALE                                                      CCITTIA5                   0            0  24 CHARACTER                 0         3
 000018 UNITS REFERENCE SIGN                                             CCITTIA5                   0            0   8 CHARACTER                 0         1
 000019 UNITS REFERENCE VALUE                                            CCITTIA5                   0            0  80 CHARACTER                 0        10
 000020 ELEMENT DATA WIDTH                                               CCITTIA5                   0            0  24 CHARACTER                 0         3
 000024 CODE FIGURE                                                      CCITTIA5                   0            0  64 CHARACTER                 0         8
 000025 CODE FIGURE MEANING                                              CCITTIA5                   0            0 496 CHARACTER                 0        62
 000026 BIT NUMBER                                                       CCITTIA5                   0            0  16 CHARACTER                 0         2
 000027 BIT NUMBER MEANING                                               CCITTIA5                   0            0 496 CHARACTER                 0        62
 000030 DESCRIPTOR DEFINING SEQUENCE                                     CCITTIA5                   0            0  48 CHARACTER                 0         6
 001001 WMO BLOCK NUMBER                                                 NUMERIC                    0            0   7 NUMERIC                   0         2
 001002 WMO STATION NUMBER                                               NUMERIC                    0            0  10 NUMERIC                   0         3
 001003 WMO REGION NUMBER/GEOGRAPHICAL AREA                              CODETABLE                  0            0   3 CODE TABLE                0         1
 001004 WMO REGION SUB-AREA                                              NUMERIC                    0            0   3 NUMERIC                   0         1
 001005 BUOY/PLATFORM IDENTIFIER                                         NUMERIC                    0            0  17 NUMERIC                   0         5
 001006 AIRCRAFT FLIGHT NUMBER                                           CCITTIA5                   0            0  64 CHARACTER                 0         8
 001007 SATELLITE IDENTIFIER                                             CODETABLE                  0            0  10 CODE TABLE                0         4
 001008 AIRCRAFT REGISTRATION NUMBER OR OTHER IDENTIFICATION             CCITTIA5                   0            0  64 CHARACTER                 0         8
 001009 TYPE OF COMMERCIAL AIRCRAFT                                      CCITTIA5                   0            0  64 CHARACTER                 0         8
 001010 STATIONARY BUOY PLATFORM IDENTIFIER; E.G. C-MAN BUOYS            CCITTIA5                   0            0  64 CHARACTER                 0         8
 001011 SHIP OR MOBILE LAND STATION IDENTIFIER                           CCITTIA5                   0            0  72 CHARACTER                 0         9
 001012 DIRECTION OF MOTION OF MOVING OBSERVING PLATFORM (DEGREE TRUE)   DEG                        0            0   9 DEG                       0         3
 001013 SPEED OF MOTION OF MOVING OBSERVING PLATFORM                     M/S                        0            0  10 M/S                       0         3
 001014 PLATFORM DRIFT SPEED (HIGH PRECISION)                            M/S                        2            0  10 M/S                       2         4
 001015 STATION OR SITE NAME                                             CCITTIA5                   0            0 160 CHARACTER                 0        20
 001018 SHORT STATION OR SITE NAME                                       CCITTIA5                   0            0  40 CHARACTER                 0         5
 001019 LONG STATION OR SITE NAME                                        CCITTIA5                   0            0 256 CHARACTER                 0        32
 001020 WMO REGION SUB-AREA                                              NUMERIC                    0            0   4 NUMERIC                   0         2
 001021 SYNOPTIC FEATURE IDENTIFIER                                      NUMERIC                    0            0  14 NUMERIC                   0         4
 001022 NAME OF FEATURE                                                  CCITTIA5                   0            0 224 CHARACTER                 0        28
 001023 OBSERVATION SEQUENCE NUMBER                                      NUMERIC                    0            0   9 NUMERIC                   0         3
 001024 WIND SPEED SOURCE                                                CODETABLE                  0            0   5 CODE TABLE                0         2
 001025 STORM IDENTIFIER                                                 CCITTIA5                   0            0  24 CHARACTER                 0         3
 001026 WMO STORM NAME                                                   CCITTIA5                   0            0  64 CHARACTER                 0         8
 001027 WMO LONG STORM NAME                                              CCITTIA5                   0            0  80 CHARACTER                 0        10
 001028 AEROSOL OPTICAL DEPTH (AOD) SOURCE                               CODETABLE                  0            0   5 CODE TABLE                0         2
 001029 SSI SOURCE                                                       CODETABLE                  0            0   5 CODE TABLE                0         2
 001030 NUMERICAL MODEL IDENTIFIER                                       CCITTIA5                   0            0 128 CHARACTER                 0        16
 001031 IDENTIFICATION OF ORIGINATING/GENERATING CENTRE                  CODETABLE                  0            0  16 CODE TABLE                0         5
 001032 GENERATING APPLICATION                                           CODETABLE                  0            0   8 CODE TABLE                0         3
 001033 IDENTIFICATION OF ORIGINATING/GENERATING CENTRE                  COMMONCODETABLEC-1         0            0   8 COMMON CODE TABLE C-1      0         3
 001034 IDENTIFICATION OF ORIGINATING/GENERATING SUB-CENTRE              COMMONCODETABLEC-12        0            0   8 COMMON CODE TABLE C-12      0         3
 001035 ORIGINATING CENTRE                                               COMMONCODETABLEC-11        0            0  16 COMMON CODE TABLE C-11      0         5
 001036 AGENCY IN CHARGE OF OPERATING THE OBSERVING PLATFORM             CODETABLE                  0            0  20 CODE TABLE                0         7
 001037 SIGMET SEQUENCE IDENTIFIER                                       CCITTIA5                   0            0  24 CHARACTER                 0         3
 001038 SOURCE OF SEA ICE FRACTION                                       CODETABLE                  0            0   5 CODE TABLE                0         2
 001039 GRAPHICAL AREA FORECAST (GFA) SEQUENCE IDENTIFIER                CCITTIA5                   0            0  40 CHARACTER                 0         5
 001041 ABSOLUTE PLATFORM VELOCITY - FIRST COMPONENT                     M/S                        5  -1073741824  31 M/S                       5        10
 001042 ABSOLUTE PLATFORM VELOCITY - SECOND COMPONENT                    M/S                        5  -1073741824  31 M/S                       5        10
 001043 ABSOLUTE PLATFORM VELOCITY - THIRD COMPONENT                     M/S                        5  -1073741824  31 M/S                       5        10
 001050 PLATFORM TRANSMITTER ID NUMBER                                   NUMERIC                    0            0  17 NUMERIC                   0         6
 001051 PLATFORM TRANSMITTER ID NUMBER                                   CCITTIA5                   0            0  96 CHARACTER                 0        12
 001052 PLATFORM TRANSMITTER ID                                          CODETABLE                  0            0   3 CODE TABLE                0         1
 001053 TSUNAMETER REPORT SEQUENCE NUMBER TRIGGERED BY A TSUNAMI EVENT   NUMERIC                    0            0   7 NUMERIC                   0         2
 001060 AIRCRAFT REPORTING POINT (BEACON IDENTIFIER)                     CCITTIA5                   0            0  64 CHARACTER                 0         8
 001062 SHORT ICAO LOCATION INDICATOR                                    CCITTIA5                   0            0  32 CHARACTER                 0         4
 001063 ICAO LOCATION INDICATOR                                          CCITTIA5                   0            0  64 CHARACTER                 0         8
 001064 RUNWAY DESIGNATOR                                                CCITTIA5                   0            0  32 CHARACTER                 0         4
 001065 ICAO REGION IDENTIFIER                                           CCITTIA5                   0            0 256 CHARACTER                 0        32
 001075 TIDE STATION IDENTIFICATION                                      CCITTIA5                   0            0  40 CHARACTER                 0         5
 001080 SHIP LINE NUMBER ACCORDING TO SOOP                               CCITTIA5                   0            0  32 CHARACTER                 0         4
 001081 RADIOSONDE SERIAL NUMBER                                         CCITTIA5                   0            0 160 CHARACTER                 0        20
 001082 RADIOSONDE ASCENSION NUMBER                                      NUMERIC                    0            0  14 NUMERIC                   0         4
 001083 RADIOSONDE RELEASE NUMBER                                        NUMERIC                    0            0   3 NUMERIC                   0         1
 001085 OBSERVING PLATFORM MANUFACTURER'S MODEL                          CCITTIA5                   0            0 160 CHARACTER                 0        20
 001086 OBSERVING PLATFORM MANUFACTURER'S SERIAL NUMBER                  CCITTIA5                   0            0 256 CHARACTER                 0        32
 001087 WMO MARINE OBSERVING PLATFORM EXTENDED IDENTIFIER                NUMERIC                    0            0  23 NUMERIC                   0         7
 001090 TECHNIQUE FOR MAKING UP INITIAL PERTURBATIONS                    CODETABLE                  0            0   8 CODE TABLE                0         3
 001091 ENSEMBLE MEMBER NUMBER                                           NUMERIC                    0            0  10 NUMERIC                   0         4
 001092 TYPE OF ENSEMBLE FORECAST                                        CODETABLE                  0            0   8 CODE TABLE                0         3
 001093 BALLOON LOT NUMBER                                               CCITTIA5                   0            0  96 CHARACTER                 0        12
 001094 WBAN NUMBER                                                      NUMERIC                    0            0  17 NUMERIC                   0         5
 001095 OBSERVER IDENTIFICATION                                          CCITTIA5                   0            0  32 CHARACTER                 0         4
 001096 STATION ACQUISITION                                              CCITTIA5                   0            0 160 CHARACTER                 0        20
 001097 STAR CATALOG NUMBER                                              NUMERIC                    0            0  13 NUMERIC                   0         4
 001098 TYPE OF PRODUCT                                                  CODETABLE                  0            0  12 CODE TABLE                0         4
 001099 UNIQUE PRODUCT DEFINITION                                        CCITTIA5                   0            0 248 CHARACTER                 0        31
 001101 STATE IDENTIFIER                                                 CODETABLE                  0            0  10 CODE TABLE                0         3
 001102 NATIONAL STATION NUMBER                                          NUMERIC                    0            0  30 NUMERIC                   0         9
 001103 IMO NUMBER. UNIQUE LLOYD'S REGISTRY                              NUMERIC                    0            0  14 NUMERIC                   0         5
 001110 AIRCRAFT TAIL NUMBER                                             CCITTIA5                   0            0  48 CHARACTER                 0         6
 001111 ORIGINATION AIRPORT                                              CCITTIA5                   0            0  24 CHARACTER                 0         3
 001112 DESTINATION AIRPORT                                              CCITTIA5                   0            0  24 CHARACTER                 0         3
 001113 TEMPLATE VERSION NUMBER DEFINED BY ORIGINATING CENTRE            NUMERIC                    1            0   9 NUMERIC                   1         3
 001124 GRID POINT IDENTIFIER                                            NUMERIC                    0            0  24 NUMERIC                   0         8
 001144 SNAPSHOT IDENTIFIER                                              NUMERIC                    0            0  31 NUMERIC                   0        10
 002001 TYPE OF STATION                                                  CODETABLE                  0            0   2 CODE TABLE                0         1
 002002 TYPE OF INSTRUMENTATION FOR WIND MEASUREMENT                     FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 002003 TYPE OF MEASURING EQUIPMENT USED                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 002004 TYPE OF INSTRUMENTATION FOR EVAPORATION MEASUREMENT              CODETABLE                  0            0   4 CODE TABLE                0         2
 002005 PRECISION OF TEMPERATURE OBSERVATION                             K                          2            0   7 K                         2         3
 002007 TYPE OF SENSOR FOR WATER LEVEL MEASURING INSTRUMENT              CODETABLE                  0            0   4 CODE TABLE                0         2
 002011 RADIOSONDE TYPE                                                  CODETABLE                  0            0   8 CODE TABLE                0         3
 002012 RADIOSONDE COMPUTATIONAL METHOD                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 002013 SOLAR AND INFRARED RADIATION CORRECTION                          CODETABLE                  0            0   4 CODE TABLE                0         2
 002014 TRACKING TECHNIQUE/STATUS OF SYSTEM USED                         CODETABLE                  0            0   7 CODE TABLE                0         3
 002015 RADIOSONDE COMPLETENESS                                          CODETABLE                  0            0   4 CODE TABLE                0         2
 002016 RADIOSONDE CONFIGURATION                                         FLAGTABLE                  0            0   5 FLAG TABLE                0         2
 002019 SATELLITE INSTRUMENTS                                            CODETABLE                  0            0  11 CODE TABLE                0         4
 002020 SATELLITE CLASSIFICATION                                         CODETABLE                  0            0   9 CODE TABLE                0         3
 002021 SATELLITE INSTRUMENT DATA USED IN PROCESSING                     FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 002022 SATELLITE DATA-PROCESSING TECHNIQUE USED                         FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 002023 SATELLITE-DERIVED WIND COMPUTATION METHOD                        CODETABLE                  0            0   4 CODE TABLE                0         2
 002024 INTEGRATED MEAN HUMIDITY COMPUTATIONAL METHOD                    CODETABLE                  0            0   4 CODE TABLE                0         2
 002025 SATELLITE CHANNEL(S) USED IN COMPUTATION                         FLAGTABLE                  0            0  25 FLAG TABLE                0         9
 002026 CROSS-TRACK RESOLUTION                                           M                          2            0  12 M                         2         4
 002027 ALONG-TRACK RESOLUTION                                           M                          2            0  12 M                         2         4
 002028 SEGMENT SIZE AT NADIR IN X-DIRECTION                             M                          0            0  18 M                         0         6
 002029 SEGMENT SIZE AT NADIR IN Y-DIRECTION                             M                          0            0  18 M                         0         6
 002030 METHOD OF CURRENT MEASUREMENT                                    CODETABLE                  0            0   3 CODE TABLE                0         1
 002031 DURATION AND TIME OF CURRENT MEASUREMENT                         CODETABLE                  0            0   5 CODE TABLE                0         2
 002032 INDICATOR FOR DIGITIZATION                                       CODETABLE                  0            0   2 CODE TABLE                0         1
 002033 METHOD OF SALINITY/DEPTH MEASUREMENT                             CODETABLE                  0            0   3 CODE TABLE                0         1
 002034 DROGUE TYPE                                                      CODETABLE                  0            0   5 CODE TABLE                0         2
 002035 CABLE LENGTH                                                     M                          0            0   9 M                         0         3
 002036 BUOY TYPE                                                        CODETABLE                  0            0   2 CODE TABLE                0         1
 002037 METHOD OF TIDAL OBSERVATION                                      CODETABLE                  0            0   3 CODE TABLE                0         1
 002038 METHOD OF WATER TEMPERATURE AND/OR SALINITY MEASUREMENT          CODETABLE                  0            0   4 CODE TABLE                0         2
 002039 METHOD OF WET-BULB TEMPERATURE MEASUREMENT                       CODETABLE                  0            0   3 CODE TABLE                0         1
 002040 METHOD OF REMOVING VELOCITY AND MOTION OF PLATFORM FROM CURRENT  CODETABLE                  0            0   4 CODE TABLE                0         2
 002041 METHOD FOR ESTIMATING REPORTS RELATED TO SYNOPTIC FEATURES       CODETABLE                  0            0   6 CODE TABLE                0         2
 002042 INDICATOR FOR SEA SURFACE CURRENT SPEED                          CODETABLE                  0            0   2 CODE TABLE                0         1
 002044 INDICATOR FOR METHOD OF CALCULATING SPECTRAL WAVE DATA           CODETABLE                  0            0   4 CODE TABLE                0         2
 002045 INDICATOR FOR TYPE OF PLATFORM                                   CODETABLE                  0            0   4 CODE TABLE                0         2
 002046 WAVE MEASUREMENT INSTRUMENTATION                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 002047 DEEP-OCEAN TSUNAMETER TYPE                                       CODETABLE                  0            0   7 CODE TABLE                0         2
 002048 SATELLITE SENSOR INDICATOR                                       CODETABLE                  0            0   4 CODE TABLE                0         2
 002049 GEOSTATIONARY SATELLITE DATA-PROCESSING TECHNIQUE USED           FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 002050 GEOSTATIONARY SOUNDER SATELLITE CHANNELS USED                    FLAGTABLE                  0            0  20 FLAG TABLE                0         7
 002051 INDICATOR TO SPECIFY OBSERVING METHOD FOR EXTREME TEMPERATURES   CODETABLE                  0            0   4 CODE TABLE                0         2
 002052 GEOSTATIONARY IMAGER SATELLITE CHANNELS USED                     FLAGTABLE                  0            0   6 FLAG TABLE                0         2
 002053 GOES-I/M BRIGHTNESS TEMPERATURE CHARACTERISTICS                  CODETABLE                  0            0   4 CODE TABLE                0         2
 002054 GOES-I/M SOUNDINGS PARAMETER CHARACTERISTICS                     CODETABLE                  0            0   4 CODE TABLE                0         2
 002055 GEOSTATIONARY SOUNDINGS STATISTICAL PARAMETERS                   CODETABLE                  0            0   4 CODE TABLE                0         2
 002056 GEOSTATIONARY SOUNDINGS ACCURACY STATISTICS                      CODETABLE                  0            0   4 CODE TABLE                0         2
 002057 ORIGIN OF FIRST-GUESS INFORMATION FOR GOES-I/M SOUNDINGS         CODETABLE                  0            0   4 CODE TABLE                0         2
 002058 VALID TIMES OF FIRST GUESS INFORMATION FOR GOES-I/M SOUNDINGS    CODETABLE                  0            0   4 CODE TABLE                0         2
 002059 ORIGIN OF ANALYSIS INFORMATION FOR GOES-I/M SOUNDINGS            CODETABLE                  0            0   4 CODE TABLE                0         2
 002060 ORIGIN OF SURFACE INFORMATION FOR GOES-I/M SOUNDINGS             CODETABLE                  0            0   4 CODE TABLE                0         2
 002061 AIRCRAFT NAVIGATIONAL SYSTEM                                     CODETABLE                  0            0   3 CODE TABLE                0         1
 002062 TYPE OF AIRCRAFT DATA RELAY SYSTEM                               CODETABLE                  0            0   4 CODE TABLE                0         2
 002063 AIRCRAFT ROLL ANGLE                                              DEG                        2       -18000  16 DEG                       2         5
 002064 AIRCRAFT ROLL ANGLE QUALITY                                      CODETABLE                  0            0   2 CODE TABLE                0         1
 002065 ACARS GROUND-RECEIVING STATION                                   CCITTIA5                   0            0  40 CHARACTER                 0         5
 002066 RADIOSONDE GROUND RECEIVING SYSTEM                               CODETABLE                  0            0   6 CODE TABLE                0         2
 002067 RADIOSONDE OPERATING FREQUENCY                                   HZ                        -5            0  15 HZ                       -5         5
 002070 ORIGINAL SPECIFICATION OF LATITUDE/LONGITUDE                     CODETABLE                  0            0   4 CODE TABLE                0         2
 002071 SPECTROGRAPHIC WAVELENGTH                                        M                         13            0  30 M                        13        10
 002072 SPECTROGRAPHIC WIDTH                                             M                         13            0  30 M                        13        10
 002080 BALLOON MANUFACTURER                                             CODETABLE                  0            0   6 CODE TABLE                0         2
 002081 TYPE OF BALLOON                                                  CODETABLE                  0            0   5 CODE TABLE                0         2
 002082 WEIGHT OF BALLOON                                                KG                         3            0  12 KG                        3         4
 002083 TYPE OF BALLOON SHELTER                                          CODETABLE                  0            0   4 CODE TABLE                0         2
 002084 TYPE OF GAS USED IN BALLOON                                      CODETABLE                  0            0   4 CODE TABLE                0         2
 002085 AMOUNT OF GAS USED IN BALLOON                                    KG                         3            0  13 KG                        3         4
 002086 BALLOON FLIGHT TRAIN LENGTH                                      M                          1            0  10 M                         1         4
 002091 ENTRY SENSOR 4/20 MA                                             A                          4            0  10 A                         4         3
 002095 TYPE OF PRESSURE SENSOR                                          CODETABLE                  0            0   5 CODE TABLE                0         2
 002096 TYPE OF TEMPERATURE SENSOR                                       CODETABLE                  0            0   5 CODE TABLE                0         2
 002097 TYPE OF HUMIDITY SENSOR                                          CODETABLE                  0            0   5 CODE TABLE                0         2
 002098 TYPE OF WAVE SENSOR                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 002099 POLARIZATION                                                     CODETABLE                  0            0   3 CODE TABLE                0         1
 002100 RADAR CONSTANT                                                   DB                         1            0  12 DB                        1         4
 002101 TYPE OF ANTENNA                                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 002102 ANTENNA HEIGHT ABOVE TOWER BASE                                  M                          0            0   8 M                         0         3
 002103 RADOME                                                           FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 002104 ANTENNA POLARIZATION                                             CODETABLE                  0            0   4 CODE TABLE                0         2
 002105 MAXIMUM ANTENNA GAIN                                             DB                         0            0   6 DB                        0         2
 002106 3-DB BEAMWIDTH                                                   DEG                        1            0   6 DEG                       1         2
 002107 SIDELOBE SUPPRESSION                                             DB                         0            0   6 DB                        0         2
 002108 CROSSPOL DISCRIMINATION (ON AXIS)                                DB                         0            0   6 DB                        0         2
 002109 ANTENNA SPEED (AZIMUTH)                                          DEG/S                      2            0  12 DEG/S                     2         4
 002110 ANTENNA SPEED (ELEVATION)                                        DEG/S                      2            0  12 DEG/S                     2         4
 002111 RADAR INCIDENCE ANGLE                                            DEG                        1            0  10 DEG                       1         4
 002112 RADAR LOOK ANGLE                                                 DEG                        1            0  12 DEG                       1         4
 002113 NUMBER OF AZIMUTH LOOKS                                          NUMERIC                    0            0   4 NUMERIC                   0         2
 002114 ANTENNA EFFECTIVE SURFACE AREA                                   M2                         0            0  15 M2                        0         5
 002115 TYPE OF SURFACE OBSERVING EQUIPMENT                              CODETABLE                  0            0   5 CODE TABLE                0         2
 002116 PERCENTAGE OF 320 MHZ BAND PROCESSED                             %                          0            0   7 %                         0         3
 002117 PERCENTAGE OF 80 MHZ BAND PROCESSED                              %                          0            0   7 %                         0         3
 002118 PERCENTAGE OF 20 MHZ BAND PROCESSED                              %                          0            0   7 %                         0         3
 002119 INSTRUMENT OPERATIONS                                            CODETABLE                  0            0   3 CODE TABLE                0         1
 002120 OCEAN WAVE FREQUENCY                                             HZ                         3            0  10 HZ                        3         4
 002121 MEAN FREQUENCY                                                   HZ                        -8            0   7 HZ                       -8         3
 002122 FREQUENCY AGILITY RANGE                                          HZ                        -6         -128   8 HZ                       -6         3
 002123 PEAK POWER                                                       W                         -4            0   7 W                        -4         3
 002124 AVERAGE POWER                                                    W                         -1            0   7 W                        -1         3
 002125 PULSE REPETITION FREQUENCY                                       HZ                        -1            0   8 HZ                       -1         3
 002126 PULSE WIDTH                                                      S                          7            0   6 S                         7         2
 002127 RECEIVER INTERMEDIATE FREQUENCY                                  HZ                        -6            0   7 HZ                       -6         3
 002128 INTERMEDIATE FREQUENCY BANDWIDTH                                 HZ                        -5            0   6 HZ                       -5         2
 002129 MINIMUM DETECTABLE SIGNAL                                        DB                         0         -150   5 DB                        0         3
 002130 DYNAMIC RANGE                                                    DB                         0            0   7 DB                        0         3
 002131 SENSITIVITY TIME CONTROL (STC)                                   FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 002132 AZIMUTH POINTING ACCURACY                                        DEG                        2            0   6 DEG                       2         2
 002133 ELEVATION POINTING ACCURACY                                      DEG                        2            0   6 DEG                       2         2
 002134 ANTENNA BEAM AZIMUTH                                             DEG                        2            0  16 DEG                       2         5
 002135 ANTENNA ELEVATION                                                DEG                        2        -9000  15 DEG                       2         5
 002136 RANGE PROCESSED BY RANGE ATTENUATION CORRECTION                  M                         -3            0  16 M                        -3         5
 002137 RADAR DUAL PRF RATIO                                             CODETABLE                  0            0   4 CODE TABLE                0         2
 002138 ANTENNA ROTATION DIRECTION                                       CODETABLE                  0            0   2 CODE TABLE                0         1
 002140 SATELLITE RADAR BEAM AZIMUTH ANGLE                               DEG                        0            0   9 DEG                       0         3
 002141 MEASUREMENT TYPE                                                 CCITTIA5                   0            0  24 CHARACTER                 0         3
 002142 OZONE INSTRUMENT SERIAL NUMBER/IDENTIFICATION                    CCITTIA5                   0            0  32 CHARACTER                 0         4
 002143 OZONE INSTRUMENT TYPE                                            CODETABLE                  0            0   7 CODE TABLE                0         3
 002144 LIGHT SOURCE TYPE FOR BREWER SPECTROPHOTOMETER                   CODETABLE                  0            0   4 CODE TABLE                0         2
 002145 WAVELENGTH SETTING FOR DOBSON INSTRUMENTS                        CODETABLE                  0            0   4 CODE TABLE                0         2
 002146 SOURCE CONDITIONS FOR DOBSON INSTRUMENTS                         CODETABLE                  0            0   4 CODE TABLE                0         2
 002147 METHOD OF TRANSMISSION TO COLLECTION CENTRE                      CODETABLE                  0            0   7 CODE TABLE                0         2
 002148 DATA COLLECTION AND/OR LOCATION SYSTEM                           CODETABLE                  0            0   5 CODE TABLE                0         2
 002149 TYPE OF DATA BUOY                                                CODETABLE                  0            0   6 CODE TABLE                0         2
 002150 TOVS/ATOVS/AVHRR INSTRUMENTATION CHANNEL NUMBER                  CODETABLE                  0            0   6 CODE TABLE                0         2
 002151 RADIOMETER IDENTIFIER                                            CODETABLE                  0            0  11 CODE TABLE                0         4
 002152 SATELLITE INSTRUMENT USED IN DATA PROCESSING                     FLAGTABLE                  0            0  31 FLAG TABLE                0        10
 002153 SATELLITE CHANNEL CENTRE FREQUENCY                               HZ                        -8            0  26 HZ                       -8         8
 002154 SATELLITE CHANNEL BAND WIDTH                                     HZ                        -8            0  26 HZ                       -8         8
 002155 SATELLITE CHANNEL WAVELENGTH                                     M                          9            0  16 M                         9         5
 002156 PERCENTAGE OF VALID KU OCEAN RETRACKER MEASUREMENTS              %                          0            0   7 %                         0         3
 002157 PERCENTAGE OF VALID S OCEAN RETRACKER MEASUREMENTS               %                          0            0   7 %                         0         3
 002158 RA-2 INSTRUMENTS                                                 FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 002159 MWR INSTRUMENTS                                                  FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 002160 WAVE LENGTH OF THE RADAR                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 002163 HEIGHT ASSIGNMENT METHOD                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 002164 TRACER CORRELATION METHOD                                        CODETABLE                  0            0   3 CODE TABLE                0         1
 002165 RADIANCE TYPE FLAGS                                              FLAGTABLE                  0            0  15 FLAG TABLE                0         5
 002166 RADIANCE TYPE                                                    CODETABLE                  0            0   4 CODE TABLE                0         2
 002167 RADIANCE COMPUTATIONAL METHOD                                    CODETABLE                  0            0   4 CODE TABLE                0         2
 002168 HYDROSTATIC PRESSURE OF LOWER END OF CABLE (THERMISTOR STRING)   PA                        -3            0  16 KPA                       0         5
 002169 ANEMOMETER TYPE                                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 002171 INSTRUMENT SERIAL NUMBER FOR WATER TEMPERATURE PROFILE           CCITTIA5                   0            0  64 CCITT IA5                 0         8
 002172 PRODUCT TYPE FOR RETRIEVED ATMOSPHERIC GASES                     CODETABLE                  0            0   8 CODE TABLE                0         3
 002173 SQUARE OF THE OFF-NADIR ANGLE                                    DEG2                       4            0  10 DEG2                      4         4
 002174 MEAN ACROSS TRACK PIXEL NUMBER                                   NUMERIC                    0            0   9 NUMERIC                   0         3
 002175 METHOD OF PRECIPITATION MEASUREMENT                              CODETABLE                  0            0   4 CODE TABLE                0         2
 002176 METHOD OF STATE OF GROUND MEASUREMENT                            CODETABLE                  0            0   4 CODE TABLE                0         2
 002177 METHOD OF SNOW DEPTH MEASUREMENT                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 002178 METHOD OF LIQUID CONTENT MEASUREMENT OF PRECIPITATION            CODETABLE                  0            0   4 CODE TABLE                0         2
 002179 TYPE OF SKY CONDITION ALGORITHM                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 002180 MAIN PRESENT WEATHER DETECTING SYSTEM                            CODETABLE                  0            0   4 CODE TABLE                0         2
 002181 SUPPLEMENTARY PRESENT WEATHER SENSOR                             FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 002182 VISIBILITY MEASUREMENT SYSTEM                                    CODETABLE                  0            0   4 CODE TABLE                0         2
 002183 CLOUD DETECTION SYSTEM                                           CODETABLE                  0            0   4 CODE TABLE                0         2
 002184 TYPE OF LIGHTNING DETECTION SENSOR                               CODETABLE                  0            0   4 CODE TABLE                0         2
 002185 METHOD OF EVAPORATION MEASUREMENT                                CODETABLE                  0            0   4 CODE TABLE                0         2
 002186 CAPABILITY TO DETECT PRECIPITATION PHENOMENA                     FLAGTABLE                  0            0  30 FLAG TABLE                0        10
 002187 CAPABILITY TO DETECT OTHER WEATHER PHENOMENA                     FLAGTABLE                  0            0  18 FLAG TABLE                0         6
 002188 CAPABILITY TO DETECT OBSCURATION                                 FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 002189 CAPABILITY TO DISCRIMINATE LIGHTNING STRIKES                     FLAGTABLE                  0            0  12 FLAG TABLE                0         4
 002190 LAGRANGIAN DRIFTER SUBMERGENCE (% TIME SUBMERGED)                %                          0            0   7 %                         0         3
 002191 GEOPOTENTIAL HEIGHT CALCULATION                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 004001 YEAR                                                             A                          0            0  12 A                         0         4
 004002 MONTH                                                            MON                        0            0   4 MON                       0         2
 004003 DAY                                                              D                          0            0   6 D                         0         2
 004004 HOUR                                                             H                          0            0   5 H                         0         2
 004005 MINUTE                                                           MIN                        0            0   6 MIN                       0         2
 004006 SECOND                                                           S                          0            0   6 S                         0         2
 004007 SECONDS WITHIN A MINUTE (MICROSECOND ACCURACY)                   S                          6            0  26 S                         6         8
 004008 SECONDS WITHIN A MINUTE (HIGH ACCURACY)                          S                          7            0  30                                      
 004011 TIME INCREMENT                                                   A                          0        -1024  11 A                         0         4
 004012 TIME INCREMENT                                                   MON                        0        -1024  11 MON                       0         4
 004013 TIME INCREMENT                                                   D                          0        -1024  11 D                         0         4
 004014 TIME INCREMENT                                                   H                          0        -1024  11 H                         0         4
 004015 TIME INCREMENT                                                   MIN                        0        -2048  12 MIN                       0         4
 004016 TIME INCREMENT                                                   S                          0        -4096  13 S                         0         4
 004017 REFERENCE TIME PERIOD FOR ACCUMULATED OR EXTREME DATA            MIN                        0        -1440  12 MIN                       0         4
 004021 TIME PERIOD OR DISPLACEMENT                                      A                          0        -1024  11 A                         0         4
 004022 TIME PERIOD OR DISPLACEMENT                                      MON                        0        -1024  11 MON                       0         4
 004023 TIME PERIOD OR DISPLACEMENT                                      D                          0        -1024  11 D                         0         4
 004024 TIME PERIOD OR DISPLACEMENT                                      H                          0        -2048  12 H                         0         4
 004025 TIME PERIOD OR DISPLACEMENT                                      MIN                        0        -2048  12 MIN                       0         4
 004026 TIME PERIOD OR DISPLACEMENT                                      S                          0        -4096  13 S                         0         4
 004031 DURATION OF TIME RELATING TO FOLLOWING VALUE                     H                          0            0   8 H                         0         3
 004032 DURATION OF TIME RELATING TO FOLLOWING VALUE                     MIN                        0            0   6 MIN                       0         2
 004041 TIME DIFFERENCE, UTC - LMT                                       MIN                        0        -1440  12 MIN                       0         4
 004043 DAY OF THE YEAR                                                  D                          0            0   9 D                         0         3
 004051 PRINCIPAL TIME OF DAILY READING OF MAXIMUM TEMPERATURE           H                          0            0   5 H                         0         2
 004052 PRINCIPAL TIME OF DAILY READING OF MINIMUM TEMPERATURE           H                          0            0   5 H                         0         2
 004053 NUMBER OF DAYS WITH PRECIPITATION EQUAL TO OR MORE THAN 1 MM     NUMERIC                    0            0   6 NUMERIC                   0         2
 004059 TIMES OF OBSERVATION USED TO COMPUTE THE REPORTED MEAN VALUES    FLAGTABLE                  0            0   6 FLAG TABLE                0         2
 004065 SHORT TIME INCREMENT                                             MIN                        0         -128   8 MIN                       0         2
 004066 SHORT TIME INCREMENT                                             S                          0         -128   8 S                         0         2
 004073 SHORT TIME PERIOD OR DISPLACEMENT                                D                          0         -128   8 D                         0         2
 004074 SHORT TIME PERIOD OR DISPLACEMENT                                H                          0         -128   8 H                         0         2
 004075 SHORT TIME PERIOD OR DISPLACEMENT                                MIN                        0         -128   8 MIN                       0         2
 004080 AVERAGING PERIOD FOR FOLLOWING VALUE                             CODETABLE                  0            0   4 CODE TABLE                0         2
 004086 LONG TIME PERIOD OR DISPLACEMENT                                 S                          0        -8192  15 S                         0         5
 005001 LATITUDE (HIGH ACCURACY)                                         DEG                        5     -9000000  25 DEG                       5         7
 005002 LATITUDE (COARSE ACCURACY)                                       DEG                        2        -9000  15 DEG                       2         4
 005011 LATITUDE INCREMENT (HIGH ACCURACY)                               DEG                        5     -9000000  25 DEG                       5         7
 005012 LATITUDE INCREMENT (COARSE ACCURACY)                             DEG                        2        -9000  15 DEG                       2         4
 005015 LATITUDE DISPLACEMENT (HIGH ACCURACY)                            DEG                        5     -9000000  25 DEG                       5         7
 005016 LATITUDE DISPLACEMENT (COARSE ACCURACY)                          DEG                        2        -9000  15 DEG                       2         4
 005021 BEARING OR AZIMUTH (DEGREE TRUE)                                 DEG                        2            0  16 DEG                       2         5
 005022 SOLAR AZIMUTH (DEGREE TRUE)                                      DEG                        2            0  16 DEG                       2         5
 005023 SUN TO SATELLITE AZIMUTH DIFFERENCE                              DEG                        1        -1800  12 DEG                       1         4
 005030 DIRECTION (SPECTRAL)                                             DEG                        0            0  12 DEG                       0         4
 005031 ROW NUMBER                                                       NUMERIC                    0            0  12 NUMERIC                   0         4
 005033 PIXEL SIZE ON HORIZONTAL - 1                                     M                         -1            0  16 M                        -1         5
 005034 ALONG TRACK ROW NUMBER                                           NUMERIC                    0            0  11 NUMERIC                   0         4
 005035 MAXIMUM SIZE OF X-DIMENSION                                      NUMERIC                    0            0  12 NUMERIC                   0         4
 005036 SHIP TRANSECT NUMBER ACCORDING TO SOOP                           NUMERIC                    0            0   7 NUMERIC                   0         2
 005040 ORBIT NUMBER                                                     NUMERIC                    0            0  24 NUMERIC                   0         8
 005041 SCAN LINE NUMBER                                                 NUMERIC                    0            0   8 NUMERIC                   0         3
 005042 CHANNEL NUMBER                                                   NUMERIC                    0            0   6 NUMERIC                   0         2
 005043 FIELD OF VIEW NUMBER                                             NUMERIC                    0            0   8 NUMERIC                   0         3
 005044 SATELLITE CYCLE NUMBER                                           NUMERIC                    0            0  11 NUMERIC                   0         4
 005045 FIELD OF REGARD NUMBER                                           NUMERIC                    0            0   8 NUMERIC                   0         3
 005052 CHANNEL NUMBER INCREMENT                                         NUMERIC                    0            0   5 NUMERIC                   0         2
 005053 FIELD OF VIEW NUMBER INCREMENT                                   NUMERIC                    0            0   5 NUMERIC                   0         2
 005060 Y ANGULAR POSITION FROM CENTRE OF GRAVITY                        DEG                        6     -8000000  24 DEG                       6         8
 005061 Z ANGULAR POSITION FROM CENTRE OF GRAVITY                        DEG                        6     -8000000  24 DEG                       6         8
 006001 LONGITUDE (HIGH ACCURACY)                                        DEG                        5    -18000000  26 DEG                       5         8
 006002 LONGITUDE (COARSE ACCURACY)                                      DEG                        2       -18000  16 DEG                       2         5
 006011 LONGITUDE INCREMENT (HIGH ACCURACY)                              DEG                        5    -18000000  26 DEG                       5         8
 006012 LONGITUDE INCREMENT (COARSE ACCURACY)                            DEG                        2       -18000  16 DEG                       2         5
 006015 LONGITUDE DISPLACEMENT (HIGH ACCURACY)                           DEG                        5    -18000000  26 DEG                       5         8
 006016 LONGITUDE DISPLACEMENT (COARSE ACCURACY)                         DEG                        2       -18000  16 DEG                       2         5
 006021 DISTANCE                                                         M                         -1            0  13 M                        -1         4
 006029 WAVE NUMBER                                                      M-1                        1            0  22 M-1                       1         7
 006030 WAVE NUMBER (SPECTRAL)                                           RAD/M                      5            0  13 RAD/M                     5         4
 006031 COLUMN NUMBER                                                    NUMERIC                    0            0  12 NUMERIC                   0         4
 006033 PIXEL SIZE ON HORIZONTAL - 2                                     M                         -1            0  16 M                        -1         5
 006034 CROSS-TRACK CELL NUMBER                                          NUMERIC                    0            0   7 NUMERIC                   0         3
 006035 MAXIMUM SIZE OF Y-DIMENSION                                      NUMERIC                    0            0  12 NUMERIC                   0         4
 006040 RADIUS OF CONFIDENCE                                             M                          0            0  13 M                         0         4
 007001 HEIGHT OF STATION                                                M                          0         -400  15 M                         0         5
 007002 HEIGHT OR ALTITUDE                                               M                         -1          -40  16 M                        -1         5
 007003 GEOPOTENTIAL                                                     M2S-2                     -1         -400  17 M2 S-2                   -1         6
 007004 PRESSURE                                                         PA                        -1            0  14 PA                       -1         5
 007005 HEIGHT INCREMENT                                                 M                          0         -400  12 M                         0         4
 007006 HEIGHT ABOVE STATION                                             M                          0            0  15 M                         0         5
 007007 HEIGHT                                                           M                          0        -1000  17 M                         0         6
 007008 GEOPOTENTIAL                                                     M2S-2                      0       -10000  20 M2 S-2                    0         7
 007009 GEOPOTENTIAL HEIGHT                                              GPM                        0        -1000  17 GPM                       0         5
 007010 FLIGHT LEVEL                                                     M                          0        -1024  16 FT                       -1         5
 007011 PRESSURE (HIGH PRECISION)                                        PA                         0            0  30 PA                        0        10
 007012 GRID POINT ALTITUDE                                              M                          2       -50000  20 M                         2         7
 007021 ELEVATION                                                        DEG                        2        -9000  15 DEG                       2         5
 007022 SOLAR ELEVATION                                                  DEG                        2        -9000  15 DEG                       2         5
 007024 SATELLITE ZENITH ANGLE                                           DEG                        2        -9000  15 DEG                       2         5
 007025 SOLAR ZENITH ANGLE                                               DEG                        2        -9000  15 DEG                       2         5
 007026 SATELLITE ZENITH ANGLE                                           DEG                        4      -900000  21 DEG                       4         7
 007030 HEIGHT OF STATION GROUND ABOVE MEAN SEA LEVEL                    M                          1        -4000  17 M                         1         5
 007031 HEIGHT OF BAROMETER ABOVE MEAN SEA LEVEL                         M                          1        -4000  17 M                         1         5
 007032 HEIGHT OF SENSOR ABOVE LOCAL GROUND (OR DECK OF MARINE PLATFORM) M                          2            0  16 M                         2         5
 007033 HEIGHT OF SENSOR ABOVE WATER SURFACE                             M                          1            0  12 M                         1         4
 007035 MAXIMUM SIZE OF Z-DIMENSION                                      NUMERIC                    0            0  12 NUMERIC                   0         4
 007036 LEVEL INDEX OF Z                                                 NUMERIC                    0            0  12 NUMERIC                   0         4
 007040 IMPACT PARAMETER                                                 M                          1     62000000  22 M                         1         8
 007061 DEPTH BELOW LAND SURFACE                                         M                          2            0  14 M                         2         5
 007062 DEPTH BELOW SEA/WATER SURFACE                                    M                          1            0  17 M                         1         6
 007063 DEPTH BELOW SEA/WATER SURFACE (CM)                               M                          2            0  20 M                         2         7
 007064 REPRESENTATIVE HEIGHT OF SENSOR ABOVE STATION                    M                          0            0   4 M                         0         2
 007065 WATER PRESSURE                                                   PA                        -3            0  17 PA                       -3         6
 007070 DROGUE DEPTH                                                     M                          0            0  10 M                         0         4
 008001 VERTICAL SOUNDING SIGNIFICANCE                                   FLAGTABLE                  0            0   7 FLAG TABLE                0         3
 008002 VERTICAL SIGNIFICANCE (SURFACE OBSERVATIONS)                     CODETABLE                  0            0   6 CODE TABLE                0         2
 008003 VERTICAL SIGNIFICANCE (SATELLITE OBSERVATIONS)                   CODETABLE                  0            0   6 CODE TABLE                0         2
 008004 PHASE OF AIRCRAFT FLIGHT                                         CODETABLE                  0            0   3 CODE TABLE                0         1
 008005 METEOROLOGICAL ATTRIBUTE SIGNIFICANCE                            CODETABLE                  0            0   4 CODE TABLE                0         2
 008006 OZONE VERTICAL SOUNDING SIGNIFICANCE                             FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 008007 DIMENSIONAL SIGNIFICANCE                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 008008 RADIATION VERTICAL SOUNDING SIGNIFICANCE                         FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 008009 DETAILED PHASE OF FLIGHT                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 008010 SURFACE QUALIFIER (FOR TEMPERATURE DATA)                         CODETABLE                  0            0   5 CODE TABLE                0         2
 008011 METEOROLOGICAL FEATURE                                           CODETABLE                  0            0   6 CODE TABLE                0         2
 008012 LAND/SEA QUALIFIER                                               CODETABLE                  0            0   2 CODE TABLE                0         1
 008013 DAY/NIGHT QUALIFIER                                              CODETABLE                  0            0   2 CODE TABLE                0         1
 008014 QUALIFIER FOR RUNWAY VISUAL RANGE                                CODETABLE                  0            0   4 CODE TABLE                0         2
 008015 SIGNIFICANCE QUALIFIER FOR SENSOR                                CODETABLE                  0            0   3 CODE TABLE                0         1
 008016 CHANGE QUALIFIER OF A TREND-TYPE FORECAST OR AN AERODROME        CODETABLE                  0            0   3 CODE TABLE                0         1
 008017 QUALIFIER OF THE TIME WHEN THE FORECAST CHANGE IS EXPECTED       CODETABLE                  0            0   2 CODE TABLE                0         1
 008018 SEAWINDS LAND/ICE SURFACE TYPE                                   FLAGTABLE                  0            0  17 FLAG TABLE                0         6
 008019 QUALIFIER FOR FOLLOWING CENTRE IDENTIFIER                        CODETABLE                  0            0   4 CODE TABLE                0         2
 008020 TOTAL NUMBER OF MISSING ENTITIES (WITH RESPECT TO ACCUMULATION ) NUMERIC                    0            0  16 NUMERIC                   0         5
 008021 TIME SIGNIFICANCE                                                CODETABLE                  0            0   5 CODE TABLE                0         2
 008022 TOTAL NUMBER (WITH RESPECT TO ACCUMULATION OR AVERAGE)           NUMERIC                    0            0  16 NUMERIC                   0         5
 008023 FIRST-ORDER STATISTICS                                           CODETABLE                  0            0   6 CODE TABLE                0         2
 008024 DIFFERENCE STATISTICS                                            CODETABLE                  0            0   6 CODE TABLE                0         2
 008025 TIME DIFFERENCE QUALIFIER                                        CODETABLE                  0            0   4 CODE TABLE                0         2
 008026 MATRIX SIGNIFICANCE                                              CODETABLE                  0            0   6 CODE TABLE                0         2
 008027 MATRIX GEOMETRY                                                  CODETABLE                  0            0   6 CODE TABLE                0         2
 008029 SURFACE TYPE                                                     CODETABLE                  0            0   8 CODE TABLE                0         3
 008030 MANUAL ON CODES (VOLUME I.1, SECTION C) CODE TABLE               NUMERIC                    0            0  13 NUMERIC                   0         4
 008031 DATA CATEGORY - CREX TABLE A                                     NUMERIC                    0            0   8 NUMERIC                   0         3
 008032 STATUS OF OPERATION                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 008033 METHOD OF DERIVATION OF PERCENTAGE CONFIDENCE                    CODETABLE                  0            0   7 CODE TABLE                0         3
 008035 TYPE OF MONITORING EXERCISE                                      CODETABLE                  0            0   3 CODE TABLE                0         1
 008036 TYPE OF CENTRE OR STATION PERFORMING MONITORING                  CODETABLE                  0            0   3 CODE TABLE                0         1
 008039 TIME SIGNIFICANCE (AVIATION FORECAST)                            CODETABLE                  0            0   6 CODE TABLE                0         2
 008040 FLIGHT LEVEL SIGNIFICANCE                                        CODETABLE                  0            0   6 CODE TABLE                0         2
 008041 DATA SIGNIFICANCE                                                CODETABLE                  0            0   5 CODE TABLE                0         2
 008042 EXTENDED VERTICAL SOUNDING SIGNIFICANCE                          FLAGTABLE                  0            0  18 FLAG TABLE                0         6
 008043 ATMOSPHERIC CHEMICAL OR PHYSICAL CONSTITUENT TYPE                CODETABLE                  0            0   8 CODE TABLE                0         3
 008044 CAS REGISTRY NUMBER                                              CCITTIA5                   0            0  88 CHARACTER                 0        11
 008045 PARTICULATE MATTER CHARACTERIZATION                              CODETABLE                  0            0   8 CODE TABLE                0         3
 008046 ATMOSPHERIC CHEMICAL OR PHYSICAL CONSTITUENT TYPE                CODETABLE                  0            0  16 COMMON CODE TABLE C-14      0         5
 008049 NUMBER OF OBSERVATIONS                                           NUMERIC                    0            0   8 NUMERIC                   0         3
 008050 QUALIFIER FOR NUMBER OF MISSING VALUES IN CALCULATION OF STATIST CODETABLE                  0            0   4 CODE TABLE                0         2
 008051 QUALIFIER FOR NUMBER OF MISSING VALUES IN CALCULATION OF STATIST CODETABLE                  0            0   3 CODE TABLE                0         1
 008052 CONDITION FOR WHICH NUMBER OF DAYS OF OCCURRENCE FOLLOWS         CODETABLE                  0            0   5 CODE TABLE                0         2
 008053 DAY OF OCCURRENCE QUALIFIER                                      CODETABLE                  0            0   2 CODE TABLE                0         1
 008054 QUALIFIER FOR WIND SPEED OR WIND GUSTS                           CODETABLE                  0            0   3 CODE TABLE                0         1
 008060 SAMPLE SCANNING MODE SIGNIFICANCE                                CODETABLE                  0            0   4 CODE TABLE                0         2
 008065 SUN-GLINT INDICATOR                                              CODETABLE                  0            0   2 CODE TABLE                0         1
 008066 SEMI-TRANSPARENCY INDICATOR                                      CODETABLE                  0            0   2 CODE TABLE                0         1
 008070 TOVS/ATOVS PRODUCT QUALIFIER                                     CODETABLE                  0            0   4 CODE TABLE                0         2
 008072 PIXEL(S) TYPE                                                    CODETABLE                  0            0   3 CODE TABLE                0         1
 008074 ALTIMETER ECHO TYPE                                              CODETABLE                  0            0   2 CODE TABLE                0         1
 008075 ASCENDING/DESCENDING ORBIT QUALIFIER                             CODETABLE                  0            0   2 CODE TABLE                0         1
 008076 TYPE OF BAND                                                     CODETABLE                  0            0   6 CODE TABLE                0         2
 008077 RADIOMETER SENSED SURFACE TYPE                                   CODETABLE                  0            0   7 CODE TABLE                0         3
 008079 AVIATION PRODUCT STATUS                                          CODETABLE                  0            0   4 CODE TABLE                0         2
 008080 QUALIFIER FOR GTSPP QUALITY FLAG                                 CODETABLE                  0            0   6 CODE TABLE                0         2
 008081 TYPE OF EQUIPMENT                                                CODETABLE                  0            0   6 CODE TABLE                0         2
 008082 MODIFICATION OF SENSOR HEIGHT TO ANOTHER VALUE                   CODETABLE                  0            0   3 CODE TABLE                0         1
 008083 NOMINAL VALUE INDICATOR                                          FLAGTABLE                  0            0  15 FLAG TABLE                0         5
 008085 BEAM IDENTIFIER                                                  CODETABLE                  0            0   3 CODE TABLE                0         1
 008086 VERTICAL SIGNIFICANCE FOR NWP                                    FLAGTABLE                  0            0  12 FLAG TABLE                           
 008090 DECIMAL SCALE OF FOLLOWING SIGNIFICANDS                          NUMERIC                    0         -127   8 NUMERIC                   0         3
 010001 HEIGHT OF LAND SURFACE                                           M                          0         -400  15 M                         0         5
 010002 HEIGHT                                                           M                         -1          -40  16 M                        -1         5
 010003 GEOPOTENTIAL                                                     M2S-2                     -1         -400  17 M2 S-2                   -1         6
 010004 PRESSURE                                                         PA                        -1            0  14 PA                       -1         5
 010007 HEIGHT                                                           M                          0        -1000  17 M                         0         6
 010008 GEOPOTENTIAL                                                     M2S-2                      0       -10000  20 M2 S-2                    0         7
 010009 GEOPOTENTIAL HEIGHT                                              GPM                        0        -1000  17 GPM                       0         5
 010010 MINIMUM PRESSURE REDUCED TO MEAN SEA LEVEL                       PA                        -1            0  14 PA                       -1         5
 010011 MAXIMUM PRESSURE REDUCED TO MEAN SEA LEVEL                       PA                        -1            0  14 PA                       -1         5
 010012 DENSITY ALTITUDE                                                 M                          0        -1525  13 M                         0         4
 010031 IN DIRECTION OF THE NORTH POLE, DISTANCE FROM THE EARTH'S CENTRE M                          2  -1073741824  31 M                         2        10
 010032 SATELLITE DISTANCE TO EARTH'S CENTRE                             M                          1            0  27 M                         2         9
 010033 ALTITUDE (PLATFORM TO ELLIPSOID)                                 M                          1            0  27 M                         2         9
 010034 EARTH'S RADIUS                                                   M                          1            0  27 M                         2         9
 010035 EARTH'S LOCAL RADIUS OF CURVATURE                                M                          1     62000000  22 M                         1         8
 010036 GEOID UNDULATION                                                 M                          2       -15000  15 M                         2         6
 010040 NUMBER OF RETRIEVED LAYERS                                       NUMERIC                    0            0  10 NUMERIC                   0         4
 010050 STANDARD DEVIATION ALTITUDE                                      M                          2            0  16 M                         2         5
 010051 PRESSURE REDUCED TO MEAN SEA LEVEL                               PA                        -1            0  14 PA                       -1         5
 010052 ALTIMETER SETTING (QNH)                                          PA                        -1            0  14 PA                       -1         5
 010053 GLOBAL NAVIGATION SATELLITE SYSTEM ALTITUDE                      M                          0        -1000  17 M                         0         5
 010060 PRESSURE CHANGE                                                  PA                        -1        -1024  11 PA                       -1         4
 010061 3-HOUR PRESSURE CHANGE                                           PA                        -1         -500  10 PA                       -1         4
 010062 24-HOUR PRESSURE CHANGE                                          PA                        -1        -1000  11 PA                       -1         4
 010063 CHARACTERISTIC OF PRESSURE TENDENCY                              CODETABLE                  0            0   4 CODE TABLE                0         2
 010064 SIGMET CRUISING LEVEL                                            CODETABLE                  0            0   3 CODE TABLE                0         1
 010070 INDICATED AIRCRAFT ALTITUDE                                      M                          0         -400  16 M                         0         5
 010080 VIEWING ZENITH ANGLE                                             DEG                        2        -9000  15 DEG                       2         5
 010081 ALTITUDE OF COG ABOVE REFERENCE ELLIPSOID                        M                          3            0  31 M                         3        10
 010082 INSTANTANEOUS ALTITUDE RATE                                      M/S                        3       -65536  17 M/S                       3         6
 010083 SQUARED OFF NADIR ANGLE OF THE SATELLITE FROM PLATFORM DATA      DEG2                       2            0  16 DEG2                      2         5
 010084 SQUARED OFF NADIR ANGLE OF THE SATELLITE FROM WAVEFORM DATA      DEG2                       2            0  16 DEG2                      2         5
 010085 MEAN SEA SURFACE HEIGHT                                          M                          3      -131072  18 M                         3         6
 010086 GEOID'S HEIGHT                                                   M                          3      -131072  18 M                         3         6
 010087 OCEAN DEPTH/LAND ELEVATION                                       M                          1      -131072  18 M                         1         6
 010088 TOTAL GEOCENTRIC OCEAN TIDE HEIGHT (SOLUTION 1)                  M                          3       -32768  16 M                         3         5
 010089 TOTAL GEOCENTRIC OCEAN TIDE HEIGHT (SOLUTION 2)                  M                          3       -32768  16 M                         3         5
 010090 LONG PERIOD TIDE HEIGHT                                          M                          3       -32768  16 M                         3         5
 010091 TIDAL LOADING HEIGHT                                             M                          3       -32768  16 M                         3         5
 010092 SOLID EARTH TIDE HEIGHT                                          M                          3       -32768  16 M                         3         5
 010093 GEOCENTRIC POLE TIDE HEIGHT                                      M                          3       -32768  16 M                         3         5
 010095 HEIGHT OF ATMOSPHERE USED                                        M                          0            0  16 M                         0         5
 010096 MEAN DYNAMIC TOPOGRAPHY                                          M                          3      -131072  18 M                         3         6
 010097 MEAN SEA SURFACE HEIGHT FROM ALTIMETER ONLY                      M                          3      -131072  18 M                         3         6
 010098 LOADING TIDE HEIGHT GEOCENTRIC OCEAN TIDE SOLUTION 1             M                          4        -2000  12 M                         4         4
 010099 LOADING TIDE HEIGHT GEOCENTRIC OCEAN TIDE SOLUTION 2             M                          4        -2000  12 M                         4         4
 010100 NON-EQUILIBRIUM LONG PERIOD TIDE HEIGHT                          M                          4        -2000  12 M                         4         4
 010101 SQUARED OFF NADIR ANGLE OF THE SATELLITE FROM WAVEFORM DATA      DEG2                       2       -32768  16 DEG2                      2         5
 010102 SEA SURFACE HEIGHT ANOMALY                                       M                          3       -32768  16 M                         3         5
 011001 WIND DIRECTION (DEGREE TRUE)                                     DEG                        0            0   9 DEG                       0         3
 011002 WIND SPEED                                                       M/S                        1            0  12 M/S                       1         4
 011003 U-COMPONENT                                                      M/S                        1        -4096  13 M/S                       1         4
 011004 V-COMPONENT                                                      M/S                        1        -4096  13 M/S                       1         4
 011005 W-COMPONENT                                                      PA/S                       1         -512  10 PA/S                      1         4
 011006 W-COMPONENT                                                      M/S                        2        -4096  13 M/S                       2         4
 011010 WIND DIRECTION ASSOCIATED WITH WIND SPEED WHICH FOLLOWS (DEGREE) DEG                        0            0   9 DEG                       0         3
 011011 WIND DIRECTION AT 10 M (DEGREE TRUE)                             DEG                        0            0   9 DEG                       0         3
 011012 WIND SPEED AT 10 M                                               M/S                        1            0  12 M/S                       1         4
 011013 WIND DIRECTION AT 5 M (DEGREE TRUE)                              DEG                        0            0   9 DEG                       0         3
 011014 WIND SPEED AT 5 M                                                M/S                        1            0  12 M/S                       1         4
 011016 EXTREME COUNTERCLOCKWISE WIND DIRECTION OF A VARIABLE WIND       DEG                        0            0   9 DEG                       0         3
 011017 EXTREME CLOCKWISE WIND DIRECTION OF A VARIABLE WIND DEGREE TRUE  DEG                        0            0   9 DEG                       0         3
 011019 STEADINESS OF WIND                                               %                          0            0   7 %                         0         3
 011021 RELATIVE VORTICITY                                               /S                         9       -65536  17 /S                        9         6
 011022 DIVERGENCE                                                       /S                         9       -65536  17 /S                        9         6
 011023 VELOCITY POTENTIAL                                               M2/S                      -2       -65536  17 M2/S                     -2         6
 011030 EXTENDED DEGREE OF TURBULENCE                                    CODETABLE                  0            0   6 CODE TABLE                0         2
 011031 DEGREE OF TURBULENCE                                             CODETABLE                  0            0   4 CODE TABLE                0         2
 011032 HEIGHT OF BASE OF TURBULENCE                                     M                         -1          -40  16 M                        -1         5
 011033 HEIGHT OF TOP OF TURBULENCE                                      M                         -1          -40  16 M                        -1         5
 011034 VERTICAL GUST VELOCITY                                           M/S                        1        -1024  11 M/S                       1         4
 011035 VERTICAL GUST ACCELERATION                                       MS-2                       2        -8192  14 M S-2                     2         5
 011036 MAXIMUM DERIVED EQUIVALENT VERTICAL GUST SPEED                   M/S                        1            0  10 M/S                       1         4
 011037 TURBULENCE INDEX                                                 CODETABLE                  0            0   6 CODE TABLE                0         2
 011038 TIME OF OCCURRENCE OF PEAK EDDY DISSIPATION RATE                 CODETABLE                  0            0   5 CODE TABLE                0         2
 011039 EXTENDED TIME OF OCCURRENCE OF PEAK EDDY DISSIPATION RATE        CODETABLE                  0            0   6 CODE TABLE                0         2
 011040 MAXIMUM WIND SPEED (MEAN WIND)                                   M/S                        1            0  12 M/S                       1         4
 011041 MAXIMUM WIND GUST SPEED                                          M/S                        1            0  12 M/S                       1         4
 011042 MAXIMUM WIND SPEED (10-MINUTE MEAN WIND)                         M/S                        1            0  12 M/S                       1         4
 011043 MAXIMUM WIND GUST DIRECTION (DEGREE TRUE)                        DEG                        0            0   9 DEG                       0         3
 011044 MEAN WIND DIRECTION FOR SURFACE - 1 500 M (5 000 FEET)           DEG                        0            0   9 DEG                       0         3
 011045 MEAN WIND SPEED FOR SURFACE - 1 500 M (5 000 FEET)               M/S                        1            0  12 M/S                       1         4
 011046 MAXIMUM INSTANTANEOUS WIND SPEED                                 M/S                        1            0  12 M/S                       1         4
 011047 MAXIMUM INSTANTANEOUS WIND SPEED OVER 10 MINUTES                 M/S                        1            0  12 M/S                       1         4
 011049 STANDARD DEVIATION OF WIND DIRECTION (DEGREE TRUE)               DEG                        0            0   9 DEG                       0         3
 011050 STANDARD DEVIATION OF HORIZONTAL WIND SPEED                      M/S                        1            0  12 M/S                       1         4
 011051 STANDARD DEVIATION OF VERTICAL WIND SPEED                        M/S                        1            0   8 M/S                       1         3
 011052 FORMAL UNCERTAINTY IN WIND SPEED                                 M/S                        2            0  13 M/S                       2         5
 011053 FORMAL UNCERTAINTY IN WIND DIRECTION (DEGREE TRUE)               DEG                        2            0  15 DEG                       2         5
 011054 MEAN WIND DIRECTION FOR 1 500 - 3 000 M (DEGREE TRUE)            DEG                        0            0   9 DEG                       0         3
 011055 MEAN WIND SPEED FOR 1 500 - 3 000 M                              M/S                        1            0  12 M/S                       1         4
 011061 ABSOLUTE WIND SHEAR IN 1 KM LAYER BELOW                          M/S                        1            0  12 M/S                       1         4
 011062 ABSOLUTE WIND SHEAR IN 1 KM LAYER ABOVE                          M/S                        1            0  12 M/S                       1         4
 011070 DESIGNATOR OF THE RUNWAY AFFECTED BY WIND SHEAR (INCLUDING ALL)  CCITTIA5                   0            0  32 CHARACTER                 0         4
 011071 TURBULENT VERTICAL MOMENTUM FLUX                                 M2S-2                      3         -128  14 M2 S-2                    3         5
 011072 TURBULENT VERTICAL BUOYANCY FLUX                                 KMS-1                      3         -128  11 K M S-1                   3         4
 011073 TURBULENT KINETIC ENERGY                                         M2S-2                      2        -1024  13 M2 S-2                    2         4
 011074 DISSIPATION ENERGY                                               M2S-2                      2        -1024  10 M2 S-2                    2         4
 011075 MEAN TURBULENCE INTENSITY (EDDY DISSIPATION RATE)                M2/3S-1                    2            0   8 M2/3 S-1                  2         3
 011076 PEAK TURBULENCE INTENSITY (EDDY DISSIPATION RATE)                M2/3S-1                    2            0   8 M2/3 S-1                  2         3
 011077 REPORTING INTERVAL OR AVERAGING TIME FOR EDDY DISSIPATION RATE   S                          0            0  12 S                         0         4
 011081 MODEL WIND DIRECTION AT 10 M (DEGREE TRUE)                       DEG                        2            0  16 DEG                       2         5
 011082 MODEL WIND SPEED AT 10 M                                         M/S                        2            0  14 M/S                       2         4
 011083 WIND SPEED                                                       KM/H                       0            0   9 KM/H                      0         3
 011084 WIND SPEED                                                       KT                         0            0   8 KT                        0         3
 011085 MAXIMUM WIND GUST SPEED                                          KM/H                       0            0   9 KM/H                      0         3
 011086 MAXIMUM WIND GUST SPEED                                          KT                         0            0   8 KT                        0         3
 011095 U-COMPONENT OF THE MODEL WIND VECTOR                             M/S                        1        -4096  13 M/S                       1         4
 011096 V-COMPONENT OF THE MODEL WIND VECTOR                             M/S                        1        -4096  13 M/S                       1         4
 011097 WIND SPEED FROM ALTIMETER                                        M/S                        2            0  12 M/S                       2         4
 011098 WIND SPEED FROM RADIOMETER                                       M/S                        2            0  12 M/S                       2         4
 011100 TRUE AIRCRAFT SPEED                                              M/S                        1            0  12 M/S                       1         4
 011101 AIRCRAFT VELOCITY U-COMPONENT                                    M/S                        1        -4096  13 M/S                       1         4
 011102 AIRCRAFT VELOCITY V-COMPONENT                                    M/S                        1        -4096  13 M/S                       1         4
 011103 AIRCRAFT VELOCITY W-COMPONENT                                    M/S                        1         -512  10 M/S                       1         4
 011104 AIRCRAFT TRUE HEADING                                            DEG                        0            0   9 DEG                       0         3
 011105 EDR ALGORITHM VERSION                                            NUMERIC                    0            0   6 NUMERIC                   0         2
 011106 RUNNING MINIMUM CONFIDENCE                                       NUMERIC                    1            0   4 NUMERIC                   1         2
 011107 MAXIMUM NUMBER BAD INPUTS                                        NUMERIC                    0            0   5 NUMERIC                   0         2
 011108 PEAK LOCATION                                                    NUMERIC                    1            0   4 NUMERIC                   1         2
 011109 NUMBER OF GOOD EDR                                               NUMERIC                    0            0   4 NUMERIC                   0         2
 012001 TEMPERATURE/AIR TEMPERATURE                                      K                          1            0  12 C                         1         3
 012002 AIR TEMPERATURE                                                  K                          1            0  12 C                         1         3
 012003 DEW-POINT TEMPERATURE                                            K                          1            0  12 C                         1         3
 012004 DRY-BULB TEMPERATURE AT 2 M                                      K                          1            0  12 C                         1         3
 012005 WET-BULB TEMPERATURE AT 2 M                                      K                          1            0  12 C                         1         3
 012006 DEW-POINT TEMPERATURE AT 2 M                                     K                          1            0  12 C                         1         3
 012007 VIRTUAL TEMPERATURE                                              K                          1            0  12 C                         1         3
 012011 MAXIMUM TEMPERATURE, AT HEIGHT AND OVER PERIOD SPECIFIED         K                          1            0  12 C                         1         3
 012012 MINIMUM TEMPERATURE, AT HEIGHT AND OVER PERIOD SPECIFIED         K                          1            0  12 C                         1         3
 012013 GROUND MINIMUM TEMPERATURE, PAST 12 HOURS                        K                          1            0  12 C                         1         3
 012014 MAXIMUM TEMPERATURE AT 2 M, PAST 12 HOURS                        K                          1            0  12 C                         1         3
 012015 MINIMUM TEMPERATURE AT 2 M, PAST 12 HOURS                        K                          1            0  12 C                         1         3
 012016 MAXIMUM TEMPERATURE AT 2 M, PAST 24 HOURS                        K                          1            0  12 C                         1         3
 012017 MINIMUM TEMPERATURE AT 2 M, PAST 24 HOURS                        K                          1            0  12 C                         1         3
 012021 MAXIMUM TEMPERATURE AT 2 M                                       K                          2            0  16 C                         2         4
 012022 MINIMUM TEMPERATURE AT 2 M                                       K                          2            0  16 C                         2         4
 012023 TEMPERATURE                                                      C                          0          -99   8 C                         0         2
 012024 DEW-POINT TEMPERATURE                                            C                          0          -99   8 C                         0         2
 012030 SOIL TEMPERATURE                                                 K                          1            0  12 C                         1         3
 012049 TEMPERATURE CHANGE OVER SPECIFIED PERIOD                         K                          0          -30   6 C                         0         2
 012051 STANDARD DEVIATION TEMPERATURE                                   K                          1            0  10 C                         1         3
 012052 HIGHEST DAILY MEAN TEMPERATURE                                   K                          1            0  12 C                         1         3
 012053 LOWEST DAILY MEAN TEMPERATURE                                    K                          1            0  12 C                         1         3
 012060 AWS ENCLOSURE INTERNAL TEMPERATURE                               K                          1            0  12 C                         1         3
 012061 SKIN TEMPERATURE                                                 K                          1            0  12 C                         1         3
 012062 EQUIVALENT BLACK BODY TEMPERATURE                                K                          1            0  12 C                         1         3
 012063 BRIGHTNESS TEMPERATURE                                           K                          1            0  12 C                         1         3
 012064 INSTRUMENT TEMPERATURE                                           K                          1            0  12 K                         1         4
 012065 STANDARD DEVIATION BRIGHTNESS TEMPERATURE                        K                          1            0  12 K                         1         4
 012066 ANTENNA TEMPERATURE                                              K                          2            0  16 C                         2         5
 012070 WARM LOAD TEMPERATURE                                            K                          2            0  16 K                         2         5
 012071 COLDEST CLUSTER TEMPERATURE                                      K                          1            0  12 K                         1         4
 012072 RADIANCE                                                         WM-2SR-1                   6            0  31 W M-2 SR-1                6         9
 012075 SPECTRAL RADIANCE                                                WM-3SR-1                  -3            0  16 W M-3 SR-1               -3         5
 012076 RADIANCE                                                         WM-2SR-1                   3            0  16 W M-2 SR-1                3         5
 012080 BRIGHTNESS TEMPERATURE REAL PART                                 K                          2       -10000  16 K                         2         5
 012081 BRIGHTNESS TEMPERATURE IMAGINARY PART                            K                          2       -10000  16 K                         2         5
 012082 PIXEL RADIOMETRIC ACCURACY                                       K                          2            0  12 K                         2         4
 012101 TEMPERATURE/AIR TEMPERATURE                                      K                          2            0  16 C                         2         4
 012102 WET-BULB TEMPERATURE                                             K                          2            0  16 C                         2         4
 012103 DEW-POINT TEMPERATURE                                            K                          2            0  16 C                         2         4
 012104 AIR TEMPERATURE AT 2 M                                           K                          2            0  16 C                         2         4
 012105 WEB-BULB TEMPERATURE AT 2 M                                      K                          2            0  16 C                         2         4
 012106 DEW-POINT TEMPERATURE AT 2 M                                     K                          2            0  16 C                         2         4
 012107 VIRTUAL TEMPERATURE                                              K                          2            0  16 C                         2         4
 012111 MAXIMUM TEMPERATURE, AT HEIGHT AND OVER PERIOD SPECIFIED         K                          2            0  16 C                         2         4
 012112 MINIMUM TEMPERATURE, AT HEIGHT AND OVER PERIOD SPECIFIED         K                          2            0  16 C                         2         4
 012113 GROUND MINIMUM TEMPERATURE, PAST 12 HOURS                        K                          2            0  16 C                         2         4
 012114 MAXIMUM TEMPERATURE AT 2 M, PAST 12 HOURS                        K                          2            0  16 C                         2         4
 012115 MINIMUM TEMPERATURE AT 2 M, PAST 12 HOURS                        K                          2            0  16 C                         2         4
 012116 MAXIMUM TEMPERATURE AT 2 M, PAST 24 HOURS                        K                          2            0  16 C                         2         4
 012117 MINIMUM TEMPERATURE AT 2 M, PAST 24 HOURS                        K                          2            0  16 C                         2         4
 012118 MAXIMUM TEMPERATURE AT HEIGHT SPECIFIED, PAST 24 HOURS           K                          2            0  16 C                         2         4
 012119 MINIMUM TEMPERATURE AT HEIGHT SPECIFIED, PAST 24 HOURS           K                          2            0  16 C                         2         4
 012120 GROUND TEMPERATURE                                               K                          2            0  16 C                         2         4
 012121 GROUND MINIMUM TEMPERATURE                                       K                          2            0  16 C                         2         4
 012122 GROUND MINIMUM TEMPERATURE OF THE PRECEDING NIGHT                K                          2            0  16 C                         2         4
 012130 SOIL TEMPERATURE                                                 K                          2            0  16 C                         2         4
 012131 SNOW TEMPERATURE                                                 K                          2            0  16 C                         2         4
 012132 ICE SURFACE TEMPERATURE                                          K                          2            0  16 C                         2         4
 012151 STANDARD DEVIATION OF DAILY MEAN TEMPERATURE                     K                          2            0  12 C                         2         4
 012152 HIGHEST DAILY MEAN TEMPERATURE                                   K                          2            0  16 C                         2         4
 012153 LOWEST DAILY MEAN TEMPERATURE                                    K                          2            0  16 C                         2         4
 012158 NOISE-EQUIVALENT DELTA TEMPERATURE WHILE VIEWING COLD TARGET     K                          2            0  12 C                         2         4
 012159 NOISE-EQUIVALENT DELTA TEMPERATURE WHILE VIEWING WARM TARGET     K                          2            0  12 C                         2         4
 012161 SKIN TEMPERATURE                                                 K                          2            0  16 C                         2         4
 012162 EQUIVALENT BLACK BODY TEMPERATURE                                K                          2            0  16 C                         2         4
 012163 BRIGHTNESS TEMPERATURE                                           K                          2            0  16 C                         2         4
 012164 INSTRUMENT TEMPERATURE                                           K                          2            0  16 K                         2         5
 012165 DIRECT SUN BRIGHTNESS TEMPERATURE                                K                          0            0  23 K                         0         7
 012166 SNAPSHOT ACCURACY                                                K                          1        -4000  13 K                         1         4
 012167 RADIOMETRIC ACCURACY (PURE POLARISATION)                         K                          1            0   9 K                         1         3
 012168 RADIOMETRIC ACCURACY (CROSS POLARISATION)                        K                          1            0   9 K                         1         3
 012171 COLDEST CLUSTER TEMPERATURE                                      K                          2            0  16 K                         2         5
 012180 AVERAGED 12 MICRON BT FOR ALL CLEAR PIXELS AT NADIR              K                          2            0  16 K                         2         5
 012181 AVERAGED 11 MICRON BT FOR ALL CLEAR PIXELS AT NADIR              K                          2            0  16 K                         2         5
 012182 AVERAGED 3.7 MICRON BT FOR ALL CLEAR PIXELS AT NADIR             K                          2            0  16 K                         2         5
 012183 AVERAGED 12 MICRON BT FOR ALL CLEAR PIXELS, FORWARD VIEW         K                          2            0  16 K                         2         5
 012184 AVERAGED 11 MICRON BT FOR ALL CLEAR PIXELS, FORWARD VIEW         K                          2            0  16 K                         2         5
 012185 AVERAGED 3.7 MICRON BT FOR ALL CLEAR PIXELS, FORWARD VIEW        K                          2            0  16 K                         2         5
 012186 MEAN NADIR SEA-SURFACE TEMPERATURE                               K                          2            0  16 K                         2         5
 012187 MEAN DUAL VIEW SEA-SURFACE TEMPERATURE                           K                          2            0  16 K                         2         5
 012188 INTERPOLATED 23.8 GHZ BRIGHTNESS T FROM MWR                      K                          2            0  16 K                         2         5
 012189 INTERPOLATED 36.5 GHZ BRIGHTNESS T FROM MWR                      K                          2            0  16 K                         2         5
 013001 SPECIFIC HUMIDITY                                                KG/KG                      5            0  14 KG/KG                     5         5
 013002 MIXING RATIO                                                     KG/KG                      5            0  14 KG/KG                     5         5
 013003 RELATIVE HUMIDITY                                                %                          0            0   7 %                         0         3
 013004 VAPOUR PRESSURE                                                  PA                        -1            0  10 PA                       -1         4
 013005 VAPOUR DENSITY                                                   KGM-3                      3            0   7 KG M-3                    3         3
 013006 MIXING HEIGHTS                                                   M                         -1          -40  16 M                        -1         5
 013007 MINIMUM RELATIVE HUMIDITY                                        %                          0            0   7 %                         0         3
 013008 MAXIMUM RELATIVE HUMIDITY                                        %                          0            0   7 %                         0         3
 013009 RELATIVE HUMIDITY                                                %                          1        -1000  12 %                         1         4
 013011 TOTAL PRECIPITATION/TOTAL WATER EQUIVALENT                       KGM-2                      1           -1  14 KG M-2                    1         5
 013012 DEPTH OF FRESH SNOW                                              M                          2           -2  12 M                         2         4
 013013 TOTAL SNOW DEPTH                                                 M                          2           -2  16 M                         2         5
 013014 RAINFALL/WATER EQUIVALENT OF SNOW (AVERAGED RATE)                KGM-2S-1                   4            0  12 KG M-2 S-1                4         4
 013015 SNOWFALL (AVERAGED RATE)                                         M/S                        7            0  12 M/S                       7         4
 013016 PRECIPITABLE WATER                                               KGM-2                      0            0   7 KG M-2                    0         3
 013019 TOTAL PRECIPITATION PAST 1 HOUR                                  KGM-2                      1           -1  14 KG M-2                    1         4
 013020 TOTAL PRECIPITATION PAST 3 HOURS                                 KGM-2                      1           -1  14 KG M-2                    1         5
 013021 TOTAL PRECIPITATION PAST 6 HOURS                                 KGM-2                      1           -1  14 KG M-2                    1         5
 013022 TOTAL PRECIPITATION PAST 12 HOURS                                KGM-2                      1           -1  14 KG M-2                    1         5
 013023 TOTAL PRECIPITATION PAST 24 HOURS                                KGM-2                      1           -1  14 KG M-2                    1         5
 013031 EVAPOTRANSPIRATION                                               KGM-2                      0            0   7 KG M-2                    0         3
 013032 EVAPORATION/EVAPOTRANSPIRATION                                   KGM-2                      1            0   8 KG M-2                    1         3
 013033 EVAPORATION/EVAPOTRANSPIRATION                                   KGM-2                      1            0  10 KG M-2                    1         4
 013038 SUPERADIABATIC INDICATOR                                         CODETABLE                  0            0   2 CODE TABLE                0         1
 013039 TERRAIN TYPE (ICE/SNOW)                                          CODETABLE                  0            0   3 CODE TABLE                0         1
 013040 SURFACE FLAG                                                     CODETABLE                  0            0   4 CODE TABLE                0         2
 013041 PASQUILL-GIFFORD STABILITY CATEGORY                              CODETABLE                  0            0   4 CODE TABLE                0         2
 013042 PARCEL LIFTED INDEX (TO 500 HPA)                                 K                          0          -20   6 K                         0         2
 013043 BEST LIFTED INDEX (TO 500 HPA)                                   K                          0          -20   6 K                         0         2
 013044 K INDEX                                                          K                          0          -30   8 K                         0         3
 013045 KO INDEX                                                         K                          0          -30   8 K                         0         3
 013046 MAXIMUM BUOYANCY                                                 K                          0          -30   8 K                         0         3
 013047 MODIFIED SHOWALTER STABILITY INDEX                               K                          0          -60   6 C                         0         2
 013048 WATER FRACTION                                                   %                          1            0  10 %                         1         4
 013051 FREQUENCY GROUP, PRECIPITATION                                   CODETABLE                  0            0   4 CODE TABLE                0         2
 013052 HIGHEST DAILY AMOUNT OF PRECIPITATION                            KGM-2                      1           -1  14 KG M-2                    1         5
 013055 INTENSITY OF PRECIPITATION                                       KGM-2S-1                   4            0   8 MM/H                      1         4
 013056 CHARACTER AND INTENSITY OF PRECIPITATION                         CODETABLE                  0            0   4 CODE TABLE                0         2
 013057 TIME OF BEGINNING OR END OF PRECIPITATION                        CODETABLE                  0            0   4 CODE TABLE                0         2
 013058 SIZE OF PRECIPITATING ELEMENT                                    M                          4            0   7 MM                        1         3
 013059 NUMBER OF FLASHES (THUNDERSTORM)                                 NUMERIC                    0            0   7 NUMERIC                   0         3
 013060 TOTAL ACCUMULATED PRECIPITATION                                  KGM-2                      1           -1  17 KG M-2                    1         5
 013071 UPSTREAM WATER LEVEL                                             M                          2            0  14 M                         2         4
 013072 DOWNSTREAM WATER LEVEL                                           M                          2            0  14 M                         2         4
 013073 MAXIMUM WATER LEVEL                                              M                          2            0  14 M                         2         4
 013074 GROUND WATER LEVEL                                               M                          2            0  18 M                         2         6
 013080 WATER PH                                                         PHUNIT                     1            0  10 PH UNIT                   1         3
 013081 WATER CONDUCTIVITY                                               S/M                        3            0  14 S/M                       3         4
 013082 WATER TEMPERATURE                                                K                          1            0  12 K                         1         4
 013083 DISSOLVED OXYGEN                                                 KGM-3                      6            0  15 KG M-3                    6         5
 013084 TURBIDITY                                                        LM                         0            0  14 LM                        0         4
 013085 OXYDATION REDUCTION POTENTIAL (ORP)                              V                          3            0  14 V                         3         4
 013090 RADIOMETER WATER VAPOUR CONTENT                                  KGM-2                      1            0  10 KG M-2                    1         4
 013091 RADIOMETER LIQUID CONTENT                                        KGM-2                      2            0   8 KG M-2                    2         3
 013093 CLOUD OPTICAL THICKNESS                                          NUMERIC                    0            0   8 NUMERIC                   0         3
 013095 TOTAL COLUMN WATER VAPOUR                                        KGM-2                      4            0  19 KG M-2                    4         6
 013096 MWR WATER VAPOUR CONTENT                                         KGM-2                      2            0  14 KG M-2                    2         5
 013097 MWR LIQUID WATER CONTENT                                         KGM-2                      2            0  14 KG M-2                    2         5
 013098 INTEGRATED WATER VAPOUR DENSITY                                  KGM-2                      8            0  30 KG M-2                    8        10
 013110 MASS MIXING RATIO                                                %                          0            0   7 %                         0         3
 013111 SOIL MOISTURE                                                    G/KG                       0            0  10 G/KG                      0         4
 013112 OBJECT WETNESS DURATION                                          S                          0            0  17 S                         0         5
 013114 RATE OF ICE ACCRETION                                            KGM-2H-1                   1            0  11 KG M-2 H-1                1         4
 013115 ICE THICKNESS                                                    M                          2            0  19 M                         2         6
 013117 SNOW DENSITY (LIQUID WATER CONTENT)                              KGM-3                      0            0  10 KG M-3                    0         3
 013118 DEPTH OF FRESH SNOW (HIGH ACCURACY)                              M                          3            0  14 M                         3         5
 013155 INTENSITY OF PRECIPITATION (HIGH ACCURACY)                       KGM-2S-1                   5           -1  16 MM/H                      2         5
 014001 LONG-WAVE RADIATION, INTEGRATED OVER 24 HOURS                    JM-2                      -3       -65536  17 J M-2                    -3         5
 014002 LONG-WAVE RADIATION, INTEGRATED OVER PERIOD SPECIFIED            JM-2                      -3       -65536  17 J M-2                    -3         5
 014003 SHORT-WAVE RADIATION, INTEGRATED OVER 24 HOURS                   JM-2                      -3       -65536  17 J M-2                    -3         5
 014004 SHORT-WAVE RADIATION, INTEGRATED OVER PERIOD SPECIFIED           JM-2                      -3       -65536  17 J M-2                    -3         5
 014011 NET LONG-WAVE RADIATION, INTEGRATED OVER 24 HOURS                JM-2                      -3       -65536  17 J M-2                    -3         5
 014012 NET LONG-WAVE RADIATION, INTEGRATED OVER PERIOD SPECIFIED        JM-2                      -3       -65536  17 J M-2                    -3         5
 014013 NET SHORT-WAVE RADIATION, INTEGRATED OVER 24 HOURS               JM-2                      -3       -65536  17 J M-2                    -3         5
 014014 NET SHORT-WAVE RADIATION, INTEGRATED OVER PERIOD SPECIFIED       JM-2                      -3       -65536  17 J M-2                    -3         5
 014015 NET RADIATION, INTEGRATED OVER 24 HOURS                          JM-2                      -4       -16384  15 J M-2                    -4         5
 014016 NET RADIATION, INTEGRATED OVER PERIOD SPECIFIED                  JM-2                      -4       -16384  15 J M-2                    -4         5
 014017 INSTANTANEOUS LONG-WAVE RADIATION                                WM-2                       0         -512  10 W M-2                     0         4
 014018 INSTANTANEOUS SHORT-WAVE RADIATION                               WM-2                       0        -2048  12 W M-2                     0         4
 014019 SURFACE ALBEDO                                                   %                          0            0   7 %                         0         3
 014020 GLOBAL SOLAR RADIATION, INTEGRATED OVER 24 HOURS                 JM-2                      -4            0  15 J M-2                    -4         5
 014021 GLOBAL SOLAR RADIATION, INTEGRATED OVER PERIOD SPECIFIED         JM-2                      -4            0  15 J M-2                    -4         5
 014022 DIFFUSE SOLAR RADIATION, INTEGRATED OVER 24 HOURS                JM-2                      -4            0  15 J M-2                    -4         5
 014023 DIFFUSE SOLAR RADIATION, INTEGRATED OVER PERIOD SPECIFIED        JM-2                      -4            0  15 J M-2                    -4         5
 014024 DIRECT SOLAR RADIATION, INTEGRATED OVER 24 HOURS                 JM-2                      -4            0  15 J M-2                    -4         5
 014025 DIRECT SOLAR RADIATION, INTEGRATED OVER PERIOD SPECIFIED         JM-2                      -4            0  15 J M-2                    -4         5
 014026 ALBEDO AT THE TOP OF CLOUDS                                      %                          0            0   7 %                         0         3
 014027 ALBEDO                                                           %                          0            0   7 %                         0         3
 014028 GLOBAL SOLAR RADIATION (HIGH ACCURACY), INTEGRATED OVER PERIOD   JM-2                      -2            0  20 J M-2                    -2         6
 014029 DIFFUSE SOLAR RADIATION (HIGH ACCURACY), INTEGRATED OVER PERIOD  JM-2                      -2            0  20 J M-2                    -2         6
 014030 DIRECT SOLAR RADIATION (HIGH ACCURACY), INTEGRATED OVER PERIOD   JM-2                      -2            0  20 J M-2                    -2         6
 014031 TOTAL SUNSHINE                                                   MIN                        0            0  11 MIN                       0         4
 014032 TOTAL SUNSHINE                                                   H                          0            0  10 H                         0         4
 014033 TOTAL SUNSHINE                                                   %                          0            0   9 %                         0         3
 014034 SUNSHINE OVER PERIOD SPECIFIED                                   MIN                        0            0  11 MIN                       0         4
 014035 SOLAR RADIATION FLUX                                             WM-2                       1            0  14 W M-2                     1         5
 014042 BIDIRECTIONAL REFLECTANCE                                        %                          0            0   7 %                         0         3
 014043 CHANNEL RADIANCE                                                 WM-2SR-1UM-1               4            0  23 W M-2 SR-1 UM-1           4         7
 014044 CHANNEL RADIANCE                                                 WM-2SR-1CM                 7      -100000  22 W M-2 SR-1 CM             7         7
 014045 CHANNEL RADIANCE                                                 WM-2SR-1CM                 0            0  11 W M-2 SR-1 CM             0         4
 014046 SCALED IASI RADIANCE                                             WM-2SR-1M                  0        -5000  16 W M-2 SR-1 M              0         5
 014047 SCALED MEAN AVHRR RADIANCE                                       WM-2SR-1M                  0            0  31 W M-2 SR-1 M              0        10
 014048 SCALED STANDARD DEVIATION AVHRR RADIANCE                         WM-2SR-1M                  0            0  31 W M-2 SR-1 M              0        10
 014050 EMISSIVITY                                                       %                          1            0  10 %                         1         4
 014051 DIRECT SOLAR RADIATION INTEGRATED OVER LAST HOUR                 JM-2                      -3            0  14 J M-2                    -3         4
 014052 GLOBAL UPWARD SOLAR RADIATION, INTEGRATED OVER PERIOD SPECIFIED  JM-2                      -2     -1048574  20 J M-2                    -2         7
 014053 NET RADIATION (HIGH ACCURACY), INTEGRATED OVER PERIOD SPECIFIED  JM-2                      -2     -1048574  21 J M-2                    -2         7
 014054 PHOTOSYNTETICALLY ACTIVE RADIATION, INTEGRATED OVER PERIOD       JM-2                      -3            0  16 J M-2                    -3         5
 014055 SOLAR ACTIVITY INDEX                                             NUMERIC                    0       -32768  16 NUMERIC                   0         5
 014056 BACKGROUND LUMINANCE                                             CDM-2                      0            0  18 CD M-2                    0         6
 014057 SOIL HEAT FLUX                                                   JM-2                      -1        -1000  11 J M-2                    -1         4
 014071 GLOBAL UV SPECTRAL IRRADIANCE                                    WM-2NM-1                   6     -1048576  21 W M-2 NM-1                6         7
 014072 GLOBAL UV IRRADIATION                                            JM-2                       0     -4000000  23 J M-2                     0         7
 014073 GLOBAL ERYTHEMAL IRRADIATION                                     JM-2                      -3          -32   6 J M-2                    -3         2
 015001 TOTAL OZONE                                                      DU                         0            0  10 DU                        0         4
 015002 AIR MASS (SLANT PATH AT 22 KM)                                   NUMERIC                    2            0  10 NUMERIC                   2         3
 015003 MEASURED OZONE PARTIAL PRESSURE (SOUNDING)                       PA                         4            0   9 NBAR                      0         3
 015004 OZONE SOUNDING CORRECTION FACTOR (CF)                            NUMERIC                    3            0  11 NUMERIC                   3         4
 015005 OZONE P                                                          DU                         0            0  10 DU                        0         3
 015007 MOLECULAR MASS                                                   U                          2            0  15 U                         2         5
 015008 SIGNIFICAND OF VOLUMETRIC MIXING RATIO                           NUMERIC                    0            0  10 NUMERIC                   0         4
 015009 INTEGRATED NUMBER DENSITY                                        M-2                        0            0  10 M-2                       0         4
 015010 PARTIAL PRESSURE                                                 PA                         0            0  10 PA                        0         4
 015011 LOG 10 OF INTEGRATED ELECTRON DENSITY                            LOG(M-2)                   3        14000  13 LOG (M-2)                 3         4
 015012 TOTAL ELECTRON COUNT PER SQUARE METRE                            M-2                      -16            0   6 M-2                     -16         2
 015015 MAXIMUM IMAGE SPECTRAL COMPONENT BEFORE NORMALIZATION            NUMERIC                    0            0  31 NUMERIC                   0        10
 015020 INTEGRATED OZONE DENSITY                                         KGM-2                      8            0  21 KG M-2                    8         7
 015021 INTEGRATED MASS DENSITY                                          KGM-2                     11            0  31 KG M-2                   11        10
 015022 INTEGRATED NUMBER DENSITY                                        M-3                        0            0  10 M-3                       0         4
 015023 MASS DENSITY                                                     KGM-3                      0            0  10 KG M-3                    0         4
 015024 OPTICAL DEPTH                                                    NUMERIC                    4            0  24 NUMERIC                   4         8
 015025 TYPE OF POLLUTANT                                                CODETABLE                  0            0   4 CODE TABLE                0         2
 015026 CONCENTRATION OF POLLUTANT (MOL MOL-1)                           MOL/MOL                    9            0   9 MOL/MOL                   9         3
 015027 CONCENTRATION OF POLLUTANT (KG M-3)                              KGM-3                      9            0  10 KG M-3                    9         4
 015028 PHOTO DISSOCIATION RATE                                          /S                         0            0  10 /S                        0         4
 015029 EXTINCTION COEFFICIENT                                           M-1                        9            0  30 M-1                       9        10
 015030 AEROSOL CONTAMINATION INDEX                                      NUMERIC                    2        -1000  12 NUMERIC                   2         4
 015031 ATMOSPHERIC PATH DELAY IN SATELLITE SIGNAL                       M                          4        10000  15 M                         4         5
 015032 ESTIMATED ERROR IN ATMOSPHERIC PATH DELAY                        M                          4            0  10 M                         4         4
 015033 DIFFERENCE IN PATH DELAYS FOR LIMB VIEWS AT EXTREMES OF SCAN     M                          5       -10000  15 M                         5         5
 015034 ESTIMATED ERROR IN PATH DELAY DIFFERENCE                         M                          5            0  14 M                         5         5
 015035 COMPONENT OF ZENITH PATH DELAY DUE TO WATER VAPOUR               M                          4            0  14 M                         4         5
 015036 ATMOSPHERIC REFRACTIVITY                                         NUNITS                     3            0  19 N UNITS                   3         6
 015037 BENDING ANGLE                                                    RAD                        8      -100000  23 RAD                       8         7
 015040 PARTICULATE MATTER DIAMETER                                      M                          8            0   9 M                         8         3
 015042 REFLECTANCE                                                      %                          2            0  14 %                         2         5
 015043 NUMBER OF AVERAGING KERNEL LAYERS                                NUMERIC                    0            0  10 NUMERIC                   0         4
 015044 AVERAGING KERNEL VALUE                                           NUMERIC                    6     -5000000  24 NUMERIC                   6         8
 015045 Sulfur dioxide                                                   DU                         0            0  10 DU                        0         4
 015046 Volcano contamination index                                      NUMERIC                    0            0  10 NUMERIC                   0         4
 015049 Aerosol Angstrom wavelength exponent                             NUMERIC                    4            0  16 NUMERIC                   4         5
 015051 METEOROLOGICAL OPTICAL RANGE                                     M                          0            0  18 M                         0         6
 019001 TYPE OF SYNOPTIC FEATURE                                         CODETABLE                  0            0   6 CODE TABLE                0         2
 019002 EFFECTIVE RADIUS OF FEATURE                                      M                         -2            0  12 M                        -2         4
 019003 WIND SPEED THRESHOLD                                             M/S                        0            0   8 M/S                       0         3
 019004 EFFECTIVE RADIUS WITH RESPECT TO WIND SPEEDS ABOVE THRESHOLD     M                         -2            0  12 M                        -2         4
 019005 DIRECTION OF MOTION OF FEATURE (DEGREE TRUE)                     DEG                        0            0   9 DEG                       0         3
 019006 SPEED OF MOTION OF FEATURE                                       M/S                        2            0  14 M/S                       2         5
 019007 EFFECTIVE RADIUS OF FEATURE                                      M                         -3            0  12 M                        -3         4
 019008 VERTICAL EXTENT OF CIRCULATION                                   CODETABLE                  0            0   3 CODE TABLE                0         1
 019009 EFFECTIVE RADIUS WITH RESPECT TO WIND SPEEDS ABOVE THRESHOLD     M                         -3            0  12 M                        -3         4
 019010 METHOD FOR TRACKING THE CENTRE OF SYNOPTIC FEATURE               CODETABLE                  0            0   4 CODE TABLE                0         2
 019100 TIME INTERVAL TO CALCULATE THE MOVEMENT OF THE TROPICAL CYCLONE  CODETABLE                  0            0   4 CODE TABLE                0         2
 019101 ACCURACY OF THE POSITION OF THE CENTRE OF THE TROPICAL CYCLONE   CODETABLE                  0            0   4 CODE TABLE                0         2
 019102 SHAPE AND DEFINITION OF THE EYE OF THE TROPICAL CYCLONE          CODETABLE                  0            0   3 CODE TABLE                0         1
 019103 DIAMETER OF MAJOR AXIS OF THE EYE OF THE TROPICAL CYCLONE        CODETABLE                  0            0   4 CODE TABLE                0         2
 019104 CHANGE IN CHARACTER OF THE EYE DURING THE 30 MINUTES             CODETABLE                  0            0   4 CODE TABLE                0         2
 019105 DISTANCE BETWEEN THE END OF SPIRAL BAND AND THE CENTRE           CODETABLE                  0            0   4 CODE TABLE                0         2
 019106 IDENTIFICATION NUMBER OF TROPICAL CYCLONE                        NUMERIC                    0            0   7 NUMERIC                   0         3
 019107 TIME INTERVAL OVER WHICH THE MOVEMENT OF THE TROPICAL CYCLONE    CODETABLE                  0            0   4 CODE TABLE                0         2
 019108 ACCURACY OF GEOGRAPHICAL POSITION OF THE TROPICAL CYCLONE        CODETABLE                  0            0   3 CODE TABLE                0         1
 019109 MEAN DIAMETER OF THE OVERCAST CLOUD OF THE TROPICAL CYCLONE      CODETABLE                  0            0   4 CODE TABLE                0         2
 019110 APPARENT 24-HOUR CHANGE IN INTENSITY OF THE TROPICAL CYCLONE     CODETABLE                  0            0   4 CODE TABLE                0         2
 019111 CURRENT INTENSITY (CI) NUMBER OF THE TROPICAL CYCLONE            NUMERIC                    1            0   7 NUMERIC                   1         3
 019112 DATA TROPICAL (DT) NUMBER OF THE TROPICAL CYCLONE                NUMERIC                    1            0   7 NUMERIC                   1         3
 019113 CLOUD PATTERN TYPE OF THE DT-NUMBER                              CODETABLE                  0            0   4 CODE TABLE                0         2
 019114 MODEL EXPECTED TROPICAL (MET) NUMBER OF THE TROPICAL CYCLONE     NUMERIC                    1            0   7 NUMERIC                   1         3
 019115 TREND OF THE PAST 24-HOUR CHANGE (+: DEVELOPED, -: WEAKENED)     NUMERIC                    1          -30   6 NUMERIC                   1         2
 019116 PATTERN TROPICAL (PT) NUMBER OF THE TROPICAL CYCLONE             NUMERIC                    1            0   7 NUMERIC                   1         3
 019117 CLOUD PICTURE TYPE OF THE PT-NUMBER                              CODETABLE                  0            0   3 CODE TABLE                0         1
 019118 FINAL TROPICAL (T) NUMBER OF THE TROPICAL CYCLONE                NUMERIC                    1            0   7 NUMERIC                   1         3
 019119 TYPE OF THE FINAL T-NUMBER                                       CODETABLE                  0            0   3 CODE TABLE                0         1
 019150 TYPHOON INTERNATIONAL COMMON NUMBER (TYPHOON COMMITTEE)          CCITTIA5                   0            0  32 CHARACTER                 0         4
 020001 HORIZONTAL VISIBILITY                                            M                         -1            0  13 M                        -1         4
 020002 VERTICAL VISIBILITY                                              M                         -1            0   7 M                        -1         3
 020003 PRESENT WEATHER                                                  CODETABLE                  0            0   9 CODE TABLE                0         3
 020004 PAST WEATHER (1)                                                 CODETABLE                  0            0   5 CODE TABLE                0         2
 020005 PAST WEATHER (2)                                                 CODETABLE                  0            0   5 CODE TABLE                0         2
 020006 FLIGHT RULES                                                     CODETABLE                  0            0   3 CODE TABLE                0         1
 020008 CLOUD DISTRIBUTION FOR AVIATION                                  CODETABLE                  0            0   5 CODE TABLE                0         2
 020009 GENERAL WEATHER INDICATOR (TAF/METAR)                            CODETABLE                  0            0   4 CODE TABLE                0         2
 020010 CLOUD COVER (TOTAL)                                              %                          0            0   7 %                         0         3
 020011 CLOUD AMOUNT                                                     CODETABLE                  0            0   4 CODE TABLE                0         2
 020012 CLOUD TYPE                                                       CODETABLE                  0            0   6 CODE TABLE                0         2
 020013 HEIGHT OF BASE OF CLOUD                                          M                         -1          -40  11 M                        -1         4
 020014 HEIGHT OF TOP OF CLOUD                                           M                         -1          -40  11 M                        -1         4
 020015 PRESSURE AT BASE OF CLOUD                                        PA                        -1            0  14 PA                       -1         5
 020016 PRESSURE AT TOP OF CLOUD                                         PA                        -1            0  14 PA                       -1         5
 020017 CLOUD TOP DESCRIPTION                                            CODETABLE                  0            0   4 CODE TABLE                0         2
 020018 TENDENCY OF RUNWAY VISUAL RANGE                                  CODETABLE                  0            0   2 CODE TABLE                0         1
 020019 SIGNIFICANT PRESENT OR FORECAST WEATHER                          CCITTIA5                   0            0  72 CHARACTER                 0         9
 020020 SIGNIFICANT RECENT WEATHER PHENOMENA                             CCITTIA5                   0            0  32 CHARACTER                 0         4
 020021 TYPE OF PRECIPITATION                                            FLAGTABLE                  0            0  30 FLAG TABLE                0        10
 020022 CHARACTER OF PRECIPITATION                                       CODETABLE                  0            0   4 CODE TABLE                0         2
 020023 OTHER WEATHER PHENOMENA                                          FLAGTABLE                  0            0  18 FLAG TABLE                0         6
 020024 INTENSITY OF PHENOMENA                                           CODETABLE                  0            0   3 CODE TABLE                0         1
 020025 OBSCURATION                                                      FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 020026 CHARACTER OF OBSCURATION                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 020027 PHENOMENA OCCURRENCE                                             FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 020028 EXPECTED CHANGE IN INTENSITY                                     CODETABLE                  0            0   3 CODE TABLE                0         1
 020029 RAIN FLAG                                                        CODETABLE                  0            0   2 CODE TABLE                0         1
 020031 ICE DEPOSIT (THICKNESS)                                          M                          2            0   7 M                         2         3
 020032 RATE OF ICE ACCRETION                                            CODETABLE                  0            0   3 CODE TABLE                0         1
 020033 CAUSE OF ICE ACCRETION                                           FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 020034 SEA ICE CONCENTRATION                                            CODETABLE                  0            0   5 CODE TABLE                0         2
 020035 AMOUNT AND TYPE OF ICE                                           CODETABLE                  0            0   4 CODE TABLE                0         2
 020036 ICE SITUATION                                                    CODETABLE                  0            0   5 CODE TABLE                0         2
 020037 ICE DEVELOPMENT                                                  CODETABLE                  0            0   5 CODE TABLE                0         2
 020038 BEARING OF ICE EDGE (DEGREE TRUE)                                DEG                        0            0  12 DEG                       0         3
 020039 ICE DISTANCE                                                     M                         -1            0  13 M                        -1         4
 020040 EVOLUTION OF DRIFT SNOW                                          CODETABLE                  0            0   4 CODE TABLE                0         2
 020041 AIRFRAME ICING                                                   CODETABLE                  0            0   4 CODE TABLE                0         2
 020042 AIRFRAME ICING PRESENT                                           CODETABLE                  0            0   2 CODE TABLE                0         1
 020043 PEAK LIQUID WATER CONTENT                                        KGM-3                      4            0   7 KG M-3                    4         2
 020044 AVERAGE LIQUID WATER CONTENT                                     KGM-3                      4            0   7 KG M-3                    4         2
 020045 SUPERCOOLED LARGE DROPLET (SLD) CONDITIONS                       CODETABLE                  0            0   2 CODE TABLE                0         1
 020048 EVOLUTION OF FEATURE                                             CODETABLE                  0            0   4 CODE TABLE                0         2
 020050 CLOUD INDEX                                                      CODETABLE                  0            0   8 CODE TABLE                0         3
 020051 AMOUNT OF LOW CLOUDS                                             %                          0            0   7 %                         0         3
 020052 AMOUNT OF MIDDLE CLOUDS                                          %                          0            0   7 %                         0         3
 020053 AMOUNT OF HIGH CLOUDS                                            %                          0            0   7 %                         0         3
 020054 TRUE DIRECTION FROM WHICH A PHENOMENON OR CLOUDS ARE MOVING      DEG                        0            0   9 DEG                       0         3
 020055 STATE OF SKY IN THE TROPICS                                      CODETABLE                  0            0   4 CODE TABLE                0         2
 020056 CLOUD PHASE                                                      CODETABLE                  0            0   3 CODE TABLE                0         1
 020058 VISIBILITY SEAWARDS FROM A COASTAL STATION                       M                         -1            0  13 M                        -1         4
 020059 MINIMUM HORIZONTAL VISIBILITY                                    M                         -1            0   9 M                        -1         3
 020060 PREVAILING HORIZONTAL VISIBILITY                                 M                         -1            0  10 M                        -1         4
 020061 RUNWAY VISUAL RANGE (RVR)                                        M                          0            0  12 M                         0         4
 020062 STATE OF THE GROUND (WITH OR WITHOUT SNOW)                       CODETABLE                  0            0   5 CODE TABLE                0         2
 020063 SPECIAL PHENOMENA                                                CODETABLE                  0            0  10 CODE TABLE                0         4
 020065 SNOW COVER                                                       %                          0            0   7 %                         0         3
 020066 MAXIMUM DIAMETER OF HAILSTONES                                   M                          3            0   8 M                         3         3
 020067 DIAMETER OF DEPOSIT                                              M                          3            0   9 M                         3         3
 020070 MINIMUM NUMBER OF ATMOSPHERICS                                   NUMERIC                    0            0   7 NUMERIC                   0         3
 020071 ACCURACY OF FIX AND RATE OF ATMOSPHERICS                         CODETABLE                  0            0   4 CODE TABLE                0         2
 020079 SNOW/ICE CRYSTALS INDICATOR                                      FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 020080 CLOUD AMOUNT PERCENTAGE INTERVAL                                 CODETABLE                  0            0   3 CODE TABLE                0         1
 020081 CLOUD AMOUNT IN SEGMENT                                          %                          0            0   7 %                         0         3
 020082 AMOUNT SEGMENT CLOUD FREE                                        %                          0            0   7 %                         0         3
 020083 AMOUNT OF SEGMENT COVERED BY SCENE                               %                          0            0   7 %                         0         3
 020085 GENERAL CONDITION OF RUNWAY                                      CODETABLE                  0            0   4 CODE TABLE                0         1
 020086 RUNWAY DEPOSITS                                                  CODETABLE                  0            0   4 CODE TABLE                0         1
 020087 RUNWAY CONTAMINATION                                             CODETABLE                  0            0   4 CODE TABLE                0         1
 020088 DEPTH OF RUNWAY DEPOSITS                                         M                          3            0  12 M                         0         4
 020089 RUNWAY FRICTION COEFFICIENT                                      CODETABLE                  0            0   7 CODE TABLE                0         2
 020090 SPECIAL CLOUDS                                                   CODETABLE                  0            0   4 CODE TABLE                0         2
 020091 VERTICAL VISIBILITY                                              FT                        -2            0  10 FT                       -2         3
 020092 HEIGHT OF BASE OF CLOUD                                          FT                        -2            0  10 FT                       -2         3
 020093 HEIGHT OF INVERSION                                              M                         -1            0   8 M                        -1         3
 020095 ICE PROBABILITY                                                  NUMERIC                    3            0  10 NUMERIC                   3         4
 020096 ICE AGE (A PARAMETER)                                            DB                         2        -4096  13 DB                        2         4
 020101 LOCUST (ACRIDIAN) NAME                                           CODETABLE                  0            0   4 CODE TABLE                0         2
 020102 LOCUST (MATURITY) COLOUR                                         CODETABLE                  0            0   4 CODE TABLE                0         2
 020103 STAGE OF DEVELOPMENT OF LOCUSTS                                  CODETABLE                  0            0   4 CODE TABLE                0         2
 020104 ORGANIZATION STATE OF SWARM OR BAND OF LOCUSTS                   CODETABLE                  0            0   4 CODE TABLE                0         2
 020105 SIZE OF SWARM OR BAND OF LOCUSTS AND DURATION OF PASSAGE         CODETABLE                  0            0   4 CODE TABLE                0         2
 020106 LOCUST POPULATION DENSITY                                        CODETABLE                  0            0   4 CODE TABLE                0         2
 020107 DIRECTION OF MOVEMENTS OF LOCUST SWARM                           CODETABLE                  0            0   4 CODE TABLE                0         2
 020108 EXTENT OF VEGETATION                                             CODETABLE                  0            0   4 CODE TABLE                0         2
 020111 X-AXIS ERROR ELLIPSE MAJOR COMPONENT                             M                         -1            0  17 M                        -1         6
 020112 Y-AXIS ERROR ELLIPSE MINOR COMPONENT                             M                         -1            0  17 M                        -1         6
 020113 Z-AXIS  ERROR ELLIPSE COMPONENT                                  M                         -1            0  17 M                        -1         6
 020114 ANGLE OF X-AXIS IN ERROR ELLIPSE                                 DEG                        2       -18000  16 DEG                       2         5
 020115 ANGLE OF Z-AXIS IN ERROR ELLIPSE                                 DEG                        2       -18000  16 DEG                       2         5
 020116 EMISSION HEIGHT OF CLOUD STROKE                                  M                          0            0  16 M                         0         5
 020117 AMPLITUDE OF LIGHTNING STRIKE                                    A                         -1       -32000  16 A                        -1         5
 020118 LIGHTNING DETECTION ERROR                                        M                          0            0  19 M                         0         6
 020119 LIGHTNING DISCHARGE POLARITY                                     CODETABLE                  0            0   2 CODE TABLE                0         1
 020121 THRESHOLD VALUE FOR POLARITY DECISION                            V                          3            0  16 V                         3         5
 020122 THRESHOLD VALUE FOR POLARITY DECISION                            A                          0            0  16 A                         0         5
 020123 MINIMUM THRESHOLD FOR DETECTION                                  V/M                        3            0  16 V/M                       3         5
 020124 LIGHTNING STROKE OR FLASH                                        CODETABLE                  0            0   2 CODE TABLE                0         1
 020126 LIGHTNING RATES OF DISCHARGE                                     H-1                        0            0  23 H-1                       0         7
 020127 LIGHTNING - DISTANCE FROM STATION                                M                         -3            0   8 M                        -3         3
 020128 LIGHTNING - DIRECTION FROM STATION (DEGREE TRUE)                 DEG                        1            0  12 DEG                       1         4
 020130 CLOUD HYDROMETEOR CONCENTRATION                                  NUMERIC                    0            0  10 NUMERIC                   0         3
 020131 EFFECTIVE RADIUS OF CLOUD HYDROMETEORS                           M                          5            0   6 M                         5         2
 020132 CLOUD LIQUID WATER CONTENT                                       KGM-3                      5            0  11 KG M-3                    5         4
 020133 HYDROMETEOR RADIUS                                               M                          5            0   6 M                         5         2
 020135 ICE MASS (ON A ROD)                                              KG/M                       1            0  10 KG/M                      1         3
 020136 SUPPLEMENTARY CLOUD TYPE                                         CODETABLE                  0            0   9 CODE TABLE                0         3
 020137 EVOLUTION OF CLOUDS                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 021001 HORIZONTAL REFLECTIVITY                                          DB                         0          -64   7 DB                        0         3
 021002 VERTICAL REFLECTIVITY                                            DB                         0          -64   7 DB                        0         3
 021003 DIFFERENTIAL REFLECTIVITY                                        DB                         1           -5   7 DB                        1         3
 021005 LINEAR DEPOLARIZATION RATIO                                      DB                         0          -65   6 DB                        0         2
 021006 CIRCULAR DEPOLARIZATION RATIO                                    DB                         0          -65   6 DB                        0         2
 021011 DOPPLER MEAN VELOCITY IN X-DIRECTION                             M/S                        0         -128   8 M/S                       0         3
 021012 DOPPLER MEAN VELOCITY IN Y-DIRECTION                             M/S                        0         -128   8 M/S                       0         3
 021013 DOPPLER MEAN VELOCITY IN Z-DIRECTION                             M/S                        0         -128   8 M/S                       0         3
 021014 DOPPLER MEAN VELOCITY (RADIAL)                                   M/S                        1        -4096  13 M/S                       1         4
 021017 DOPPLER VELOCITY SPECTRAL WIDTH                                  M/S                        1            0   8 M/S                       1         3
 021018 EXTENDED NYQUIST VELOCITY                                        M/S                        1            0  10 M/S                       1         4
 021019 HIGH NYQUIST VELOCITY                                            M/S                        1            0  10 M/S                       1         3
 021021 ECHO TOPS                                                        M                         -3            0   4 M                        -3         2
 021022 RANGE BIN OFFSET                                                 M                          1            0  14 M                         1         5
 021023 RANGE BIN SIZE                                                   M                          0            0  14 M                         0         5
 021024 AZIMUTH OFFSET                                                   DEG                        1            0  12 DEG                       1         4
 021025 AZIMUTHAL RESOLUTION                                             DEG                        1            0   8 DEG                       1         3
 021030 SIGNAL TO NOISE RATIO                                            DB                         0          -32   8 DB                        0         3
 021031 VERTICALLY-INTEGRATED LIQUID-WATER CONTENT                       KGM-2                      0            0   7 KG M-2                    0         3
 021036 RADAR RAINFALL INTENSITY                                         M/S                        7            0  12 M/S                       7         4
 021041 BRIGHT-BAND HEIGHT                                               M                         -2            0   8 M                        -2         3
 021051 SIGNAL POWER ABOVE 1 MW                                          DB                         0         -256   8 DB                        0         3
 021062 BACKSCATTER                                                      DB                         2        -5000  13 DB                        2         4
 021063 RADIOMETRIC RESOLUTION (NOISE VALUE)                             %                          1            0  10 %                         1         4
 021064 CLUTTER NOISE ESTIMATE                                           NUMERIC                    0            0   8 NUMERIC                   0         3
 021065 MISSING PACKET COUNTER                                           NUMERIC                    0         -127   8 NUMERIC                   0         3
 021066 WAVE SCATTEROMETER PRODUCT CONFIDENCE DATA                       FLAGTABLE                  0            0  12 FLAG TABLE                0         4
 021067 WIND PRODUCT CONFIDENCE DATA                                     FLAGTABLE                  0            0  13 FLAG TABLE                0         5
 021068 RADAR ALTIMETER PRODUCT CONFIDENCE DATA                          FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 021069 SST PRODUCT CONFIDENCE DATA                                      FLAGTABLE                  0            0  10 FLAG TABLE                0         4
 021070 SST PRODUCT CONFIDENCE DATA (SADIST-2)                           FLAGTABLE                  0            0  23 FLAG TABLE                0         6
 021071 PEAKINESS                                                        NUMERIC                    0            0  16 NUMERIC                   0         5
 021072 SATELLITE ALTIMETER CALIBRATION STATUS                           FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 021073 SATELLITE ALTIMETER INSTRUMENT MODE                              FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 021075 IMAGE SPECTRUM INTENSITY                                         NUMERIC                    0            0   8 NUMERIC                   0         3
 021076 REPRESENTATION OF INTENSITIES                                    CODETABLE                  0            0   3 CODE TABLE                0         1
 021077 ALTITUDE CORRECTION (IONOSPHERE)                                 M                          3            0  14 M                         3         5
 021078 ALTITUDE CORRECTION (DRY TROPOSPHERE)                            M                          3            0   9 M                         3         3
 021079 ALTITUDE CORRECTION (WET TROPOSPHERE)                            M                          3         2000  10 M                         3         4
 021080 ALTITUDE CORRECTION (CALIBRATION CONSTANT)                       M                          3            0  11 M                         3         4
 021081 OPEN LOOP CORRECTION (HEIGHT-TIME LOOP)                          M                          3            0  10 M                         3         4
 021082 OPEN LOOP CORRECTION (AUTO GAIN CONTROL)                         DB                         3        -3000  14 DB                        3         5
 021083 WARM TARGET CALIBRATION                                          NUMERIC                    0            0  16 NUMERIC                   0         5
 021084 COLD TARGET CALIBRATION                                          NUMERIC                    0            0  16 NUMERIC                   0         5
 021085 ATSR SEA SURFACE TEMPERATURE ACROSS-TRACK BAND NUMBER            NUMERIC                    0            0   4 NUMERIC                   0         2
 021086 NUMBER OF PIXELS IN NADIR ONLY, AVERAGE                          NUMERIC                    0            0   9 NUMERIC                   0         3
 021087 NUMBER OF PIXELS IN DUAL VIEW, AVERAGE                           NUMERIC                    0            0   9 NUMERIC                   0         3
 021088 WET BACKSCATTER                                                  DB                         2        -5000  13 DB                        2         4
 021091 RADAR SIGNAL DOPPLER SPECTRUM 0TH MOMENT                         DB                         0         -100   8 DB                        0         3
 021092 RASS SIGNAL DOPPLER SPECTRUM 0TH MOMENT, REFERRING TO RASS SIG   DB                         0         -100   8 DB                        0         3
 021093 KU BAND PEAKINESS                                                NUMERIC                    3            0  16 NUMERIC                   3         5
 021094 S BAND PEAKINESS                                                 NUMERIC                    3            0  16 NUMERIC                   3         5
 021101 NUMBER OF VECTOR AMBIGUITIES                                     NUMERIC                    0            0   3 NUMERIC                   0         1
 021102 INDEX OF SELECTED WIND VECTOR                                    NUMERIC                    0            0   3 NUMERIC                   0         1
 021103 TOTAL NUMBER OF SIGMA-0 MEASUREMENTS                             NUMERIC                    0            0   5 NUMERIC                   0         2
 021104 LIKELIHOOD COMPUTED FOR SOLUTION                                 NUMERIC                    3       -30000  15 NUMERIC                   3         5
 021105 NORMALIZED RADAR CROSS-SECTION                                   DB                         2       -10000  14 DB                        2         5
 021106 KP VARIANCE COEFFICIENT (ALPHA)                                  NUMERIC                    3            0  14 NUMERIC                   3         5
 021107 KP VARIANCE COEFFICIENT (BETA)                                   NUMERIC                    8            0  16 NUMERIC                   8         5
 021109 SEAWINDS WIND VECTOR CELL QUALITY                                FLAGTABLE                  0            0  17 FLAG TABLE                0         6
 021110 NUMBER OF INNER-BEAM SIGMA-0 (FORWARD OF SATELLITE)              NUMERIC                    0            0   6 NUMERIC                   0         2
 021111 NUMBER OF OUTER-BEAM SIGMA-0 (FORWARD OF SATELLITE)              NUMERIC                    0            0   6 NUMERIC                   0         2
 021112 NUMBER OF INNER-BEAM SIGMA-0 (AFT OF SATELLITE)                  NUMERIC                    0            0   6 NUMERIC                   0         2
 021113 NUMBER OF OUTER-BEAM SIGMA-0 (AFT OF SATELLITE)                  NUMERIC                    0            0   6 NUMERIC                   0         2
 021114 KP VARIANCE COEFFICIENT (GAMMA)                                  DB                         3      -140000  18 DB                        3         6
 021115 SEAWINDS SIGMA-0 QUALITY                                         FLAGTABLE                  0            0  17 FLAG TABLE                0         6
 021116 SEAWINDS SIGMA-0 MODE                                            FLAGTABLE                  0            0  17 FLAG TABLE                0         6
 021117 SIGMA-0 VARIANCE QUALITY CONTROL                                 NUMERIC                    2            0  16 NUMERIC                   2         5
 021118 ATTENUATION CORRECTION ON SIGMA-0                                DB                         2       -10000  14 DB                        2         5
 021119 WIND SCATTEROMETER GEOPHYSICAL MODEL FUNCTION                    CODETABLE                  0            0   6 CODE TABLE                0         2
 021120 PROBABILITY OF RAIN                                              NUMERIC                    3            0  10 NUMERIC                   3         4
 021121 SEAWINDS NOF RAIN INDEX                                          NUMERIC                    0            0   8 NUMERIC                   0         3
 021122 ATTENUATION CORRECTION ON SIGMA-0 (FROM TB)                      DB                         2       -10000  14 DB                        2         5
 021123 SEAWINDS NORMALIZED RADAR CROSS-SECTION                          DB                         2       -30000  15 DB                        2         5
 021128 NUMBER OF VALID POINTS PER SECOND USED TO DERIVE PREVIOUS PARAMS NUMERIC                    0            0   8 NUMERIC                   0         3
 021130 SPECTRUM TOTAL ENERGY                                            NUMERIC                    6            0  28 NUMERIC                   6         9
 021131 SPECTRUM MAX ENERGY                                              NUMERIC                    6            0  28 NUMERIC                   6         9
 021132 DIRECTION OF SPECTRUM MAX ON HIGHER RESOLUTION GRID              DEG                        3            0  19 DEG                       3         6
 021133 WAVELENGTH OF SPECTRUM MAX ON HIGHER RESOLUTION GRID             M                          3            0  29 M                         3         9
 021134 RANGE RESOLUTION OF CRESS COVARIANCE SPECTRUM                    RAD/M                      3            0  19 RAD/M                     3         6
 021135 REAL PART OF CROSS SPECTRA POLAR GRID NUMBER OF BINS             NUMERIC                    3      -524288  20 NUMERIC                   3         7
 021136 IMAGINARY PART OF CROSS SPECTRA POLAR GRID NUMBER OF BINS        NUMERIC                    3      -524288  20 NUMERIC                   3         7
 021137 KU BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT                  DB                         2       -32768  16 DB                        2         5
 021138 STD KU BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT              DB                         2       -32768  16 DB                        2         5
 021139 KU BAND NET INSTRUMENTAL CORRECTION FOR AGC                      DB                         2        -2048  12 DB                        2         4
 021140 S BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT                   DB                         2       -32768  16 DB                        2         5
 021141 STD S BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT               DB                         2       -32768  16 DB                        2         5
 021142 S BAND NET INSTRUMENTAL CORRECTION FOR AGC                       DB                         2        -1024  11 DB                        2         4
 021143 KU BAND RAIN ATTENUATION                                         DB                         2  -1073741824  31 DB                        2        10
 021144 ALTIMETER RAIN FLAG                                              FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 021145 KU BAND AUTOMATIC GAIN CONTROL                                   DB                         2            0  13 DB                        2         4
 021146 RMS KU BAND AUTOMATIC GAIN CONTROL                               DB                         2            0   8 DB                        2         3
 021147 NUMBER OF VALID POINTS FOR KU BAND AUTOMATIC GAIN CONTROL        NUMERIC                    0            0   5 NUMERIC                   0         2
 021150 BEAM CO-LOCATION                                                 CODETABLE                  0            0   2 CODE TABLE                0         1
 021151 ESTIMATED ERROR IN SIGMA-0 AT 40 DEGREES INCIDENCE ANGLE         DB                         2            0   9 DB                        2         3
 021152 SLOPE AT 40 DEGREES INCIDENCE ANGLE                              DB/DEG                     2          -80   7 DB/DEG                    2         2
 021153 ESTIMATED ERROR IN SLOPE AT 40 DEGREES INCIDENCE ANGLE           DB/DEG                     2          -40   6 DB/DEG                    2         2
 021154 SOIL MOISTURE SENSITIVITY                                        DB                         2            0  12 DB                        2         4
 021155 WIND VECTOR CELL QUALITY                                         FLAGTABLE                  0            0  24 FLAG TABLE                0         8
 021156 BACKSCATTER DISTANCE                                             NUMERIC                    1        -4096  13 NUMERIC                   1         4
 021157 LOSS PER UNIT LENGTH OF ATMOSPHERE USED                          DB/M                      10            0  22 DB/M                     10         7
 021158 ASCAT KP QUALITY ESTIMATE                                        CODETABLE                  0            0   2 CODE TABLE                0         1
 021159 ASCAT SIGMA-0 USABILITY                                          CODETABLE                  0            0   2 CODE TABLE                0         1
 021160 ASCAT USE OF SYNTHETIC DATA                                      NUMERIC                    3            0  10 NUMERIC                   3         4
 021161 ASCAT SYNTHETIC DATA QUALITY                                     NUMERIC                    3            0  10 NUMERIC                   3         4
 021162 ASCAT SATELLITE ORBIT AND ATTITUDE QUALITY                       NUMERIC                    3            0  10 NUMERIC                   3         4
 021163 ASCAT SOLAR ARRAY REFLECTION CONTAMINATION                       NUMERIC                    3            0  10 NUMERIC                   3         4
 021164 ASCAT TELEMETRY PRESENCE AND QUALITY                             NUMERIC                    3            0  10 NUMERIC                   3         4
 021165 ASCAT EXTRAPOLATED REFERENCE FUNCTION PRESENCE                   NUMERIC                    3            0  10 NUMERIC                   3         4
 021166 LAND FRACTION                                                    NUMERIC                    3            0  10 NUMERIC                   3         4
 021169 ICE PRESENCE INDICATOR                                           CODETABLE                  0            0   2 CODE TABLE                0         1
 021170 C BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT                   DB                         2       -32768  16 DB                        2         5
 021171 RMS C BAND CORRECTED OCEAN BACKSCATTER COEFFICIENT               DB                         2       -32768  16 DB                        2         5
 021172 C BAND NET INSTRUMENTAL CORRECTION FOR AGC                       DB                         2        -2048  12 DB                        2         4
 021173 C BAND AUTOMATIC GAIN CONTROL                                    DB                         2            0  13 DB                        2         4
 021174 RMS C BAND AUTOMATIC GAIN CONTROL                                DB                         2            0   9 DB                        2         3
 021175 NUMBER OF VALID POINTS FOR C BAND AUTOMATIC GAIN CONTROL         NUMERIC                    0            0  10 NUMERIC                   0         4
 022001 DIRECTION OF WAVES (DEGREE TRUE)                                 DEG                        0            0   9 DEG                       0         3
 022002 DIRECTION OF WIND WAVES (DEGREE TRUE)                            DEG                        0            0   9 DEG                       0         3
 022003 DIRECTION OF SWELL WAVES (DEGREE TRUE)                           DEG                        0            0   9 DEG                       0         3
 022004 DIRECTION OF CURRENT (DEGREE TRUE)                               DEG                        0            0   9 DEG                       0         3
 022005 DIRECTION OF SEA SURFACE CURRENT (DEGREE TRUE)                   DEG                        0            0   9 DEG                       0         3
 022011 PERIOD OF WAVES                                                  S                          0            0   6 S                         0         2
 022012 PERIOD OF WIND WAVES                                             S                          0            0   6 S                         0         2
 022013 PERIOD OF SWELL WAVES                                            S                          0            0   6 S                         0         2
 022021 HEIGHT OF WAVES                                                  M                          1            0  10 M                         1         4
 022022 HEIGHT OF WIND WAVES                                             M                          1            0  10 M                         1         4
 022023 HEIGHT OF SWELL WAVES                                            M                          1            0  10 M                         1         4
 022025 STANDARD DEVIATION WAVE HEIGHT                                   M                          2            0  10 M                         2         4
 022026 STANDARD DEVIATION OF SIGNIFICANT WAVE HEIGHT                    M                          2            0  10 M                         2         4
 022031 SPEED OF CURRENT                                                 M/S                        2            0  13 M/S                       2         4
 022032 SPEED OF SEA SURFACE CURRENT                                     M/S                        2            0  13 M/S                       2         4
 022035 TIDAL ELEVATION WITH RESPECT TO LOCAL CHART DATUM                M                          2            0  14 M                         2         4
 022036 METEOROLOGICAL RESIDUAL TIDAL ELEVATION (SURGE OR OFFSET)        M                          2            0  14 M                         2         4
 022037 TIDAL ELEVATION WITH RESPECT TO NATIONAL LAND DATUM              M                          3       -10000  15 M                         3         5
 022038 TIDAL ELEVATION WITH RESPECT TO LOCAL CHART DATUM                M                          3       -10000  15 M                         3         5
 022039 METEOROLOGICAL RESIDUAL TIDAL ELEVATION (SURGE OR OFFSET)        M                          3        -5000  13 M                         3         4
 022040 METEOROLOGICAL RESIDUAL TIDAL ELEVATION (SURGE OR OFFSET)        M                          3        -5000  14 M                         3         5
 022041 SEA-SURFACE TEMPERATURE (15-DAY RUNNING MEAN)                    K                          1            0  12 K                         1         4
 022042 SEA/WATER TEMPERATURE                                            K                          1            0  12 K                         1         4
 022043 SEA/WATER TEMPERATURE                                            K                          2            0  15 K                         2         5
 022044 SOUND VELOCITY                                                   M/S                        1            0  14 M/S                       1         5
 022045 SEA/WATER TEMPERATURE                                            K                          3            0  19 K                         3         6
 022046 SEA ICE FRACTION                                                 NUMERIC                    2            0   7 NUMERIC                   2         3
 022049 SEA SURFACE TEMPERATURE                                          K                          2            0  15 K                         2         5
 022050 STANDARD DEVIATION SEA-SURFACE TEMPERATURE                       K                          2            0   8 K                         2         3
 022055 FLOAT CYCLE NUMBER                                               NUMERIC                    0            0  10 NUMERIC                   0         3
 022056 DIRECTION OF PROFILE                                             CODETABLE                  0            0   2 CODE TABLE                0         1
 022059 SEA SURFACE SALINITY                                             0/00                       2            0  14 0/00                      2         5
 022060 LAGRANGIAN DRIFTER DROGUE STATUS                                 CODETABLE                  0            0   3 CODE TABLE                0         1
 022061 STATE OF THE SEA                                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 022062 SALINITY                                                         0/00                       2            0  14 0/00                      2         5
 022063 TOTAL WATER DEPTH                                                M                          0            0  14 M                         0         5
 022064 SALINITY                                                         0/00                       3            0  17 0/00                      3         6
 022065 WATER PRESSURE                                                   PA                        -3            0  17 PA                       -3         6
 022066 WATER CONDUCTIVITY                                               S/M                        6            0  26 S/M                       6         8
 022067 INSTRUMENT TYPE FOR WATER TEMPERATURE PROFILE MEASUREMENT        CODETABLE                  0            0  10 CODE TABLE                0         4
 022068 WATER TEMPERATURE PROFILE RECORDER TYPES                         CODETABLE                  0            0   7 CODE TABLE                0         3
 022069 SPECTRAL WAVE DENSITY                                            M2HZ-1                     3            0  22 M2 HZ-1                   3         7
 022070 SIGNIFICANT WAVE HEIGHT                                          M                          2            0  13 M                         2         4
 022071 SPECTRAL PEAK WAVE PERIOD                                        S                          1            0   9 S                         1         3
 022072 SPECTRAL PEAK WAVE LENGTH                                        M                          0            0  13 M                         0         4
 022073 MAXIMUM WAVE HEIGHT                                              M                          2            0  13 M                         2         4
 022074 AVERAGE WAVE PERIOD                                              S                          1            0   9 S                         1         3
 022075 AVERAGE WAVE LENGTH                                              M                          0            0  13 M                         0         4
 022076 DIRECTION FROM WHICH DOMINANT WAVES ARE COMING (DEGREE TRUE)     DEG                        0            0   9 DEG                       0         3
 022077 DIRECTIONAL SPREAD OF DOMINANT WAVE                              DEG                        0            0   9 DEG                       0         3
 022078 DURATION OF WAVE RECORD                                          S                          0            0  12 S                         0         4
 022079 LENGTH OF WAVE RECORD                                            M                          0            0  16 M                         0         5
 022080 WAVEBAND CENTRAL FREQUENCY                                       HZ                         3            0  10 HZ                        3         4
 022081 WAVEBAND CENTRAL WAVE NUMBER                                     M-1                        5            0  13 M-1                       5         4
 022082 MAXIMUM NON-DIRECTIONAL SPECTRAL WAVE DENSITY                    M2S                        2            0  20 M2 S                      2         7
 022083 MAXIMUM NON-DIRECTIONAL SPECTRAL WAVE NUMBER                     M3                         2            0  20 M3                        2         7
 022084 BAND CONTAINING MAXIMUM NON-DIRECTIONAL SPECTRAL WAVE DENSITY    NUMERIC                    0            0   7 NUMERIC                   0         3
 022085 SPECTRAL WAVE DENSITY RATIO                                      NUMERIC                    0            0   7 NUMERIC                   0         3
 022086 MEAN DIRECTION FROM WHICH WAVES ARE COMING (DEGREE TRUE)         DEG                        0            0   9 DEG                       0         3
 022087 PRINCIPAL DIRECTION FROM WHICH WAVES ARE COMING (DEGREE TRUE)    DEG                        0            0   9 DEG                       0         3
 022088 FIRST NORMALIZED POLAR COORDINATE FROM FOURIER COEFFICIENTS      NUMERIC                    2            0   7 NUMERIC                   2         3
 022089 SECOND NORMALIZED POLAR COORDINATE FROM FOURIER COEFFICIENTS     NUMERIC                    2            0   7 NUMERIC                   2         3
 022090 NON-DIRECTIONAL SPECTRAL ESTIMATE BY WAVE FREQUENCY              M2S                        2            0  20 M2 S                      2         7
 022091 NON-DIRECTIONAL SPECTRAL ESTIMATE BY WAVE NUMBER                 M3                         2            0  20 M3                        2         7
 022092 DIRECTIONAL SPECTRAL ESTIMATE BY WAVE FREQUENCY                  M2RAD-1S                   2            0  20 M2 RAD-1 S                2         7
 022093 DIRECTIONAL SPECTRAL ESTIMATE BY WAVE NUMBER                     M4                         2            0  20 M4                        2         7
 022094 TOTAL NUMBER OF WAVE BANDS                                       NUMERIC                    0            0   7 NUMERIC                   0         3
 022095 DIRECTIONAL SPREAD OF INDIVIDUAL WAVES                           DEG                        0            0   8 DEG                       0         3
 022096 SPECTRAL BAND WIDTH                                              /S                         3            0   4 /S                        3         2
 022097 MEAN WAVELENGTH > 731 M OF IMAGE SPECTRUM AT LOW WAVE NUMBERS    M                          0            0  14 M                         0         5
 022098 WAVELENGTH SPREAD (WAVELENGTH > 731 M) AT LOW WAVE NUMBERS       M                          0            0  14 M                         0         5
 022099 MEAN DIRECTION AT LOW WAVE NUMBERS (WAVELENGTH > 731 M) (TRUE)   DEG                        0            0   9 DEG                       0         3
 022100 DIRECTION SPREAD AT LOW WAVE NUMBERS (WAVELENGTH > 731 M)        DEG                        0            0   9 DEG                       0         3
 022101 TOTAL ENERGY (WAVELENGTH > 731M) AT LOW WAVE NUMBERS             NUMERIC                    0            0  31 NUMERIC                   0        10
 022120 TIDE STATION AUTOMATED WATER LEVEL CHECK                         CODETABLE                  0            0   5 CODE TABLE                0         2
 022121 TIDE STATION MANUAL WATER LEVEL CHECK                            CODETABLE                  0            0   5 CODE TABLE                0         2
 022122 TIDE STATION AUTOMATED METEOROLOGICAL DATA CHECK                 CODETABLE                  0            0   5 CODE TABLE                0         2
 022123 TIDE STATION MANUAL METEOROLOGICAL DATA CHECK                    CODETABLE                  0            0   5 CODE TABLE                0         2
 022141 SEA-SURFACE TEMPERATURE (15-DAY RUNNING MEAN)                    K                          2            0  15 K                         2         5
 022150 NUMBER OF 18 HZ VALID POINTS FOR KU BAND                         NUMERIC                    0            0  10 NUMERIC                   0         4
 022151 KU BAND OCEAN RANGE                                              M                          3            0  31 M                         3        10
 022152 STD OF 18 HZ KU BAND OCEAN RANGE                                 M                          3            0  16 M                         3         5
 022153 NUMBER OF 18 HZ VALID POINTS FOR S BAND                          NUMERIC                    0            0  10 NUMERIC                   0         4
 022154 S BAND OCEAN RANGE                                               M                          3            0  31 M                         3        10
 022155 STD OF 18 HZ S BAND OCEAN RANGE                                  M                          3            0  16 M                         3         5
 022156 KU BAND SIGNIFICANT WAVE HEIGHT                                  M                          3            0  16 M                         3         5
 022157 STD OF 18 HZ KU BAND OCEAN RANGE                                 M                          3            0  16 M                         3         5
 022158 S BAND SIGNIFICANT WAVE HEIGHT                                   M                          3            0  16 M                         3         5
 022159 STD OF 18 HZ S BAND SIGNIFICANT WAVE HEIGHT                      M                          3            0  16 M                         3         5
 022160 NORMALIZED INVERSE WAVE AGE                                      NUMERIC                    6            0  21 NUMERIC                   6         7
 022161 WAVE SPECTRA                                                     M4                         4            0  27 M4                        4         9
 022162 RMS OF 20 HZ KU BAND OCEAN RANGE                                 M                          3            0  16 M                         3         5
 022163 NUMBER OF 20 HZ VALID POINTS FOR KU BAND                         NUMERIC                    0            0  10 NUMERIC                   0         4
 022164 RMS 20 HZ KU BAND SIGNIFICANT WAVE HEIGHT                        M                          3            0  16 M                         3         5
 022165 NUMBER OF 20 HZ VALID POINTS FOR KU BAND SIGNIFICANT WAVE HEIGHT NUMERIC                    0            0  10 NUMERIC                   0         4
 022166 KU BAND NET INSTRUMENTAL CORRECTION FOR SIGNIFICANT WAVE HEIGHT  M                          3        -1000  11 M                         3         4
 022167 NUMBER OF VALID POINTS FOR KU BAND BACKSCATTER                   NUMERIC                    0            0  10 NUMERIC                   0         4
 022168 C BAND OCEAN RANGE                                               M                          3            0  31 M                         3        10
 022169 RMS OF C BAND OCEAN RANGE                                        M                          3            0  16 M                         3         5
 022170 NUMBER OF 20 HZ VALID POINTS FOR C BAND                          NUMERIC                    0            0  10 NUMERIC                   0         4
 022171 C BAND SIGNIFICANT WAVE HEIGHT                                   M                          3            0  16 M                         3         5
 022172 RMS 20 HZ C BAND SIGNIFICANT WAVE HEIGHT                         M                          3            0  16 M                         3         5
 022173 NUMBER OF 20 HZ VALID POINTS FOR C BAND SIGNIFICANT WAVE HEIGHT  NUMERIC                    0            0  10 NUMERIC                   0         4
 022174 C BAND NET INSTRUMENTAL CORRECTION FOR SIGNIFICANT WAVE HEIGHT   M                          3        -1000  11 M                         3         4
 022175 NUMBER OF VALID POINTS FOR C BAND BACKSCATTER                    NUMERIC                    0            0  10 NUMERIC                   0         4
 022176 UNIQUE IDENTIFIER FOR THE PROFILE                                CCITTIA5                   0            0  72 CHARACTER                 0        72
 022177 HEIGHT OF XBT/XCTD LAUNCHER                                      M                          1            0   9 M                         0         3
 022178 XBT/XCTD LAUNCHER TYPE                                           CODETABLE                  0            0   8 CODE TABLE                0         3
 022179 SOFTWARE VERSION OF PROFILE RECORDER                             CCITTIA5                   0            0 256 CHARACTER                 0       256
 022180 AUTO LAUNCHER SOFTWARE VERSION NUMBER                            CCITTIA5                   0            0 256 CHARACTER                 0       256
 022181 INSTRUMENT MANUFACTURER'S SERIAL NUMBER                          CCITTIA5                   0            0  32 CHARACTER                 0        32
 022182 WATER COLUMN HEIGHT                                              M                          3            0  23 M                         3         7
 022184 WATER COLUMN HEIGHT DEVIATION FROM THE REFERENCE VALUE           M                          3        -2000  12 M                         3         4
 022185 BPR TRANSMISSION COUNT                                           NUMERIC                    0            0  10 NUMERIC                   0         3
 022186 DIRECTION FROM WHICH WAVES ARE COMING (DEGREE TRUE)              DEG                        0            0   9 DEG                       0         3
 022187 DIRECTIONAL SPREAD OF WAVE                                       DEG                        0            0   9 DEG                       0         3
 023001 ACCIDENT EARLY NOTIFICATION - ARTICLE APPLICABLE                 CODETABLE                  0            0   3 CODE TABLE                0         1
 023002 ACTIVITY OR FACILITY INVOLVED IN INCIDENT                        CODETABLE                  0            0   5 CODE TABLE                0         2
 023003 TYPE OF RELEASE                                                  CODETABLE                  0            0   3 CODE TABLE                0         1
 023004 COUNTERMEASURES TAKEN NEAR BORDER                                CODETABLE                  0            0   3 CODE TABLE                0         1
 023005 CAUSE OF INCIDENT                                                CODETABLE                  0            0   2 CODE TABLE                0         1
 023006 INCIDENT SITUATION                                               CODETABLE                  0            0   3 CODE TABLE                0         1
 023007 CHARACTERISTICS OF RELEASE                                       CODETABLE                  0            0   3 CODE TABLE                0         1
 023008 STATE OF CURRENT RELEASE                                         CODETABLE                  0            0   2 CODE TABLE                0         1
 023009 STATE OF EXPECTED RELEASE                                        CODETABLE                  0            0   2 CODE TABLE                0         1
 023016 POSSIBILITY OF SIGNIFICANT CHEMICAL TOXIC HEALTH EFFECT          CODETABLE                  0            0   2 CODE TABLE                0         1
 023017 FLOW DISCHARGE OF MAJOR RECIPIENT                                M3/S                       6            0  20 M3/S                      6         7
 023018 RELEASE BEHAVIOUR OVER TIME                                      CODETABLE                  0            0   3 CODE TABLE                0         1
 023019 ACTUAL RELEASE HEIGHT                                            M                          0       -15000  17 M                         0         6
 023021 EFFECTIVE RELEASE HEIGHT                                         M                          0       -15000  17 M                         0         6
 023022 DISTANCE OF RELEASE POINT OR SITE OF INCIDENT                    M                          0            0  24 M                         0         8
 023023 MAIN TRANSPORT SPEED IN THE ATMOSPHERE                           M/S                        1            0  12 M/S                       1         4
 023024 MAIN TRANSPORT SPEED IN WATER                                    M/S                        2            0  13 M/S                       2         4
 023025 MAIN TRANSPORT SPEED IN GROUND WATER                             M/S                        2            0  13 M/S                       2         4
 023027 MAIN TRANSPORT DIRECTION IN THE ATMOSPHERE (DEGREE TRUE)         DEG                        0            0   9 DEG                       0         3
 023028 MAIN TRANSPORT DIRECTION IN WATER (DEGREE TRUE)                  DEG                        0            0   9 DEG                       0         3
 023029 MAIN TRANSPORT DIRECTION IN GROUND WATER (DEGREE TRUE)           DEG                        0            0   9 DEG                       0         3
 023031 POSSIBILITY THAT PLUME WILL ENCOUNTER PRECIPITATION              CODETABLE                  0            0   2 CODE TABLE                0         1
 023032 PLUME WILL ENCOUNTER CHANGE IN WIND DIRECTION AND/OR SPEED FLAG  CODETABLE                  0            0   2 CODE TABLE                0         1
 023040 FLOW DISCHARGE - RIVER                                           M3/S                       1            0  22 M3/S                      1         7
 023041 FLOW DISCHARGE - WELL                                            M3/S                       3            0  16 M3/S                      3         5
 024001 ESTIMATE OF AMOUNT OF RADIOACTIVITY RELEASED UP TO SPECIFIC TIME BQ                       -11            0  28 BQ                      -11         9
 024002 ESTIMATED MAXIMUM POTENTIAL RELEASE                              BQ                       -11            0  28 BQ                      -11         9
 024003 COMPOSITION OF RELEASE                                           CODETABLE                  0            0   5 CODE TABLE                0         2
 024004 ELEMENT NAME                                                     CCITTIA5                   0            0  16 CHARACTER                 0         2
 024005 ISOTOPE MASS                                                     NUMERIC                    0            0   9 NUMERIC                   0         3
 024011 DOSE                                                             MSV                        2            0  32 MSV                       2        10
 024012 TRAJECTORY DOSE (DEFINED LOCATION AND EXPECTED TIME OF ARRIVAL)  MSV                        2            0  32 MSV                       2        10
 024013 GAMMA DOSE IN AIR ALONG THE MAIN TRANSPORT PATH                  MSV                        2            0  32 MSV                       2        10
 024014 GAMMA RADIATION DOSE RATE                                        NSV/H                      1            0  14 NSV/H                     1         4
 024021 AIR CONCENTRATION (OF NAMED ISOTOPE TYPE INCLUDING GROSS BETA)   BQM-3                      2            0  32 BQ M-3                    2        10
 024022 CONCENTRATION IN PRECIPITATION (OF NAMED ISOTOPE TYPE)           BQ/L                       2            0  32 BQ/L                      2        10
 024023 PULSE RATE OF BETA RADIATION                                     /S                         1            0  14 /S                        1         4
 024024 PULSE RATE OF GAMMA RADIATION                                    /S                         1            0  14 /S                        1         4
 025001 RANGE-GATE LENGTH                                                M                         -1            0   6 M                        -1         2
 025002 NUMBER OF GATES AVERAGED                                         NUMERIC                    0            0   4 NUMERIC                   0         2
 025003 NUMBER OF INTEGRATED PULSES                                      NUMERIC                    0            0   8 NUMERIC                   0         3
 025004 ECHO PROCESSING                                                  CODETABLE                  0            0   2 CODE TABLE                0         1
 025005 ECHO INTEGRATION                                                 CODETABLE                  0            0   2 CODE TABLE                0         1
 025006 Z TO R CONVERSION                                                CODETABLE                  0            0   3 CODE TABLE                0         1
 025007 Z TO R CONVERSION FACTOR                                         NUMERIC                    0            0  12 NUMERIC                   0         4
 025008 Z TO R CONVERSION EXPONENT                                       NUMERIC                    2            0   9 NUMERIC                   2         3
 025009 CALIBRATION METHOD                                               FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 025010 CLUTTER TREATMENT                                                CODETABLE                  0            0   4 CODE TABLE                0         2
 025011 GROUND OCCULTATION CORRECTION (SCREENING)                        CODETABLE                  0            0   2 CODE TABLE                0         1
 025012 RANGE ATTENUATION CORRECTION                                     CODETABLE                  0            0   2 CODE TABLE                0         1
 025013 BRIGHT-BAND CORRECTION                                           FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 025014 AZIMUTH CLUTTER CUT-OFF                                          NUMERIC                    0            0  12 NUMERIC                   0         4
 025015 RADOME ATTENUATION CORRECTION                                    FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 025016 CLEAR-AIR ATTENUATION CORRECTION                                 DB/M                       5            0   6 DB/M                      5         2
 025017 PRECIPITATION ATTENUATION CORRECTION                             FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 025018 A TO Z LAW FOR ATTENUATION FACTOR                                NUMERIC                    7            0   6 NUMERIC                   7         2
 025019 A TO Z LAW FOR ATTENUATION EXPONENT                              NUMERIC                    2            0   7 NUMERIC                   2         3
 025020 MEAN SPEED ESTIMATION                                            CODETABLE                  0            0   2 CODE TABLE                0         1
 025021 WIND COMPUTATION ENHANCEMENT                                     FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 025022 GHRSST REJECTION FLAG                                            FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 025023 GHRSST CONFIDENCE FLAG                                           FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 025024 GHRSST DATA QUALITY                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 025025 BATTERY VOLTAGE                                                  V                          1            0   9 V                         1         3
 025026 BATTERY VOLTAGE (LARGE RANGE)                                    V                          1            0  12 V                         1         4
 025028 OPERATOR OR MANUFACTURER DEFINED PARAMETER                       NUMERIC                    1       -16384  15 NUMERIC                   1         5
 025029 CALIBRATION METHOD                                               FLAGTABLE                  0            0   6 FLAG TABLE                0         2
 025030 RUNNING MEAN SEA-SURFACE TEMPERATURE USAGE                       CODETABLE                  0            0   2 CODE TABLE                0         1
 025031 NWP-GENERATED VERTICAL PROFILE THINNING METHOD                   CODETABLE                  0            0   3 CODE TABLE                           
 025032 WIND PROFILER MODE INFORMATION                                   CODETABLE                  0            0   2 CODE TABLE                0         1
 025033 WIND PROFILER SUBMODE INFORMATION                                CODETABLE                  0            0   2 CODE TABLE                0         1
 025034 WIND PROFILER QUALITY CONTROL TEST RESULTS                       FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 025035 DECISION METHOD FOR POLARITY                                     CODETABLE                  0            0   3 CODE TABLE                0         1
 025036 ATMOSPHERICS LOCATION METHOD                                     CODETABLE                  0            0   4 CODE TABLE                0         2
 025037 SST BIAS                                                         K                          2         -127   8 K                         2         3
 025038 DIFFERENCE BETWEEN SST AND ANALYSIS                              K                          1         -127   8 K                         1         3
 025040 CO2 WIND PRODUCT DERIVATION                                      CODETABLE                  0            0   4 CODE TABLE                0         2
 025041 MOVING PLATFORM DIRECTION REPORTING METHOD                       CODETABLE                  0            0   2 CODE TABLE                0         1
 025042 MOVING PLATFORM SPEED REPORTING METHOD                           CODETABLE                  0            0   2 CODE TABLE                0         1
 025043 WAVE SAMPLING INTERVAL (TIME)                                    S                          4            0  15 S                         4         5
 025044 WAVE SAMPLING INTERVAL (SPACE)                                   M                          2            0  14 M                         2         5
 025045 HIRS CHANNEL COMBINATION                                         FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 025046 MSU CHANNEL COMBINATION                                          FLAGTABLE                  0            0   5 FLAG TABLE                0         2
 025047 SSU CHANNEL COMBINATION                                          FLAGTABLE                  0            0   4 FLAG TABLE                0         2
 025048 AMSU-A CHANNEL COMBINATION                                       FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 025049 AMSU-B CHANNEL COMBINATION                                       FLAGTABLE                  0            0   6 FLAG TABLE                0         2
 025050 PRINCIPAL COMPONENT SCORE                                        NUMERIC                    4      -131072  18 NUMERIC                   4         6
 025051 AVHRR CHANNEL COMBINATION                                        FLAGTABLE                  0            0   7 FLAG TABLE                0         3
 025052 LOG-10 OF PRINCIPAL COMPONENTS NORMALIZED FIT TO DATA            NUMERIC                    4            0  15 NUMERIC                   4         5
 025053 OBSERVATION QUALITY                                              FLAGTABLE                  0            0  12 FLAG TABLE                0         4
 025054 SSMIS SUBFRAME ID NUMBER                                         NUMERIC                    0            0   5 NUMERIC                   0         2
 025055 MULTIPLEXER HOUSEKEEPING                                         K                          2            0  16 K                         2         5
 025060 SOFTWARE IDENTIFICATION                                          NUMERIC                    0            0  14 NUMERIC                   0         5
 025061 SOFTWARE IDENTIFICATION AND VERSION NUMBER                       CCITTIA5                   0            0  96 CHARACTER                 0        12
 025062 DATABASE IDENTIFICATION                                          NUMERIC                    0            0  14 NUMERIC                   0         5
 025063 CENTRAL PROCESSOR OR SYSTEM IDENTIFIER                           CODETABLE                  0            0   8 CODE TABLE                0         3
 025065 ORIENTATION CORRECTION (AZIMUTH)                                 DEG                        2        -1000  11 DEG                       2         4
 025066 ORIENTATION CORRECTION (ELEVATION)                               DEG                        2        -1000  11 DEG                       2         4
 025067 RADIOSONDE RELEASE POINT PRESSURE CORRECTION                     PA                         0        -8000  14 PA                        0         4
 025068 NUMBER OF ARCHIVE RECOMPUTES                                     NUMERIC                    0            0   7 NUMERIC                   0         3
 025069 FLIGHT LEVEL PRESSURE CORRECTIONS                                FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 025070 MAJOR FRAME COUNT                                                NUMERIC                    0            0   4 NUMERIC                   0         2
 025071 FRAME COUNT                                                      NUMERIC                    0            0   5 NUMERIC                   0         2
 025075 SATELLITE ANTENNA CORRECTIONS VERSION NUMBER                     NUMERIC                    0            0   5 NUMERIC                   0         2
 025076 LOG-10 OF (TEMPERATURE-RADIANCE CENTRAL WAVE NUMBER) FOR ATOVS   LOG(M-1)                   8            0  30 LOG (M-1)                 8        10
 025077 BANDWIDTH CORRECTION COEFFICIENT 1 FOR ATOVS                     NUMERIC                    5      -100000  18 NUMERIC                   5         7
 025078 BANDWIDTH CORRECTION COEFFICIENT 2 FOR ATOVS                     NUMERIC                    5            0  17 NUMERIC                   5         6
 025079 ALBEDO-RADIANCE SOLAR FILTERED IRRADIANCE FOR ATOVS              WM-2                       4            0  24 W M-2                     4         8
 025080 ALBEDO-RADIANCE EQUIVALENT FILTER WIDTH FOR ATOVS                M                         10            0  14 M                        10         5
 025081 INCIDENCE ANGLE                                                  DEG                        3            0  17 DEG                       3         6
 025082 AZIMUTH ANGLE                                                    DEG                        3            0  19 DEG                       3         6
 025083 FARADAY ROTATIONAL ANGLE                                         DEG                        3            0  19 DEG                       3         6
 025084 GEOMETRIC ROTATIONAL ANGLE                                       DEG                        5            0  26 DEG                       5         8
 025085 FRACTION OF CLEAR PIXELS IN HIRS FOV                             NUMERIC                    0            0   7 NUMERIC                   0         3
 025086 DEPTH CORRECTION INDICATOR                                       CODETABLE                  0            0   2 CODE TABLE                0         1
 025090 ORBIT STATE FLAG                                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 025091 STRUCTURE CONSTANT OF THE REFRACTION INDEX (CN2)                 DB                         3       -18192  13 DB                        3         5
 025092 ACOUSTIC PROPAGATION VELOCITY                                    M/S                        2        28000  14 M/S                       2         5
 025093 RASS COMPUTATION CORRECTION                                      FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 025095 ALTIMETER STATE FLAG                                             FLAGTABLE                  0            0   2 FLAG TABLE                0         1
 025096 RADIOMETER STATE FLAG                                            FLAGTABLE                  0            0   5 FLAG TABLE                0         2
 025097 THREE-DIMENSIONAL ERROR ESTIMATE OF THE NAVIGATOR ORBIT          CODETABLE                  0            0   4 CODE TABLE                0         2
 025098 ALTIMETER DATA QUALITY FLAG                                      FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 025099 ALTIMETER CORRECTION QUALITY FLAG                                FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 025100 XBT/XCTD FALL RATE EQUATION COEFFICIENT A                        NUMERIC                    5            0  20 NUMERIC                   5         6
 025101 XBT/XCTD FALL RATE EQUATION COEFFICIENT B                        NUMERIC                    5      -500000  21 NUMERIC                   5         6
 025102 NUMBER OF MISSING LINES EXCLUDING DATA GAPS                      NUMERIC                    0            0   8 NUMERIC                   0         3
 025103 NUMBER OF DIRECTIONAL BINS                                       NUMERIC                    0            0   8 NUMERIC                   0         3
 025104 NUMBER OF WAVELENGTH BINS                                        NUMERIC                    0            0   8 NUMERIC                   0         3
 025105 FIRST DIRECTIONAL BIN                                            DEG                        3            0  19 DEG                       3         6
 025106 DIRECTIONAL BIN STEP                                             DEG                        3            0  19 DEG                       3         6
 025107 FIRST WAVELENGTH BIN                                             M                          3            0  29 M                         3         9
 025108 LAST WAVELENGTH BIN                                              M                          3            0  29 M                         3         9
 025110 IMAGE PROCESSING SUMMARY                                         FLAGTABLE                  0            0  10 FLAG TABLE                0         4
 025111 NUMBER OF INPUT DATA GAPS                                        NUMERIC                    0            0   8 NUMERIC                   0         3
 025120 RA2-L2-PROCESSING FLAG                                           CODETABLE                  0            0   2 CODE TABLE                0         1
 025121 RA2-L2-PROCESSING QUALITY                                        %                          0            0   7 %                         0         3
 025122 HARDWARE CONFIGURATION FOR RF                                    CODETABLE                  0            0   2 CODE TABLE                0         1
 025123 HARDWARE CONFIGURATION FOR HPA                                   CODETABLE                  0            0   2 CODE TABLE                0         1
 025124 MWR-L2-PROCESSING FLAG                                           CODETABLE                  0            0   2 CODE TABLE                0         1
 025125 MWR-L2-PROCESSING QUALITY                                        %                          0            0   7 %                         0         3
 025126 MODEL DRY TROPOSPHERIC CORRECTION                                M                          3       -32768  16 M                         3         5
 025127 INVERTED BAROMETER CORRECTION                                    M                          3       -32768  16 M                         3         5
 025128 MODEL WET TROPOSPHERIC CORRECTION                                M                          3       -32768  16 M                         3         5
 025129 MWR DERIVED WET TROPOSPHERIC CORRECTION                          M                          3       -32768  16 M                         3         5
 025130 RA2 IONOSPHERIC CORRECTION ON KU BAND                            M                          3       -32768  16 M                         3         5
 025131 IONOSPHERIC CORRECTION FROM DORIS ON KU BAND                     M                          3       -32768  16 M                         3         5
 025132 IONOSPHERIC CORRECTION FROM MODEL ON KU BAND                     M                          3       -32768  16 M                         3         5
 025133 SEA STATE BIAS CORRECTION ON KU BAND                             M                          3       -32768  16 M                         3         5
 025134 RA2 IONOSPHERIC CORRECTION ON S BAND                             M                          3       -32768  16 M                         3         5
 025135 IONOSPHERIC CORRECTION FROM DORIS ON S BAND                      M                          3       -32768  16 M                         3         5
 025136 IONOSPHERIC CORRECTION FROM MODEL ON S BAND                      M                          3       -32768  16 M                         3         5
 025137 SEA STATE BIAS CORRECTION ON S BAND                              M                          3       -32768  16 M                         3         5
 025138 AVERAGE SIGNAL-TO-NOISE RATIO                                    NUMERIC                    0        -2048  12 NUMERIC                   0         4
 025140 START CHANNEL                                                    NUMERIC                    0            0  14 NUMERIC                   0         5
 025141 END CHANNEL                                                      NUMERIC                    0            0  14 NUMERIC                   0         5
 025142 CHANNEL SCALE FACTOR                                             NUMERIC                    0            0   6 NUMERIC                   0         2
 025143 LINEAR COEFFICIENT                                               NUMERIC                    6     -5000000  24 NUMERIC                   6         8
 025144 MATRIX DIMENSION (I AXIS)                                        NUMERIC                    0            0   9 NUMERIC                   0         3
 025145 MATRIX DIMENSION (J AXIS)                                        NUMERIC                    0            0   9 NUMERIC                   0         3
 025150 METHOD OF TROPICAL CYCLONE INTENSITY ANALYSIS USING SAT DATA     CODETABLE                  0            0   4 CODE TABLE                0         2
 025151 STAR RELATIVE MAGNITUDE                                          NUMERIC                    3       -20000  14 NUMERIC                   3         5
 025152 STAR BRIGHTNESS TEMPERATURE                                      K                          0            0  17 K                         0         6
 025153 LIMB                                                             CODETABLE                  0            0   2 CODE TABLE                0         1
 025160 KU BAND NET INSTRUMENTAL CORRECTION                              M                          4      -120000  18 M                         4         6
 025161 C BAND NET INSTRUMENTAL CORRECTION                               M                          4      -120000  18 M                         4         6
 025162 SEA STATE BIAS CORRECTION ON C BAND                              M                          4        -6000  13 M                         4         4
 025163 ALTIMETER IONOSPHERIC CORRECTION ON KU BAND                      M                          3       -32768  16 M                         3         5
 025164 RADIOMETER WET TROPOSPHERIC CORRECTION                           M                          4        -5000  13 M                         4         4
 025170 SAMPLING INTERVAL (TIME)                                         S                          0            0  10 S                         0         4
 025171 SAMPLE AVERAGING PERIOD                                          S                          0            0  10 S                         0         4
 025172 NUMBER OF SAMPLES                                                NUMERIC                    0            0  10 NUMERIC                   0         4
 025174 SMOS INFORMATION FLAG                                            FLAGTABLE                  0            0  14 FLAG TABLE                0         5
 025175 MODIFIED RESIDUAL                                                NUMERIC                    2            0  13 NUMERIC                   2         4
 026001 PRINCIPAL TIME OF DAILY READING IN UTC OF MAXIMUM TEMPERATURE    H                          1            0  12 H                         1         3
 026002 PRINCIPAL TIME OF DAILY READING IN UTC OF MINIMUM TEMPERATURE    H                          1            0  12 H                         1         3
 026003 TIME DIFFERENCE                                                  MIN                        0        -1440  12 MIN                       0         4
 026010 HOURS INCLUDED                                                   FLAGTABLE                  0            0  26 FLAG TABLE                0         9
 026020 DURATION OF PRECIPITATION                                        MIN                        0            0  11 MIN                       0         4
 026030 MEASUREMENT INTEGRATION TIME                                     S                          2            0   8 S                         2         3
 027001 LATITUDE (HIGH ACCURACY)                                         DEG                        5     -9000000  25 DEG                       5         7
 027002 LATITUDE (COARSE ACCURACY)                                       DEG                        2        -9000  15 DEG                       2         4
 027003 ALTERNATE LATITUDE (COARSE ACCURACY)                             DEG                        2        -9000  15 DEG                       2         4
 027004 ALTERNATE LATITUDE (HIGH ACCURACY)                               DEG                        5     -9000000  25 DEG                       5         7
 027010 FOOTPRINT AXIS 1                                                 M                         -1            0  14 M                        -1         5
 027020 SATELLITE LOCATION COUNTER                                       NUMERIC                    0            0  16 NUMERIC                   0         5
 027021 SATELLITE SUBLOCATION DIMENSION                                  NUMERIC                    0            0  16 NUMERIC                   0         5
 027031 IN DIRECTION OF 0 DEGREES LONGITUDE, DISTANCE FROM EARTH CENTRE  M                          2  -1073741824  31 M                         2        10
 027080 VIEWING AZIMUTH ANGLE (DEGREE TRUE)                              DEG                        2            0  16 DEG                       0         5
 028001 LONGITUDE (HIGH ACCURACY)                                        DEG                        5    -18000000  26 DEG                       5         8
 028002 LONGITUDE (COARSE ACCURACY)                                      DEG                        2       -18000  16 DEG                       2         5
 028003 ALTERNATE LONGITUDE (COARSE ACCURACY)                            DEG                        2       -18000  16 DEG                       2         5
 028004 ALTERNATE LONGITUDE (HIGH ACCURACY)                              DEG                        5    -18000000  26 DEG                       5         8
 028010 FOOTPRINT AXIS 2                                                 M                         -1            0  14 M                        -1         5
 028031 IN DIRECTION 90 DEGREES EAST, DISTANCE FROM THE EARTH'S CENTRE   M                          2  -1073741824  31 M                         2        10
 029001 PROJECTION TYPE                                                  CODETABLE                  0            0   3 CODE TABLE                0         1
 029002 COORDINATE GRID TYPE                                             CODETABLE                  0            0   3 CODE TABLE                0         1
 030001 PIXEL VALUE (4 BITS)                                             NUMERIC                    0            0   4 NUMERIC                   0         2
 030002 PIXEL VALUE (8 BITS)                                             NUMERIC                    0            0   8 NUMERIC                   0         3
 030004 PIXEL VALUE (16 BITS)                                            NUMERIC                    0            0  16 NUMERIC                   0         5
 030010 NUMBER OF GRID POINTS                                            NUMERIC                    0            0  13 NUMERIC                   0         4
 030021 NUMBER OF PIXELS PER ROW                                         NUMERIC                    0            0  12 NUMERIC                   0         4
 030022 NUMBER OF PIXELS PER COLUMN                                      NUMERIC                    0            0  12 NUMERIC                   0         4
 030031 PICTURE TYPE                                                     CODETABLE                  0            0   4 CODE TABLE                0         2
 030032 COMBINATION WITH OTHER DATA                                      FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 030033 NUMBER OF BINS ALONG THE RADIAL                                  NUMERIC                    0            0  12 NUMERIC                   0         4
 030034 NUMBER OF AZIMUTHS                                               NUMERIC                    0            0  12 NUMERIC                   0         4
 031000 SHORT DELAYED DESCRIPTOR REPLICATION FACTOR                      NUMERIC                    0            0   1                                      
 031001 DELAYED DESCRIPTOR REPLICATION FACTOR                            NUMERIC                    0            0   8                                      
 031002 EXTENDED DELAYED DESCRIPTOR REPLICATION FACTOR                   NUMERIC                    0            0  16                                      
 031011 DELAYED DESCRIPTOR AND DATA REPETITION FACTOR                    NUMERIC                    0            0   8                                      
 031012 EXTENDED DELAYED DESCRIPTOR AND DATA REPETITION FACTOR           NUMERIC                    0            0  16                                      
 031021 ASSOCIATED FIELD SIGNIFICANCE                                    CODETABLE                  0            0   6                                      
 031031 DATA PRESENT INDICATOR                                           FLAGTABLE                  0            0   1                                      
 033002 QUALITY INFORMATION                                              CODETABLE                  0            0   2 CODE TABLE                0         1
 033003 QUALITY INFORMATION                                              CODETABLE                  0            0   3 CODE TABLE                0         1
 033005 QUALITY INFORMATION (AWS DATA)                                   FLAGTABLE                  0            0  30 FLAG TABLE                0        10
 033006 INTERNAL MEASUREMENT STATUS INFORMATION (AWS)                    CODETABLE                  0            0   3 CODE TABLE                0         1
 033007 PER CENT CONFIDENCE                                              %                          0            0   7 %                         0         3
 033009 RELATIVE ERROR                                                   %                          2            0  14 %                         2         5
 033015 DATA QUALITY CHECK INDICATOR                                     CODETABLE                  0            0   6 CODE TABLE                0         2
 033020 QUALITY CONTROL INDICATION OF FOLLOWING VALUE                    CODETABLE                  0            0   3 CODE TABLE                0         1
 033021 QUALITY OF FOLLOWING VALUE                                       CODETABLE                  0            0   2 CODE TABLE                0         1
 033022 QUALITY OF BUOY SATELLITE TRANSMISSION                           CODETABLE                  0            0   2 CODE TABLE                0         1
 033023 QUALITY OF BUOY LOCATION                                         CODETABLE                  0            0   2 CODE TABLE                0         1
 033024 STATION ELEVATION QUALITY MARK (FOR MOBILE STATIONS)             CODETABLE                  0            0   4 CODE TABLE                0         2
 033025 ACARS INTERPOLATED VALUES INDICATOR                              CODETABLE                  0            0   3 CODE TABLE                0         1
 033026 MOISTURE QUALITY                                                 CODETABLE                  0            0   6 CODE TABLE                0         2
 033027 LOCATION QUALITY CLASS (RANGE OF RADIUS OF 66 % CONFIDENCE)      CODETABLE                  0            0   3 CODE TABLE                0         1
 033028 SNAPSHOT OVERALL QUALITY                                         CODETABLE                  0            0   3 CODE TABLE                0         1
 033030 SCAN LINE STATUS FLAGS FOR ATOVS                                 FLAGTABLE                  0            0  24 FLAG TABLE                0         8
 033031 SCAN LINE QUALITY FLAGS FOR ATOVS                                FLAGTABLE                  0            0  24 FLAG TABLE                0         8
 033032 CHANNEL QUALITY FLAGS FOR ATOVS                                  FLAGTABLE                  0            0  24 FLAG TABLE                0         8
 033033 FIELD OF VIEW QUALITY FLAGS FOR ATOVS                            FLAGTABLE                  0            0  24 FLAG TABLE                0         8
 033035 MANUAL/AUTOMATIC QUALITY CONTROL                                 CODETABLE                  0            0   4 CODE TABLE                0         2
 033036 NOMINAL CONFIDENCE THRESHOLD                                     %                          0            0   7 %                         0         3
 033037 WIND CORRELATION ERROR                                           FLAGTABLE                  0            0  20 FLAG TABLE                0         7
 033038 QUALITY FLAGS FOR GROUND-BASED GNSS DATA                         FLAGTABLE                  0            0  10 FLAG TABLE                0         4
 033039 QUALITY FLAGS FOR RADIO OCCULTATION DATA                         FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 033040 CONFIDENCE INTERVAL                                              %                          0            0   7 %                         0         3
 033041 ATTRIBUTE OF FOLLOWING VALUE                                     CODETABLE                  0            0   2 CODE TABLE                0         1
 033042 TYPE OF LIMIT REPRESENTED BY FOLLOWING VALUE                     CODETABLE                  0            0   3 CODE TABLE                0         1
 033043 AST CONFIDENCE                                                   FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 033044 ASAR QUALITY INFORMATION                                         FLAGTABLE                  0            0  15 FLAG TABLE                0         5
 033045 PROBABILITY OF FOLLOWING EVENT                                   %                          0            0   7 %                         0         3
 033046 CONDITIONAL PROBABILITY OF FOLLOWING EVENT WITH RESPECT EVENT    %                          0            0   7 %                         0         3
 033047 MEASUREMENT CONFIDENCE DATA                                      FLAGTABLE                  0            0  31 FLAG TABLE                0        11
 033048 CONFIDENCE MEASURE OF SAR INVERSION                              CODETABLE                  0            0   2 CODE TABLE                0         1
 033049 CONFIDENCE MEASURE OF WIND RETRIEVAL                             CODETABLE                  0            0   2 CODE TABLE                0         1
 033050 GLOBAL GTSPP QUALITY FLAG                                        CODETABLE                  0            0   4 CODE TABLE                0         2
 033052 S-BAND OCEAN RETRACKING QUALITY                                  FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 033053 KU BAND OCEAN RETRACKING QUALITY                                 FLAGTABLE                  0            0  21 FLAG TABLE                0         7
 033060 GQISFLAGQUAL - INDIVIDUAL IASI-SYSTEM QUALITY FLAG               CODETABLE                  0            0   2 CODE TABLE                0         1
 033061 GQISQUALINDEX - INDICATOR FOR INSTRUMENT NOISE PERFORMANCE       %                          0            0   7 %                         0         3
 033062 GQISQUALINDEXLOC - INDICATOR FOR GEOMETRIC QUALITY INDEX         %                          0            0   7 %                         0         3
 033063 GQISQUALINDEXRAD - INDICATOR FOR INSTRUMENT NOISE PERFORMANCE    %                          0            0   7 %                         0         3
 033064 GQISQUALINDEXSPECT - INDICATOR FOR INSTRUMENT NOISE PERFORMANCE  %                          0            0   7 %                         0         3
 033065 GQISSYSTECSONDQUAL - OUTPUT OF SYSTEM TEC QUALITY FUNCTION       NUMERIC                    0            0  24 NUMERIC                   0         8
 033070 TOTAL OZONE QUALITY                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 033071 PROFILE OZONE QUALITY                                            CODETABLE                  0            0   4 CODE TABLE                0         2
 033072 OZONE ERROR                                                      CODETABLE                  0            0   5 CODE TABLE                0         2
 033075 SCAN-LEVEL QUALITY FLAGS                                         FLAGTABLE                  0            0  13 FLAG TABLE                0         5
 033076 CALIBRATION QUALITY FLAGS                                        FLAGTABLE                  0            0   9 FLAG TABLE                0         3
 033077 FIELD-OF-VIEW QUALITY FLAGS                                      FLAGTABLE                  0            0  19 FLAG TABLE                0         7
 033078 GEOLOCATION QUALITY                                              CODETABLE                  0            0   4 CODE TABLE                0         2
 033079 GRANULE LEVEL QUALITY FLAGS                                      FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 033080 SCAN LEVEL QUALITY FLAGS                                         FLAGTABLE                  0            0  20 FLAG TABLE                0         7
 033081 CHANNEL DATA QUALITY FLAGS                                       FLAGTABLE                  0            0  12 FLAG TABLE                0         4
 033082 GEOLOCATION QUALITY FLAGS                                        FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 033083 RADIANCE DATA QUALITY FLAGS                                      FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 033084 Pixel level quality flags                                        FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 033085 Aerosol optical thickness quality flags                          FLAGTABLE                  0            0  18 FLAG TABLE                0         6
 033086 Quality of pixel level retrieval                                 FLAGTABLE                  0            0   3 FLAG TABLE                0         1
 033087 Extent of satellite within South Atlantic anomaly                FLAGTABLE                  0            0   4 FLAG TABLE                0         1
 033110 SCAN LINE QUALITY FLAG FOR SAPHIR/MADRAS                         FLAGTABLE                  0            0  10 FLAG TABLE                0         4
 033111 PAYLOAD MODE FOR SAPHIR                                          CODETABLE                  0            0   3 CODE TABLE                0         1                         
 033112 PAYLOAD MODE FOR MADRAS                                          CODETABLE                  0            0   3 CODE TABLE                0         1                         
 033113 SATELLITE MODE FOR SAPHIR/MADRAS                                 CODETABLE                  0            0   4 CODE TABLE                0         2                         
 033114 CHANNEL QUALITY FLAG FOR SAPHIR/MADRAS                           FLAGTABLE                  0            0  11 FLAG TABLE                0         4       
 033115 CALIBRATION FLAGS FOR SAPHIR/MADRAS                              CODETABLE                  0            0   3 CODE TABLE                0         1
 035000 FM AND REGIONAL CODE NUMBER                                      CODETABLE                  0            0  10 CODE TABLE                0         3
 035001 TIME-FRAME FOR MONITORING                                        CODETABLE                  0            0   3 CODE TABLE                0         1
 035011 NUMBER OF REPORTS ACTUALLY RECEIVED                              NUMERIC                    0            0  14 NUMERIC                   0         4
 035021 BULLETIN BEING MONITORED (TTAAII)                                CCITTIA5                   0            0  48 CHARACTER                 0         6
 035022 BULLETIN BEING MONITORED (YYGGGG)                                CCITTIA5                   0            0  48 CHARACTER                 0         6
 035023 BULLETIN BEING MONITORED (CCCC)                                  CCITTIA5                   0            0  32 CHARACTER                 0         4
 035024 BULLETIN BEING MONITORED (BBB)                                   CCITTIA5                   0            0  24 CHARACTER                 0         3
 035030 DISCREPANCIES IN THE AVAILABILITY OF EXPECTED DATA               CODETABLE                  0            0   4 CODE TABLE                0         1
 035031 QUALIFIER ON MONITORING RESULTS                                  CODETABLE                  0            0   7 CODE TABLE                0         2
 035032 CAUSE OF MISSING DATA                                            CODETABLE                  0            0   4 CODE TABLE                0         1
 035033 OBSERVATION AND COLLECTION DEFICIENCIES                          CODETABLE                  0            0   7 CODE TABLE                0         2
 035034 STATISTICAL TRENDS FOR AVAILABILITY OF DATA (DURING SURVEY)      CODETABLE                  0            0   3 CODE TABLE                0         1
 035035 REASON FOR TERMINATION                                           CODETABLE                  0            0   5 CODE TABLE                0         2
 040001 SURFACE SOIL MOISTURE (MS)                                       %                          1            0  10 %                         1         4
 040002 ESTIMATED ERROR IN SURFACE SOIL MOISTURE                         %                          1            0  10 %                         1         4
 040003 MEAN SURFACE SOIL MOISTURE                                       NUMERIC                    3            0  10 NUMERIC                   3         4
 040004 RAIN FALL DETECTION                                              NUMERIC                    3            0  10 NUMERIC                   3         4
 040005 SOIL MOISTURE CORRECTION FLAG                                    FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 040006 SOIL MOISTURE PROCESSING FLAG                                    FLAGTABLE                  0            0  16 FLAG TABLE                0         6
 040007 SOIL MOISTURE QUALITY                                            %                          1            0  10 %                         1         4
 040008 FROZEN LAND SURFACE FRACTION                                     %                          1            0  10 %                         1         4
 040009 INUNDATION AND WETLAND FRACTION                                  %                          1            0  10 %                         1         4
 040010 TOPOGRAPHIC COMPLEXITY                                           %                          1            0  10 %                         1         4
 040011 INTERPOLATION FLAG                                               FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 040012 RADIOMETER DATA QUALITY FLAG                                     FLAGTABLE                  0            0   8 FLAG TABLE                0         3
 040013 RADIOMETER BRIGHTNESS TEMPERATURE INTERPRETATION FLAG            CODETABLE                  0            0   3 CODE TABLE                0         1
 040014 HIGH-FREQUENCY FLUCTUATIONS OF THE SEA-SURFACE TOPOGRAPHY CORR   M                          4        -3000  13 M                         4         4
 040015 NORMALISED DIFFERENTIAL VEGETATION INDEX (NDVI)                  NUMERIC                    2         -100   8 NUMERIC                   2         3
 040016 RESIDUAL RMS IN BAND                                             NUMERIC                    3            0  14 NUMERIC                   3         5
 040017 NON-NORMALISED PRINCIPAL COMPONENT SCORE                         NUMERIC                    0  -1073741824  31 NUMERIC                   0        10
 040018 GIACAVGIMAGIIS - AVERAGE OF IMAGER MEASUREMENTS                  WM-2SR-1M                  6            0  24 W M-2 SR-1 M              6         8
 040019 GIACVARIMAGIIS - VARIANCE OF IMAGER MEASUREMENTS                 WM-2SR-1M                  6            0  24 W M-2 SR-1 M              6         8
 040020 GQISFLAGQUALDETAILED - QUALITY FLAG FOR THE SYSTEM               FLAGTABLE                  0            0  17 FLAG TABLE                0         6
 040021 FRACTION OF WEIGHTED AVHRR PIXEL IN IASI FOV WITH SNOW/ICE       %                          0            0   7 %                         0         3
 040022 NUMBER OF MISSING, BAD OR FAILED AVHRR PIXELS                    NUMERIC                    0            0   7 NUMERIC                   0         3
 040023 AUXILIARY ALTIMETER STATE FLAGS                                  FLAGTABLE                  0            0   5 FLAG TABLE                0         2
 040024 METEOROLOGICAL MAP AVAILABILITY                                  CODETABLE                  0            0   3 CODE TABLE                0         1
 040025 INTERPOLATION FLAG FOR MEAN DIURNAL TIDE                         CODETABLE                  0            0   2 CODE TABLE                0         1
 040026 SCORE QUANTIZATION FACTOR                                        NUMERIC                    2            0  16 NUMERIC                   2         5
